{"text_format":"2","workbook":"xls","n_sheets":16,"sheets":["Kopā","Savilkums","1","2","3","4","5","6","7","8","9","10","11","12","13","14"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Kopā","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[[7,0,7,4],[15,2,16,3],[17,2,17,3],[17,0,17,1],[15,0,16,1],[15,4,16,4]],"flags":["formulas_cached_only"]}
[null,null,"APSTIPRINU:"]
[]
[{"$nulls":4},"/______________/___________________/"]
[null,null,null,"             Paraksts                             atšifrējums"]
[{"$nulls":4},"z.v."]
[{"$nulls":4},"2011. g. \"_____  \"________________"]
[]
["Būvniecības koptāme"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[]
[null,null,"Cilvēkstundas: ",null,0]
[null,null,"Tāme sastādīta:",null,0]
["Tāmes nr.",null,"Tāmes nosaukums",null,"Izmaksas BEZ PVN 22% Ls"]
[]
["1",null,"Tautas nama vienkāršotā rekonstrukcija",null,0]
[null,null,null,"Kopā bez PVN Ls:",0]
[null,null,null,"PVN 22% Ls:",0]
[null,null,null,"Kopā ar PVN Ls:",0]

{"sheet":"Savilkums","index":1,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[[28,0,28,1],[14,5,14,7],[29,0,29,1],[6,0,6,7],[16,0,16,1],[14,0,15,1],[14,2,15,2],[14,3,15,3],[22,0,22,1],[23,0,23,1],[24,0,24,1],[17,0,17,1],[26,0,26,1],[27,0,27,1],[14,4,15,4],[21,0,21,1],[21,0,21,1],[25,0,25,1],[18,0,18,1],[19,0,19,1],[20,0,20,1]],"flags":["formulas_cached_only"]}
[{"$nulls":5},"APSTIPRINU:"]
[]
[{"$nulls":5},"/______________/___________________/"]
[{"$nulls":5},"     Paraksts                             atšifrējums"]
[{"$nulls":7},"z.v."]
[{"$nulls":5},"2011. g.","\"_____  \"________________"]
["Kopsavilkums"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[]
[null,null,"Cilvēkstundas: ",0]
[null,null,"Tāme sastādīta:"]
["Tāmes nr.",null,"Tāmes nosaukums","Tiešās izmaksas BEZ PVN 22% Ls","Darba ietilpība C/st","Kopējās izmaksas, tai skaitā"]
[{"$nulls":5},"Dalba alga Ls","Materiāli Ls","Mehanismi Ls"]
["1",null,"Sagatavošanas darbi",0,0,0,0,0]
[2,null,"Vispārējie ēkas renovācijas darbi",0,0,0,0,0]
[3,null,"Ēkas elektroapgāde",0,0,0,0,0]
[4,null,"Apkures ierīkošana ēkā",0,0,0,0,0]
[5,null,"Ventilācija, gais apstrāde ēkā",0,0,0,0,0]
[6,null,"Ūdensapgāde ēkā",0,0,0,0,0]
[7,null,"Kanalizācija ēkā",0,0,0,0,0]
[8,null,"Drenāža",0,0,0,0,0]
[9,null,"Apsardze signalizācija",0,0,0,0,0]
[10,null,"Ugunsdrošības signalizācija",0,0,0,0,0]
[11,null,"Teritorijas labiekārtošanas darbi",0,0,0,0,0]
[12,null,"Ceļi un laukumi",0,0,0,0,0]
[13,null,"Ārējais ūdenvads",0,0,0,0,0]
[14,null,"Ārējā saimnieciskā kanalizācija",0,0,0,0,0]
[null,null,"Tiešās izmaksas kopā Ls:",0,0,0,0,0]
[null,null,"Materiālu sagāde, transports ...% Ls:"]
[null,null,"Uzņēmuma virsizdevumi ...% Ls:"]
[null,null,"Plānotie uzkrājumi ...% Ls:"]
[null,null,"Neparedzētie izdevumi 4% Ls:"]
[null,null,"Darba devēja sociālais nodoklis 24.09% Ls:",0]
[null,null,"Kopā bez PVN 22% Ls:",0]

{"sheet":"1","index":2,"n_rows":24,"n_cols":17,"rows_kept":24,"cut":false,"hidden":false,"merged":[[21,0,21,4],[9,7,9,10],[9,16,12,16],[10,7,10,10],[9,12,9,15],[10,12,10,15],[0,0,0,15],[1,0,1,15],[7,11,7,12],[8,0,8,2],[8,11,8,12],[6,11,6,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 1"]
["Sagatavošanas darbi",{"$nulls":15},"Sagatavošanas darbi"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"1. Būvniecības objekta izkārtnes sagatavošana un uzstādīšana","vien.",1,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"2. Metāla konteinera  (inventārs, sadzīves telpa, birojs) uzstādīšana, noma","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"3. Biotualetes uzstādīšana, noma","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"4. Pagaidu nojume materiālu uzglabāšanai","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"5. Pagaidu elektrības pieslēguma ierīkošana būvniecības vajadzībām","kpl.",1,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"6. Mēneša maksa par elektrības izmantošanu","mēn.",5,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"2","index":3,"n_rows":403,"n_cols":17,"rows_kept":403,"cut":false,"hidden":false,"merged":[[9,16,12,16],[10,7,10,10],[9,12,9,15],[10,12,10,15],[400,0,400,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[9,7,9,10]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 2"]
["Vispārējie ēkas renovācijas darbi",{"$nulls":15},"Vispārējie ēkas renovācijas darbi"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,null,"1. Demontāžas darbi."]
[null,null,"1.1. Esošā jumta seguma nojaukšanas darbi (azbocementa loksnes), ar latojumu zem tām (ieskaitot azbesta plātņu savākšanu un nodošanu specializētā izgāztuvē)","m²",187]
[null,null,"Darba algas","c/h",0.66]
[null,null,"1.2. Esošā jumta seguma demontāžas darbi (koka šindeļi), ieskaitot latas","m²",153]
[null,null,"Darba algas","c/h",0.86]
[null,null,"1.3. Ēkas galu apšuvumu demontāžas darbi","m²",27.2]
[null,null,"Darba algas","c/h",0.34]
[null,null,"1.4. Spāru konstrukcijas demontāžas darbi,nebojātās spāres saglabāt renovācijas darbu veikšanai","m³",5.7]
[null,null,"Darba algas","c/h",14]
[null,null,"1.5. Pārseguma dēļu klāja demontāžas darbi","m²",173]
[null,null,"Darba algas","c/h",0.38]
[null,null,"1.6. Pārseguma siju,mūrlatu demontāžas darbi, nebojātās sijas saglabāt tālākai renovācijas darbu veikšanai","m³",8.7]
[null,null,"Darba algas","c/h",18]
[null,null,"1.7. Esošo sienu apšuvumu nojaukšanas darbi","m²",235]
[null,null,"Darba algas","c/h",0.34]
[null,null,"1.8. Esošo koka starpsienu nojaukšanas darbi","m²",16.2]
[null,null,"Darba algas","c/h",0.3]
[null,null,"1.9. Esošo loga rāmju demontāžas darbi,saglabājot to restaurācijai (L~ 0,7m²)","gb.",4]
[null,null,"Darba algas","c/h",0.78]
[null,null,"1.10. Esošo durvju demontāžas darbi (L~2m²)","gb.",3]
[null,null,"Darba algas","c/h",1.4]
[null,null,"1.11. Esošo koka vārtu demontāžas darbi (L=4~5,3m²)","gb.",4]
[null,null,"Darba algas","gb.",1.86]
[null,null,"1.12. Bojātās ārsienas demontāžas darbi","m³",16]
[null,null,"Darba algas","c/h",1.84]
[null,null,"2. Pamati."]
[null,null,"2.1. Pamatu atrakšanas  darbi pa posmiem (roku darbs)","m3",70.6]
[null,null,"Darba algas","c/h",1.54]
[null,null,"2.2. Šķembu pamatojums zem pamata nostiprinājuma","m³",5]
[null,null,"Darba algas","c/h",0.8]
[null,null,"Grants drupinātas šķembas","m³",1.1]
[null,null,"2.3. Koka veidņu uzstādīšana/nojaukšana pamatu pastiprināšanas betonēšanas darbiem","m²",35.3]
[null,null,"Darba algas","c/h",0.68]
[null,null,"Kokmateriāli veidņiem","m³",0.06]
[null,null,"Naglas","kg",0.1]
[null,null,"2.4. Stiegru  d=10 AIII sagatavošana, sagriešana, marķēšana betonēšanas darbiem, pamatu pastiprināšanai","m",621]
[null,null,"Darba algas","c/h",0.03]
[null,null,"Stiegras d-10AIII","m",1.05]
[null,null,"2.5. Stiegru  d=6 AIII sagatavošana, sagriešana, marķēšana betonēšanas darbiem, pamatu pastiprināšanai","m",276]
[null,null,"Darba algas","c/h",0.03]
[null,null,"Stiegras d-6AIII","m",1.05]
[null,null,"2.6. Betona masas iestrāde ar sūkni, vibrēšana B20, zem pamatiem,to nostiprināšanai","m³",9.5]
[null,null,"Darba algas","c/h",11.3]
[null,null,"Betons B 20","m³",1.05]
[null,null,"2.7. Drenāžas caurules Dn=110mm ielikšana tranšejā ap ēkas pamatiem","m",76]
[null,null,"Darba algas","c/h",0.4]
[null,null,"Drenāžas caurule Dn110","m",1.03]
[null,null,"2.8. Šķembu apbērums ap pamatiem","m³",7.9]
[null,null,"Darba algas","c/h",0.8]
[null,null,"Grants drupinātas šķembas","m³",1.1]
[null,null,"2.9. Apbērt nostiprinātos pamatus ar granti","m³",39]
[null,null,"Grants","m³",1.05]
[null,null,"2.10. Izņemt grīdas pildījumu (atlikušās grīdas konstrukcijas,atkritumi,kūtsmēsli) ēkas telpās, roku darbs","m³",68]
[null,null,"Darba algas","c/h",2.67]
[null,null,"2.11. Izrakt pamatu vietas lentveida un stabveida pamatiem telpās, roku darbs","m³",7.9]
[null,null,"Darba algas","c/h",1.54]
[null,null,"2.12. Koka veidņu uzstādīšana/nojaukšana pamatu izbūvei telpās","m²",22.7]
[null,null,"Darba algas","c/h",0.68]
[null,null,"Kokmateriāli veidņiem","m³",0.06]
[null,null,"Naglas","kg",0.1]
[null,null,"2.13. Betona masas iestrāde lentveida pamatiem ar sūkni, vibrēšana B20","m³",3.3]
[null,null,"Darba algas","c/h",0.6]
[null,null,"Betons B 20","m³",1.05]
[null,null,"2.14. Betona masas iestrāde stabveida pamatiem ar sūkni, vibrēšana B20","m³",0.4]
[null,null,"Darba algas","c/h",1.58]
[null,null,"Betons B 20","m³",1.05]
[null,null,"2.15. Pamatu hidroizolācija, horizontālā","m2",4.2]
[null,null,"Darba algas","c/h",0.4]
[null,null,"Bituma aukstā mastika","l",1.2]
[null,null,"Ruberoids","m2",2.1]
[null,null,"3. Sienas 1.stāvam."]
[null,null,"3.1. Akmens mūra sienu atjaunošanas darbi (b=60cm) no neregulāras formas laukakmeņiem un kaļķu javā ar minimālu baltā cementa piedevu","vien.",22.5]
[null,null,"Darba algas","c/h",9.66]
[null,null,"Laukakmeņi","m³",1.03]
[null,null,"Kaļķu-cementa java","m³",0.37]
[null,null,"3.2. Māla ķieģeļu mūrējums pie noturības joslas izbūves virs akmensmūra sienām pa ēkas perimetru un šķērssienām","m³",5.4]
[null,null,"Darba algas","c/h",6.86]
[null,null,"Māla ķieģeļi,celtniecības, pilnie","gb.",400]
[null,null,"Mūrjava","m³",0.22]
[null,null,"3.3. Stiegru  d=10 AIII sagatavošana, sagriešana, marķēšana joslas betonēšanas darbiem","m",260]
[null,null,"Darba algas","c/h",0.03]
[null,null,"Stiegras d-10AIII","m",1.05]
[null,null,"3.4. Tērauda enkuru (stīpdzelzs -5x50mm; l=40cm) uzstādīšana pārseguma siju noenkurošanai","gb.",34]
[null,null,"Darba algas","c/h",0.1]
[null,null,"Tērauda enkuri ","gb.",1]
[null,null,"3.5. Betona masas iestrāde ar sūkni, vibrēšana B20 monolītās joslas izbūvei virs akmens sienām","m³",4.9]
[null,null,"Darba algas","c/h",11.3]
[null,null,"Betons B 20","m³",1.05]
[null,null,"3.6. Koka statu karkasa uzstādīšana  1.stāvā (kokmateriāli no atgūtajām koka konstrukcijām)","m³",3]
[null,null,"Darba algas","c/h",24]
[null,null,"Atgūtie kokmateriāli",null,1]
[null,null,"3.7. Akmensmūra sienu bojāto virsmu attīrīšana ar drāšu suku un ūdens strūklu (fasādē un telpās)","10m²",35.3]
[null,null,"Darba algas","c/h",17]
[null,null,"3.8. Akmensmūra virsmas šuvju, izdrupumu aizdare izmantojot kaļķu javu, javā iespiežot melnos sīkakmeņus","m²",353]
[null,null,"Darba algas","c/h",0.65]
[null,null,"Kaļķa java","m3",0.04]
[null,null,"Akmeņi-melni, sīki","m³",0.01]
[null,null,"3.9. Koka karkass 5x15cm, ar siltumizolāciju, AL folliju, tvaika izolāciju gar ārsienām sienas (b=150mm), ","m²",30]
[null,null,"Darba algas","c/h",2.59]
[null,null,"AL follija","m²",1.1]
[null,null,"Akmens vate 150mm","m2",0.9]
[null,null,"Kokmateriāli 5*150cm","m³",0.017]
[null,null,"Skrūves, dībeļi","komplekts",6]
[null,null,"Tvaika izolācijas plēve","m2",1.1]
[null,null,"3.10. Koka karkasa sienas 5x15cm, siltinātas ar akmensvates plātnēm  15cm, tvaika izolācija","m2",12.2]
[null,null,"Darba algas","c/h",1.46]
[null,null,"Zāģmateriāli 5*15 cm","m³",0.016]
[null,null,"Stiprin.elementi","gab.",3]
[null,null,"Akmensvates plātnes 15cm","m²",0.9]
[null,null,"Tvaika izolācijas plēve","m²",1.1]
[null,null,"3.11. Iekšsienu apšuvums ar spundētiem dēļiem","m²",63]
[null,null,"Darba algas","c/h",0.42]
[null,null,"Apšuvuma dēļi 18mm, ar spundi","m²",1.05]
[null,null,"Celtniecības naglas","kg",0.06]
[null,null,"3.12. Koka karkasa sienas pildiņu iebūve b=20cm, savienojot ar tapām (kokmateriāli no demontētajām konstrukcijām)","m²",17.5]
[null,null,"Darba algas","c/h",0.65]
[null,null,"3.13. Apšūt sienas ar  mitrumizturīgo ģipškartonu","m2",45.6]
[null,null,"Darba algas","c/h",0.67]
[null,null,"Ģipškartons, mitrumizturīgais","m2",1.1]
[null,null,"Riģipša skrūves 25mm","gab.",24]
[null,null,"Šuvju lente","m",1.8]
[null,null,"Špahtele Uniflot","kg",0.8]
[null,null,"3.14. Sienu virsmu sagatavošana krāsošanas darbiem","m²",45.6]
[null,null,"Darba algas","c/h",0.45]
[null,null,"Špahteļmasa","l",2]
[null,null,"3.15. Sienu virsmu tonēts augstvērtīgs krāsojums","m²",45.6]
[null,null,"Darba algas","c/h",0.6]
[null,null,"Gruntskrāsa Robitix","l",0.125]
[null,null,"Krāsa Dekor ar toni","l",0.25]
[null,null,"3.16. Koka konstrukciju apstrāde ar bezkrāsainu pretpuves sastāvu","m²",84.2]
[null,null,"Darba algas","c/h",0.27]
[null,null,"Pretpuves sastāvs","l",0.3]
[null,null,"4. Pārsegums."]
[null,null,"4.1. Pārseguma pasiju uzstādīšana 20x25cm","m³",0.71]
[null,null,"Darba algas","c/h",24]
[null,null,"Kokmateriāli","m³",1.05]
[null,null,"Stiprinājumi","kg",7]
[null,null,"4.2. Pārseguma siju un izmiju iebūve 20x25(h)cm","m³",6.72]
[null,null,"Darba algas","c/h",24]
[null,null,"Kokmateriāli 20x25cm","m3",1.05]
[null,null,"Pape","m²",3.28]
[null,null,"Latas 5x5cm","m³",0.041]
[null,null,"Stiprinājumi","kg",7]
[null,null,"Celtniecības naglas","kg",0.1]
[null,null,"4.3. Apšuvums \"trinītī\" starp pārseguma sijām b=2,5cm","m²",148.3]
[null,null,"Darba algas","c/h",0.94]
[null,null,"Dēļi, collīgie, ar bomkanti","m³",0.04]
[null,null,"Celtniecības naglas","kg",0.15]
[null,null,"4.4. Grīdas gulšņu iebūve virs pārseguma sijām 5x10(h)cm, s=60cm","m²",127.6]
[null,null,"Darba algas","c/h",0.3]
[null,null,"Grīdas gulšņi","m³",0.013]
[null,null,"Celtniecības naglas","kg",0.07]
[null,null,"4.5. Akmensvates siltumizolācijas plātņu ieklājums starp gulšņiem b=10cm","m²",72.4]
[null,null,"Darba algas","c/h",0.1]
[null,null,"Akmensvates plātens 100mm","m²",0.95]
[null,null,"4.6. Tvaika izolācijas plēve","m²",72.4]
[null,null,"Darba algas","c/h",0.1]
[null,null,"Tvaika izolācijas plēve","m2",1.1]
[null,null,"4.7. Koka konstrukciju apstrāde ar bezkrāsainu pretpuves sastāvu","m²",283]
[null,null,"Darba algas","c/h",0.27]
[null,null,"Pretpuves sastāvs","l",0.3]
[null,null,"5. Kāpņu izbūve."]
[null,null,"5.1. Kāpņu izbūve (kāpnes - namdaru,ar \"vaigos\" (~7x22cm) ielaistiem pakāpieniem (5x24(b)cm","m²",28.5]
[null,null,"Darba algas","c/h",4.8]
[null,null,"Kokmateriāli","m³",0.02]
[null,null,"5.2. Vienkāršotu koka margu izbūve kāpnēm un atvērumam ap tām","m",12.2]
[null,null,"Darba algas","c/h",0.5]
[null,null,"Zāģmateriāli","m³",0.02]
[null,null,"6. Jumta nesošās konstrukcijas, segums."]
[null,null,"6.1. Mūrlatas uzstādīšanas darbi","m³",1.19]
[null,null,"Darba algas","c/h",24]
[null,null,"Kokmateriāli 15x15cm","m³",1.05]
[null,null,"Stiprinājumi","kg",7]
[null,null,"6.2. Spāru konstrukcijas izbūve 15x15cm, iesējums ar tapām, spāres nostiprināt ar tērauda iedzītņiem pie pārseguma sijām","m³",5.66]
[null,null,"Darba algas","c/h",36]
[null,null,"Kokmateriāli 15x15cm","m³",1.05]
[null,null,"Tērauda iedzītņi d=16mm; Lkop=750mm","gb.",6]
[null,null,"6.3. Sieta iebūve pie spāru un sienas salaiduma kukaiņu aizturēšanai","m²",9.2]
[null,null,"Darba algas","c/h",0.18]
[null,null,"Siets","m²",1.15]
[null,null,"Palīgmateriāli","vien.",1]
[null,null,"6.4. Latojums virs spārēm no egles koka kārtīm d=~50mm,s=30cm","m²",195]
[null,null,"Darba algas","c/h",0.23]
[null,null,"Egļu koka kārtis d=5cm","m³",0.008]
[null,null,"Celtniecības naglas","kg",0.083]
[null,null,"6.5. Latojums virs spārēm no latām 5x5cm,s=30cm","m²",145]
[null,null,"Darba algas","c/h",0.23]
[null,null,"Latas 5x5cm","m³",0.008]
[null,null,"Celtniecības naglas","kg",0.083]
[null,null,"6.6. Egles koka šindeļu segums trīs kārtās ar impregnētām skaidām virs latām","m²",334]
[null,null,"Darba algas","c/h",0.77]
[null,null,"Egles koka šindeļi","m²",1.03]
[null,null,"Šindeļu naglas","kg",0.2]
[null,null,"Dēļi","m3",0.001]
[null,null,"6.7. Koka konstrukciju apstrāde ar bezkrāsainu pretpuves sastāvu","m²",183]
[null,null,"Darba algas","c/h",0.27]
[null,null,"Pretpuves sastāvs","l",0.3]
[null,null,"6.8. Notekrenes uzstādīšana virs staļļa vārtiem (no izgrebta koka, d~18cm)","m",3]
[null,null,"Darba algas","c/h",0.7]
[null,null,"Materiāli","m",1]
[null,null,"Stiprinājumi","gb.",1.7]
[null,null,"7. Sienas bēniņu izbūvei."]
[null,null,"7.1. FIBO bloku mūris 3MPa, 20cm, bēniņstāva telpās","m³",3]
[null,null,"Darba algas","c/h",3.11]
[null,null,"Armatūra","kg",12]
[null,null,"Cementa java","m3",0.15]
[null,null,"FIBO bloki 3MPa","m3",0.96]
[null,null,"7.2. Fibo bloku mūra apšuvums ar dēļiem \"trinītī\"virs latu 4x4cm karkasa","m²",26.8]
[null,null,"Darba algas","c/h",0.72]
[null,null,"Latas 4x4cm","m³",0.0034]
[null,null,"Apšuvuma dēļi b=22mm","m³",0.035]
[null,null,"Celtniecības naglas","kg",0.07]
[null,null,"7.3. Pretvēja izolācija  Paroc WAS 25t - 30mm (vai analoga) starp spārēm","100m²",1.16]
[null,null,"Darba algas","c/h",40]
[null,null,"Latas 5x5cm","m³",0.525]
[null,null,"Celtniecības naglas","kg",8.3]
[null,null,"Paroc WAS 25t - 30mm","m²",94]
[null,null,"7.4. Akmens vates izolāciju iestrādāt starp spārēm b=50mm","100m²",1.16]
[null,null,"Darba algas","c/h",18]
[null,null,"Akmens vate 50mm","m2",90]
[null,null,"7.5. Šķērslatas 50x100 mm zem spārēm, solis 600mm","m³",1.22]
[null,null,"Darba algas","c/h",24]
[null,null,"Antiseptiķis","kg",3.1]
[null,null,"Naglas, skrūves un leņķa savienojumi","kg",10.6]
[null,null,"Zāģmateriāli","m3",1.05]
[null,null,"7.6. Akmens vates izolāciju iestrādāt starp latām b=100mm","100m²",1.16]
[null,null,"Darba algas","c/h",18]
[null,null,"Akmens vate 100mm","m2",90]
[null,null,"7.7. Tvaika izolācijas plēves ieklājums zem spārēm, nostiprinot ar latām 25mm","m²",116]
[null,null,"Darba algas","c/h",0.4]
[null,null,"Tvaika izolācijas plēve","m²",1.15]
[null,null,"Latas 50x25mm","m³",0.004]
[null,null,"7.8. Koka statņu sienu karkasu  50x150 mm, izbūve bēniņstāva telpās ierīkojot logu un durvju ailes projektā norādītajās vietās","m3",1.28]
[null,null,"Darba algas","c/h",24]
[null,null,"Antiseptiķis","kg",3.1]
[null,null,"Naglas, skrūves un leņķa savienojumi","kg",10.6]
[null,null,"Zāģmateriāli","m3",1.08]
[null,null,"7.9. Koka konstrukciju apstrāde ar bezkrāsainu pretpuves sastāvu","m²",124.4]
[null,null,"Darba algas","c/h",0.27]
[null,null,"Pretpuves sastāvs","l",0.3]
[null,null,"7.10. Pretvēja izolācija  Paroc WAS 25t - 30mm (vai analoga)  ārsienu daļā bēniņstāva telpās","100m²",0.14]
[null,null,"Darba algas","c/h",40]
[null,null,"Paroc WAS 25t - 30mm","m²",94]
[null,null,"7.11. Akmens vates izolāciju iestrādāt starp karkasa statņiem b=150mm","100m²",0.29]
[null,null,"Darba algas","c/h",18]
[null,null,"Akmens vate 150mm","m2",90]
[null,null,"7.12. Tvaika izolācijas plēves ieklājums sienās","m²",29]
[null,null,"Darba algas","c/h",0.4]
[null,null,"Tvaika izolācijas plēve","m²",1.15]
[null,null,"7.13. Virsmu apšuvums ar spundētiem dēļiem bēniņstāva telpās","m²",88.6]
[null,null,"Darba algas","c/h",0.42]
[null,null,"Apšuvuma dēļi 18mm, ar spundi","m²",1.05]
[null,null,"Celtniecības naglas","kg",0.06]
[null,null,"7.14. Apšūt sienas ar  mitrumizturīgo ģipškartonu muzeja krātuvē un tās priekštelpā","m2",134.9]
[null,null,"Darba algas","c/h",0.67]
[null,null,"Ģipškartons, mitrumizturīgais","m2",1.1]
[null,null,"Riģipša skrūves 25mm","gab.",24]
[null,null,"Šuvju lente","m",1.8]
[null,null,"Špahtele Uniflot","kg",0.8]
[null,null,"7.15. Riģipša sienu virsmu sagatavošana krāsošanas darbiem","m²",134.9]
[null,null,"Darba algas","c/h",0.45]
[null,null,"Špahteļmasa","l",2]
[null,null,"7.16. Riģipša sienu virsmu tonēts augstvērtīgs krāsojums","m²",134.9]
[null,null,"Darba algas","c/h",0.6]
[null,null,"Gruntskrāsa Robitix","l",0.125]
[null,null,"Krāsa Dekor ar toni","l",0.25]
[null,null,"7.17. Ārsienu apšuvums ar collīgajiem dēļiem \"trinītī\"(ar bomkanti) bēniņu izbūvei","m²",25.6]
[null,null,"Darba algas","c/h",0.42]
[null,null,"Dēļi 25mm, ar bomkanti","m³",0.04]
[null,null,"Celtniecības naglas","kg",0.06]
[null,null,"8. Ailes."]
[null,null,"8.1. Esošo logailu rāmju restaurācija (izmantojot demontētos kokmateriālus)un atpakaļiebūve","m2",1.38]
[null,null,"Darba algas","c/h",12]
[null,null,"8.2. Logu rāmja iebūves darbi (vienstikla rāmis + vasaras sezonas laikā izņemams rāmis)","m2",0.74]
[null,null,"Darba algas","c/h",4.5]
[null,null,"Ailes aizpildījuma rāmji","m2",1]
[null,null,"8.3. Logs, koka ar divkāršu stiklojumu,L-4, rāmis verams uz āru, kā durvis. Logam priekšā slēģi (D-4) ar slēdzeni iekšpusē.","kpl.",1]
[1,null,"Darba algas","c/h",8]
[2,null,"Logu bloks","m2",2.11]
[3,null,"Koka slēģi","m²",2.11]
[4,null,"Stiprinājumi","gab.",6]
[5,null,"Slēdzene","kpl.",1]
[6,null,"8.4. Vārtu un durvju ailu malu aplodojuma renovācijas darbi (nostiprināšana, darvošana)","m",52]
[7,null,"Darba algas","c/h",0.5]
[8,null,"Brusas 12x12, ozolkoka","m³",0.015]
[9,null,"Priežu darva","kg",0.2]
[10,null,"8.5. Vārtu bloks V-1(4,33m²). Vārtu vērtnes no divu dēļu klāja, ārējais ar puspundi. Izmantojamas vecās vērtnes eņģes. Atslēga - iekaļamā, atbilstoša laika periodam 1849-1930. Ailei izņemams koka slieksnis.","kpl.",1]
[11,null,"Darba algas","c/h",16]
[12,null,"Vārtu vērtnes","m²",4.33]
[13,null,"Piekaramās atslēgas kronšteins","kpl.",1]
[14,null,"Iekaļamā atslēga","kpl.",1]
[15,null,"8.6. Vārtu bloks V-2(3,13m²). Vārtu vērtnes no divu dēļu klāja, ārējais ar puspundi. Izmantojamas vecās vērtnes eņģes, vērtņu krampji. Atslēga - iekaļamā, atbilstoša laika periodam 1849-1930. Ailei izņemams koka slieksnis.","kpl.",1]
[15,null,"Darba algas","c/h",16]
[16,null,"Vārtu vērtnes","m²",3.13]
[16,null,"Priekškaramās atslēgas kronšteins","kpl.",1]
[17,null,"Iekaļamā atslēga","kpl.",1]
[18,null,"Krampis","kpl.",2]
[19,null,"8.7. Vārtu bloks V-3 (4,64m²). Vārtu vērtnes no divu dēļu klāja, ārējais ar puspundi. Izmantojamas vecās vērtnes eņģes, vērtņu krampji. Atslēga - iekaļamā, atbilstoša laika periodam 1849-1930. Ailei izņemams koka slieksnis.","kpl.",2]
[20,null,"Darba algas","c/h",20]
[21,null,"Vārtu vērtnes","m²",4.64]
[22,null,"Priekškaramās atslēgas kronšteins","kpl.",1]
[23,null,"Iekaļamā atslēga","kpl.",1]
[24,null,"Vārtu eņģes","kpl.",2]
[25,null,"8.8. Ārdurvju bloks D-1 (1,68m²). Vērtne no divu dēļu klāja, ārējais ar puspundi. Daļēji izmantojamas vecās vērtnes eņģes. Atslēga - iekaļamā, atbilstoša laika periodam 1849-1930. Ailei izņemams koka slieksnis.","kpl.",2]
[26,null,"Darba algas","c/h",20]
[27,null,"Durvju vērtne","m²",1.68]
[28,null,"Priekškaramās atslēgas kronšteins","kpl.",1]
[29,null,"Iekaļamā atslēga","kpl.",1]
[30,null,"Ēņģes","kpl.",2]
[31,null,"8.9. Ārējās lūkas bloks Lū-1 (0,81m²). Vērtne no divu dēļu klāja, ārējais ar puspundi. Izmantojamas vecās vērtnes eņģes. Atslēga - priekškaramā, atbilstoša laika periodam 1849-1930","kpl.",1]
[32,null,"Darba algas","c/h",20]
[33,null,"Lūkas vērtne","m²",0.81]
[34,null,"Atslēga","kpl.",1]
[35,null,"8.10. Lūkas bloks, namdaru, D-3 (1,5m²). Izmantojamas vecās vērtnes eņģes. Atslēga - priekškaramā, atbilstoša laika periodam 1849-1930","kpl.",1]
[36,null,"Darba algas","c/h",20]
[37,null,"Lūkas vērtne","m²",1.5]
[38,null,"Atslēga","kpl.",1]
[39,null,"8.11. Iekšdurvju bloku iebūve D-2 (1,78m²). Divu dēļu klāju konstrukcijā.Ar eņģēm un atslēgām","kpl.",3]
[40,null,"Darba algas","c/h",2]
[41,null,"Durvju bloks","m²",1.78]
[42,null,"Eņģes","gb.",2]
[43,null,"Atslēgas","kpl.",1]
[44,null,"9. Grīdas."]
[45,null,"9.1. Grīdas segums ar grīdas dēļiem 32mm (b=20-25cm), ieskaitot grīdlīstes bēniņstāva telpās","m²",106.3]
[46,null,"Darba algas","c/h",0.8]
[47,null,"Grīdas dēļi 32mm","m²",1.05]
[48,null,"Grīdlīstes","m",1.03]
[49,null,"Naglas","kg",0.23]
[50,null,"9.2. Grīdas dēļu apstrāde ar lineļļu divās kārtās","m²",106.3]
[51,null,"Darba algas","c/h",0.49,null,null,0,null,null,0,0,0,0,0,0]
[52,null,"Lineļļa","l",0.67,null,null,0,null,null,0,0,0,0,0,0]
[53,null,"9.3. Grīdas segums kūtsaugšā b=45mm","m²",41.8,null,null,0,null,null,0,0,0,0,0,0]
[54,null,"Darba algas","c/h",0.6,null,null,0,null,null,0,0,0,0,0,0]
[55,null,"Dēļi 45mm","m³",0.048,null,null,0,null,null,0,0,0,0,0,0]
[56,null,"Naglas","kg",0.5,null,null,0,null,null,0,0,0,0,0,0]
[57,null,"9.4. Blietēta grunts pirmā stāva grīdām","m²",159.5,null,null,0,null,null,0,0,0,0,0,0]
[58,null,"Darba algas","c/h",0.1,null,null,0,null,null,0,0,0,0,0,0]
[59,null,"9.5. Vājbetons B5 50mm biezumā grīdā muzeja darbnīcā un saimniecības telpā, ailēs","m³",2.1,null,null,0,null,null,0,0,0,0,0,0]
[60,null,"Darba algas","c/h",2.9,null,null,0,null,null,0,0,0,0,0,0]
[61,null,"Betons B 5","m³",1.05,null,null,0,null,null,0,0,0,0,0,0]
[62,null,"9.6. Hidroizolācijas kārta 1.stāva telpās ","m²",36.6]
[63,null,"Darba algas","c/h",0.33]
[64,null,"Akrila hidroizolācija omis","l",0.5]
[65,null,"9.7. Siltumizolācijas slānis 1.stāva telpās 100mm (EPS 150) muzeja darbnīcas telpā","m²",10.7]
[66,null,"Darba algas","c/h",0.1]
[67,null,"Tenapors EPS 150","m²",1.05]
[68,null,"9.8. Betona nesošais slānis B25 zem grīdu seguma 1.stāvā -60mm, ar stiegru sietu 5/5/100/100","m²",41.4]
[69,null,"Darba algas","c/h",1.3]
[70,null,"Betons B25 ","m³",0.063]
[71,null,"Stiegru siets 5/5/100/100","m²",1.1]
[72,null,"9.9. Grīdas segums ar pilnajiem māla ķieģeļiem 65mm","m²",41.4]
[73,null,"Darba algas","c/h",0.8]
[74,null,"Māla pilnie ķieģeli b=65mm","gb.",35,null,null,0,null,null,0,0,0,0,0,0]
[75,null,"Smilts","m³",0.01]
[76,null,"9.10. Smilts pamatojuma kārta 10cm","m³",17.8]
[77,null,"Darba algas","c/h",3]
[78,null,"Smilts","t",1.58]
[79,null,"9.11. Oļu pamatojuma kārta grīdām 15cm","m³",17.8]
[80,null,"Darba algas","c/h",3.19]
[81,null,"Oļi ,fr.20-40","t",1.68]
[82,null,"9.12. Hidroizolācijas plēve grīdām vāgūžos, klētī","m²",118.1]
[83,null,"Darba algas","c/h",0.1]
[84,null,"Hidroizolācijas plēve","m²",1.2]
[85,null,"9.13. Betona izlīdzinošais slānis B20 zem grīdu seguma 1.stāvā -60mm","m²",118.1]
[86,null,"Darba algas","c/h",0.6]
[87,null,"Betons B20","m³",0.063]
[88,null,"9.14. Antiseptētu grīdas lagu uzstādīšana 75x100mm, s=60cm, zem dēļu grīdām","m²",118.1]
[89,null,"Darba algas","c/h",0.3]
[90,null,"Lagas 75x100mm","m³",0.012]
[91,null,"9.15. Grīdas segums ar  dēļiem 40mm (b=18-27cm), 1.stāva telpās","m²",118.1]
[92,null,"Darba algas","c/h",0.8]
[93,null,"Dēļi 40mm","m²",1.05]
[94,null,"Naglas","kg",0.3]
[95,null,"9.16. Dēļu apstrāde ar lineļļu divās kārtās","m²",118.1,null,null,0,null,null,0,0,0,0,0,0]
[96,null,"Darba algas","c/h",0.49]
[97,null,"Lineļļa","l",0.87]
[98,null,"10. Aizgaldu izbūve"]
[99,null,"10.1. Apcirkņu un aizgaldu noturošais karkass no mizota ozolkoka apaļkoka","m²",54]
[100,null,"Darba algas","c/h",0.26]
[101,null,"Ozolkoka zāģmateriāli","m³",0.028]
[102,null,"10.2. Apcirkņu un aizgaldu sienas no mizotām skujkoku kārtīm, dēļiem","m²",54]
[103,null,"Darba algas","c/h",0.4]
[104,null,"Skujkoku zāģmateriāli, mizoti","m³",0.053]
[105,null,"10.3. Dēļu grīdas apcirkņos no skujkoku materiāla 45x18-24mm, kam nomaļu mala pietesta","m²",29.6,null,null,0,null,null,0,0,0,0,0,0]
[106,null,"Darba algas","c/h",0.65,null,null,0,null,null,0,0,0,0,0,0]
[107,null,"Skujkoku dēļi ~24mm","m²",1.05]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"3","index":4,"n_rows":75,"n_cols":17,"rows_kept":75,"cut":false,"hidden":false,"merged":[[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[9,16,12,16],[9,7,9,10],[10,7,10,10],[72,0,72,4],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 3"]
["Ēkas elektroapgāde",{"$nulls":15},"Ēkas elektroapgāde"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Apg. armat IP54 1x36w d/g pie sienas","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Apg. armatūra IP65 ar sp. 2X36W TORNADO","gab.",10,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Apg. Spuldze 15w ekonom E27","gab.",5,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Apg. Spuldze Hi-Spot ReflLED PAR30 10W Warm White","gab.",40,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Gaismeklis IP65 230V NEPA MAX OUTDOOR BRAS E27","gab.",40,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Gaismeklis IP65 230V PORTO 6 BRAS E27","gab.",5,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Automātslēdzis PL6-B10/1","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Automātslēdzis PL6-B16/1","gab.",10,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Automātslēdzis PL6-B16/3","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Automātsl.s diferenc. aizsardz. 40A/0.1 4p","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Caurule lokana plastmasas melna D20 KABUFLEX","m",45,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Caurule lokana plastmasas melna D32 KABUFLEX","m",65,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"Caurule lokana plastmasas pelēka IPS16F 320N","m",800,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Kabelis CYKY 3x2.5","m",50,null,null,0,null,null,0,0,0,0,0,0]
[13,null,"Kabelis CYKY 5x6","m",67,null,null,0,null,null,0,0,0,0,0,0]
[14,null,"Kabelis NYM (MMJ) 3x1.5","m",1400,null,null,0,null,null,0,0,0,0,0,0]
[15,null,"Kabelis FTP CAT5E 4x2x0.5","m",30,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"Kabeļa kanāls PVC 18X18mm brūns","m",40,null,null,0,null,null,0,0,0,0,0,0]
[17,null,"Kabeļa kanāls PVC 130x60mm","m",4,null,null,0,null,null,0,0,0,0,0,0]
[18,null,"Kontaktdakša 3P+N+E 16A IP44 V/A","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"Kontakt rozete 3P+N+E 16A IP44 V/A","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"Lenta \"Kabelis\" 40mm dzeltena","m",100,null,null,0,null,null,0,0,0,0,0,0]
[21,null,"Nozarkārba 1v PK 1x60 z/a","gab.",7,null,null,0,null,null,0,0,0,0,0,0]
[22,null,"Nozarkārba 2v PK 2x60 z/a","gab.",15,null,null,0,null,null,0,0,0,0,0,0]
[23,null,"Nozarkārba 3v PK 3x60 z/a","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[24,null,"Nozarkārba 4v PK 4x60 z/a","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[25,null,"Rāmis 1v 2511-92-507 Basic 55 ABB","gab.",7,null,null,0,null,null,0,0,0,0,0,0]
[26,null,"Rāmis 2v 2512-92-507 Basic 55 ABB","gab.",15,null,null,0,null,null,0,0,0,0,0,0]
[27,null,"Rāmis 3v 2513-92-507 Basic 55 ABB","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[28,null,"Rāmis 4v 2514-92-507 Basic 55 ABB","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[29,null,"Rozetes meh. 2P+E z/a 20 EUC-92-507 Basic 55 ABB","gab.",21,null,null,0,null,null,0,0,0,0,0,0]
[30,null,"Rozetes meh. 2P+E z/a 20 EUK-92-507 Basic 55 ABB ar vāku","gab.",4,null,null,0,null,null,0,0,0,0,0,0]
[31,null,"Rozetes meh. DATA Basic 55 ABB","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[32,null,"Rozetes DATA vāciņš Basic 55 ABB","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[33,null,"Slēdža meh. 1p z/a 2006/1 UC-92-507 Basic 55 ABB","gab.",4,null,null,0,null,null,0,0,0,0,0,0]
[34,null,"Slēdža meh. 1p z/a 2006/6 UC-92-507 Basic 55 ABB pārsledzis","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[35,null,"Slēdža meh. 2p z/a 2006/5 UC-92-507 Basic 55 ABB","gab.",8,null,null,0,null,null,0,0,0,0,0,0]
[36,null,"Rozete IP44 v/a 16A 2P+E","gab.",8,null,null,0,null,null,0,0,0,0,0,0]
[37,null,"Sadalne KAEDRA  13986  36-MOD.   IP65","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[38,null,"Slēdzis-pārpslēdzis ģeneratora pieslēgšanai 3f 32A","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[39,null,"Vads PV-3 16mm2","m",15,null,null,0,null,null,0,0,0,0,0,0]
[40,null,"Zemējuma elektrods cinkots 219/20ST  1500mm","gab.",15,null,null,0,null,null,0,0,0,0,0,0]
[41,null,"Zemējuma elektroda spice 1819/20 BP","gab.",5]
[42,null,"Zemējuma stieple RD8 8mm FT zemē","m",70]
[43,null,"Zemējuma stieple RD8 8mm FT uz ēkas","m",65]
[44,null,"Savienojuma Spaile 2760/20 RD8-10/FL40","gab.",5]
[45,null,"Stiprin.elem. 113 Z-20","gab.",70]
[46,null,"Krusta klemme 251  8-10x8-10 FT","gab.",6]
[47,null,"Pārsprieguma aizsardzība V25-B+C/3+NPE","kompl.",1]
[48,null,"Palīgmateriāli (skavas, savilces, izol.lent, apzīmējumi.u.tml.)","kompl.",1]
[49,null,"Esošās instalācijas demontāža","cil.st.",2]
[50,null,"Izpilddokumentācija un elektriskie mērījumi","kompl.",1]
[51,null,"Tranšejas rakšana ar mehanismu","m",90,null,null,0,null,null,0,0,0,0,0,0]
[52,null,"Tranšejas rakšana ar roku darbu","m",6,null,null,0,null,null,0,0,0,0,0,0]
[53,null,"Sastatņu montāža, demontāža","100m2",2.9,null,null,0,null,null,0,0,0,0,0,0]
[54,null,"Sastaņu noma","m2",290,null,null,0,null,null,0,0,0,0,0,0]
[]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"4","index":5,"n_rows":22,"n_cols":17,"rows_kept":22,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[19,0,19,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 4"]
["Apkures ierīkošana ēkā",{"$nulls":15},"Apkures ierīkošana ēkā"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Konvektors Ensto Beta paneļtipa 719х389х85 750 W ar stipr.","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Konvektors Ensto Beta paneļtipa 853х389х85 1000 W ar stipr.","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Konvektors Ensto Beta paneļtipa 1121х389х85 1500 W ar stipr","kompl.",2,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Montāžas materiāli","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"5","index":6,"n_rows":39,"n_cols":17,"rows_kept":39,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[36,0,36,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 5"]
["Ventilācija, gais apstrāde ēkā",{"$nulls":15},"Ventilācija, gais apstrāde ēkā"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Kanāla ventilators  Mixvent TD 500/160","gab",1]
[2,null,"Kanāla ventilators  Mixvent TD 350/125","gab",1]
[3,null,"El slēdzis divātrumu Regul 2","gab",2]
[4,null,"Nosūces konuss  70x70 -uzstādīt ","gab",1]
[5,null,"Klusinātājs 160/600","gab",1]
[6,null,"Pretvārsts d 160","gab",1]
[7,null,"Pretvārsts d 125","gab",1]
[8,null,"Āra reste alumīnija 160","gab",1]
[9,null,"Āra reste alumīnija 125","gab",2]
[10,null,"Cinkotā skārda vītais gaisvads D 125","gab",4]
[11,null,"Cinkotā skārda vītais gaisvads D 160","gab",9]
[12,null,"Vīto gaisvadu veidgabali","k-ts",1]
[13,null,"Ventilācijas reste regulējama ND12R","gab",3]
[14,null,"Nosūces difuzors DVS 125","gab",3,null,null,0,null,null,0,0,0,0,0,0]
[15,null,"Plastm.reste  ND12","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"Gaisa susinātājs glabātavas telpām","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[17,null,"Mobīlais kondicionieris","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[18,null,"Lokanais gaisvads","m",5,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"Āra reste","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"Pieplūde durvīs","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[21,null,"Palīgmateriāli","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"6","index":7,"n_rows":32,"n_cols":17,"rows_kept":32,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[29,0,29,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 6"]
["Ūdensapgāde ēkā",{"$nulls":15},"Ūdensapgāde ēkā"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Vairākslāņu caurule Pe-Al-Pe d20","m",15,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Vairākslāņu caurule Pe-Al-Pe d16","m",12,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Veidgabali daudzslāņu caurulei","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Izolācija daudzslāņu caurulei","m",27,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Mehāniskais filtrs  ar ieliktni","kompl",2,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Lodveida krāns Dn 25","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Lodveida krāns Dn 20","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Lodveida krāns Dn 15","gab",8,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Manometrs 0-10 bar","gab",3,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Rokas izlietnes viensviras jaucējkrāns  ","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"Virtuves izlietnes viensviras jaucējkrāns","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Sant.ierīču pieslēgšanas ventīļi","gab",6,null,null,0,null,null,0,0,0,0,0,0]
[13,null,"Elektriskais boilers 50l","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[14,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"7","index":8,"n_rows":27,"n_cols":17,"rows_kept":27,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[24,0,24,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 7"]
["Kanalizācija ēkā",{"$nulls":15},"Kanalizācija ēkā"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Kanalizācijas plastmasas caurules D 110, fasondaļas, stiprinājumi","m",3,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Kanalizācijas plastmasas caurules D 50, fasondaļas, stiprinājumi","m",4,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Kanalizācijas caurule ārdarbiem D110","m",5,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Roku mazgājamā izl. ar krānu un sifonu fajansa 50x50","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Nerūsējošā tērauda vanna ar sifonu ","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Santehnisko objektu komplektācija, pieslēgšana ","kompl",3,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Trapa ierīkošana grīdā","vieta",1,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Montāžas materiāli santehniskajiem darbiem","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"8","index":9,"n_rows":27,"n_cols":17,"rows_kept":27,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[24,0,24,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 8"]
["Drenāža",{"$nulls":15},"Drenāža"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Caurule PVC D=100 drenāžai perforēta,veidgabali","m",80,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Caurule PVC D=125 drenāžai bez perforācijas,savienojumi","m",10,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Drenāžas skataka Veto 315 ar vāku un pamatni","kts",5,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Tranšejas rakšana cauruļvadu montāžai mehanizēti","m³",20,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Liekās grunts aizvešana līdz 0.5 km attālumam","m³",20,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Oļu-šķembu (fr. 8-16), grants apbērums drenāžas sistēmai","m³",2.6,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Izvada ierīkošana esošajā dīķī","vieta",1,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Tranšejas aizbēršana (smilts)","m³",17]
[9,null,"Digitālā uzmērīšana","aka",5,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"9","index":10,"n_rows":37,"n_cols":17,"rows_kept":37,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[34,0,34,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 9"]
["Apsardze signalizācija",{"$nulls":15},"Apsardze signalizācija"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Kontroles panelis \"Texecom\"","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Zonu paplašinātājs \"Texecom\"","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Akumolatoru baterija 12v/7ah","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Vadības pults LED","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Vadības pults LCD","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Sirēna SEM 923","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Kustību signāldevējs RX-40","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Kronšteins","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Barošanas bloks ar akumulatoru","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Sirēna MR 300","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"Raidītājs ar antenu","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Kabelis 12x0,22","m",200,null,null,0,null,null,0,0,0,0,0,0]
[13,null,"Kabelis 3x1,5","m",15,null,null,0,null,null,0,0,0,0,0,0]
[14,null,"Kabelis 30x2x0,5","m",60,null,null,0,null,null,0,0,0,0,0,0]
[15,null,"Montāžas kārba","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"Gofrēta caurule d-32","m",10,{"$nulls":6},0,null,0,0]
[17,null,"Sistēmas pārbaude, regulēšana","k-ts",1,{"$nulls":6},0,null,0,0]
[18,null,"Izpilddokumentācija","k-ts",1]
[19,null,"Palīgmateriāli","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"10","index":11,"n_rows":30,"n_cols":17,"rows_kept":30,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[27,0,27,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 10"]
["Ugunsdrošības signalizācija",{"$nulls":15},"Ugunsdrošības signalizācija"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Kontroles panelis Bentel J 408-8","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Dūmu detektors NB 338-2","gab",11,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Rokas signāldevējs FP/3RD","gab",7,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Sirēna LD 96","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Sirēna MR 300","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Akumolātoru baterija 12v/7Ah","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Kabelis KLM 1x2x0,8","m",180,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Kabelis EUROSAFE 2x0,8","m",80,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"PVC caurule d-50","m",6,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Gofrēta caurule d-32","m",90,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"Sistēmas pārbaude, regulēšana","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Palīgmateriāli","k-ts","1",null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"11","index":12,"n_rows":163,"n_cols":17,"rows_kept":163,"cut":false,"hidden":false,"merged":[[160,0,160,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[38,2,38,10],[49,2,49,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[15,2,15,10],[26,2,26,10],[125,2,125,10],[145,2,145,10],[157,2,157,10],[60,2,60,10],[71,2,71,10],[82,2,82,10],[93,2,93,10],[106,2,106,10],[119,2,119,10]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 11"]
["Teritorijas labiekārtošanas darbi",{"$nulls":15},"Teritorijas labiekārtošanas darbi"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"1. \"Riķu\" žogs - h=1,15m, posma garums~4m, Stabi no ozola  koka ar d~22-32cm, l=1,65m, ar trīs caurumiem - žoga kāršu ielikšanai, stabu gali aptēšami ar cirvi, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi . Žoga kopgarums - 42m"]
[2,null,"1.1. Stabu vietu izurbšana d=40, h=60cm","vietas",12]
[3,null,"1.2. Ozolkoka staba sagatavošana, uzstādīšana d=22-32cm, gals darvots","vietas",12]
[4,null,"Darba algas","c/h",0.8]
[5,null,"Stabs d=22-32cm,h=1,65","gb.",1]
[6,null,"Priežu darva","kg",0.15]
[7,null,"Rupja grants, oļi","t",0.07]
[8,null,"1.3. Žoga kāršu ielikšana statos, trīs rindās; egļu zaru locījuma izveidošana žogam","m",42]
[9,null,"Darba algas","c/h",1.1]
[10,null,"Žoga kārtis~10cm","m",3.3]
[11,null,"Egļu zari","m²",1.2]
[12,null,"2. \"Zedeņu\" žogs - h=1,15m, posma garums~4m, Stabi no ozola  koka ar d~22-32cm, l=1,65m, ar diviem caurumiem žoga kāršu ievietošanai, stabu gali aptēšami ar cirvi, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi. Zoga kopgarums - 82m"]
[13,null,"2.1. Stabu vietu izurbšana d=40, h=60cm","vietas",22]
[14,null,"2.2. Koka staba sagatavošana, uzstādīšana d=22-32cm","vietas",22]
[15,null,"Darba algas","c/h",0.8]
[16,null,"Stabs d=22-32cm,h=1,65","gb.",1]
[17,null,"Priežu darva","kg",0.15]
[18,null,"Rupja grants, oļi","t",0.07]
[19,null,"2.3. Žoga kāršu ielikšana statos, divās rindās, nostiprinot ar koka tapām; žoga latu pienaglošana s=120-150mm","m",82]
[20,null,"Darba algas","c/h",1.25]
[21,null,"Žoga kārtis~10cm","m",2.2]
[22,null,"Žoga latas","m³",0.02]
[23,null,"Naglas","kg",0.065]
[24,null,"3. \"Sklandu\" žogs (1) - h=1,15m, posma garums~4m, Stabi no egles koka ar d~10-12cm, stabu gali aptēšami ar cirvi, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi.Trīs kārtis. Žoga kopgarums - 80,4m"]
[25,null,"3.1. Stabu vietu izurbšana d=40, h=60cm","vietas",22]
[26,null,"3.2. Koka stabu uzstādīšana d=2x12cm","vietas",22]
[27,null,"Darba algas","c/h",0.6]
[28,null,"Stabi  d=12cm,h=1,65","gb.",2]
[29,null,"Priežu darva","kg",0.15]
[30,null,"Rupja grants, oļi","t",0.07]
[31,null,"3.3. Žoga kāršu ielikšana statos, nostiprinot ar paegļu vicām","m",80.2]
[32,null,"Darba algas","c/h",0.4]
[33,null,"Žoga kārtis~10cm","m",3.3]
[34,null,"Paegļu vicas","gb.",1.5]
[35,null,"4. \"Sklandu\" žogs (2) - h=1,15m, posma garums~4m, Stabi no mizota ozolkoka koka ar d~22-32cm, l=1,65m, stabu gali aptēšami ar cirvi,trīs caurumi kāršu ielikšanai, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi.Žoga kārtis trīs rindās. Žoga kopgarums - 47m"]
[36,null,"4.1. Stabu vietu izurbšana d=40, h=60cm","vietas",13]
[37,null,"4.2. Ozolkoka stabu sagatavošana, uzstādīšana 22-32cm","vietas",13]
[38,null,"Darba algas","c/h",0.6]
[39,null,"Stabs d=22-32cm,h=1,65","gb.",1]
[40,null,"Priežu darva","kg",0.15]
[41,null,"Rupja grants, oļi","t",0.07]
[42,null,"4.3. Žoga kāršu ielikšana statos, trīs rindās, nostiprinot ar paegļu vicām","m",47]
[43,null,"Darba algas","c/h",0.4]
[44,null,"Žoga kārtis~10cm","m",3.3]
[45,null,"Paegļu vicas","gb.",1.5]
[46,null,"5. \"Kāršu\" žogs (1) - h=1,15m, posma garums~4m, Stabi no ozola  koka ar d~22-32cm, l=1,65m, ar diviem caurumiem - žoga kāršu ielikšanai, stabu gali aptēšami ar cirvi, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi . Žoga kopgarums - 83m"]
[47,null,"5.1. Stabu vietu izurbšana d=40, h=60cm","vietas",22]
[48,null,"5.2. Ozolkoka staba sagatavošana, uzstādīšana d=22-32cm, gals darvots","vietas",22]
[49,null,"Darba algas","c/h",0.8]
[50,null,"Stabs d=22-32cm,h=1,65","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[51,null,"Priežu darva","kg",0.15,null,null,0,null,null,0,0,0,0,0,0]
[52,null,"Rupja grants, oļi","t",0.07,null,null,0,null,null,0,0,0,0,0,0]
[53,null,"5.3. Žoga kāršu ielikšana statos, trīs rindās","m",83,null,null,0,null,null,0,0,0,0,0,0]
[54,null,"Darba algas","c/h",0.4,null,null,0,null,null,0,0,0,0,0,0]
[55,null,"Žoga kārtis~10cm","m",2.2,null,null,0,null,null,0,0,0,0,0,0]
[56,null,"Egļu zari","m²",1.2,null,null,0,null,null,0,0,0,0,0,0]
[57,null,"6. \"Kāršu\" žogs (2) - h=1,15m, posma garums~4m, Stabi no ozola  koka ar d~22-32cm, l=1,65m, ar četriem caurumiem - žoga kāršu ielikšanai, stabu gali aptēšami ar cirvi, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi . Žoga kopgarums - 83m",{"$nulls":8},0,0,0,0,0]
[58,null,"6.1. Stabu vietu izurbšana d=40, h=60cm","vietas",18,null,null,0,null,null,0,0,0,0,0,0]
[59,null,"6.2. Ozolkoka staba sagatavošana, uzstādīšana d=22-32cm, gals darvots","vietas",18,null,null,0,null,null,0,0,0,0,0,0]
[60,null,"Darba algas","c/h",0.8,null,null,0,null,null,0,0,0,0,0,0]
[61,null,"Stabs d=22-32cm,h=1,65","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[62,null,"Priežu darva","kg",0.15,null,null,0,null,null,0,0,0,0,0,0]
[63,null,"Rupja grants, oļi","t",0.07,null,null,0,null,null,0,0,0,0,0,0]
[64,null,"6.3. Žoga kāršu ielikšana statos, četrās rindās","m",66,null,null,0,null,null,0,0,0,0,0,0]
[65,null,"Darba algas","c/h",0.6,null,null,0,null,null,0,0,0,0,0,0]
[66,null,"Žoga kārtis~10cm","m",4.4,null,null,0,null,null,0,0,0,0,0,0]
[67,null,"Egļu zari","m²",1.2,null,null,0,null,null,0,0,0,0,0,0]
[68,null,"7. \"Kāršu\" žogs (3) - h=1,15m, posma garums~4m, Stabi no ozola  koka ar d~22-32cm, l=1,65m, ar trim caurumiem - žoga kāršu ielikšanai, stabu gali aptēšami ar cirvi, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi . Žoga kopgarums - 124,4m",{"$nulls":8},0,0,0,0,0]
[69,null,"7.1. Stabu vietu izurbšana d=40, h=60cm","vietas",33,null,null,0,null,null,0,0,0,0,0,0]
[70,null,"7.2. Ozolkoka staba sagatavošana, uzstādīšana d=22-32cm, gals darvots","vietas",33,null,null,0,null,null,0,0,0,0,0,0]
[71,null,"Darba algas","c/h",0.8]
[72,null,"Stabs d=22-32cm,h=1,65","gb.",1]
[73,null,"Priežu darva","kg",0.15]
[74,null,"Rupja grants, oļi","t",0.07]
[75,null,"7.3. Žoga kāršu ielikšana statos, trīs rindās","m",124.4]
[76,null,"Darba algas","c/h",0.6]
[77,null,"Žoga kārtis~10cm","m",3.3]
[78,null,"Egļu zari","m²",1.2]
[79,null,"8. Vārti B=3,5m, atceļami. Stabi no mizota ozola  koka ar d~22-32cm, stabu gali aptēšami ar cirvi, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi"]
[80,null,"8.1. Stabu vietu izurbšana d=40, h=60cm","vietas",2]
[81,null,"8.2. Koka staba uzstādīšana d=22-32cm, gals darvots","vietas",2]
[82,null,"Darba algas","c/h",0.8]
[83,null,"Stabs d=25cm,h=1,65","gb.",1]
[84,null,"Priežu darva","kg",0.15]
[85,null,"Rupja grants, oļi","t",0.07]
[86,null,"8.3. Atceļamu vērtņu uzstādīšana B=3,5m; H=1,15m","kpl.",1]
[87,null,"Darba algas","c/h",6]
[88,null,"Žoga kārtis~10cm","m",11.6]
[89,null,"Žoga latas 5x5cm","m³",0.055]
[90,null,"Naglas","kg",0.24]
[91,null,"Egļu sīkzari","gb.",6]
[92,null,"9. Vārtiņi  B=1,0m, atceļami. Stabi no ozola vai sveķaina priežu koka ar d~25cm, stabu gali aptēšami ar cirvi, zemē ierokamais staba gals - darvots, staba iebūve zemē ~0,5m, ap stabu blietēta rupja garnts, oļi"]
[93,null,"9.1. Stabu vietu izurbšana d=40, h=60cm","vietas",2]
[94,null,"9.2. Koka staba uzstādīšana d=25cm, gals darvots","vietas",2]
[95,null,"Darba algas","c/h",0.8]
[96,null,"Stabs d=25cm,h=1,65","gb.",1]
[97,null,"Priežu darva","kg",0.15]
[98,null,"Rupja grants, oļi","t",0.07]
[99,null,"9.3. Atceļamas vērtnes uzstādīšana B=1,0m; H=1,15m","kpl.",1,null,null,0,null,null,0,0,0,0,0,0]
[100,null,"Darba algas","c/h",2,null,null,0,null,null,0,0,0,0,0,0]
[101,null,"Žoga kārtis~10cm","m",3.8,null,null,0,null,null,0,0,0,0,0,0]
[102,null,"Žoga latas 5x5cm","m³",0.002]
[103,null,"Naglas","kg",0.08]
[104,null,"Egļu sīkzari","gb.",4]
[105,null,"10.  Koka tiltiņa izbūve no mizotiem ozola apaļkokiem. Klāju nesošie koki d=15-20cm. Klāja un margu koki d=~10cm. Koka elementi, kas saskaras ar pamatni - darvoti. Tiltiņiš balstās uz lieliem laukakmeņiem."]
[106,null,"10.1. Tiltiņa izbūve (1,37m³ - apaļkoku), uzstādīšana","kpl.",1]
[107,null,"Darba algas","c/h",44]
[108,null,"Apaļkoki","m³",1.45]
[109,null,"Priežu darva","kg",4]
[110,null,"Laukakmeņi","t",0.46]
[111,null,"11. Akas virszemes daļas izbūve (koka guļbaļķu akas \"galva\" ar vāku. Koka rullis ar ķēdi un tērauda rokturi. Koka šindeļu jumtiņš virs grodiem."]
[112,null,"11.1. Akas \"galvas\" guļbaļķu konstrukcijas izbūve, viņčas statu un jumtiņa spāru uzstādīšana","m³",1.66]
[113,null,"Darba algas","c/h",44]
[114,null,"Kokmateriāli","m³",1.05]
[115,null,"Celtniecības naglas","kg",6]
[116,null,"11.2. Vinčas ruļļa sagatavošana, uzstādīšana","kpl.",1]
[117,null,"Darba algas","c/h",9.5]
[118,null,"Ozola apaļkoka vinča d=30cm","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[119,null,"Apaļdzelzs ass/rokturis d=25mm","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[120,null,"Ķēde d=5mm,l=5m","kpl.",1,null,null,0,null,null,0,0,0,0,0,0]
[121,null,"Spainis metāla 10l","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[122,null,"11.3. Latojums virs spārēm no egles koka kārtīm d=~50mm,s=30cm","m²",4,null,null,0,null,null,0,0,0,0,0,0]
[123,null,"Darba algas","c/h",0.23,null,null,0,null,null,0,0,0,0,0,0]
[124,null,"Egļu koka kārtis d=5cm","m³",0.008,null,null,0,null,null,0,0,0,0,0,0]
[125,null,"Celtniecības naglas","kg",0.083,null,null,0,null,null,0,0,0,0,0,0]
[126,null,"11.4. Egles koka šindeļu segums trīs kārtās ar impregnētām skaidām virs latām","m²",4,null,null,0,null,null,0,0,0,0,0,0]
[127,null,"Darba algas","c/h",0.77,null,null,0,null,null,0,0,0,0,0,0]
[128,null,"Egles koka šindeļi","m²",1.03,null,null,0,null,null,0,0,0,0,0,0]
[129,null,"Šindeļu naglas","kg",0.2,null,null,0,null,null,0,0,0,0,0,0]
[130,null,"Dēļi","m3",0.001,null,null,0,null,null,0,0,0,0,0,0]
[131,null,"12. Egļu dzīvžoga atjaunošanas darbi (veco izcērt, sagatavo augsni, jauno iestāda) gar zedeņu žogu",{"$nulls":8},0,0,0,0,0]
[132,null,"12.1. Dzīvžoga izciršana, zaru, gružu savākšana, sadedzināšana","100gab.",2.49,null,null,0,null,null,0,0,0,0,0,0]
[133,null,"Darba algas","c/h",10.4,null,null,0,null,null,0,0,0,0,0,0]
[134,null,"12.2. Dzīvžoga celmu izraušana","100gab.",2.49,null,null,0,null,null,0,0,0,0,0,0]
[135,null,"Darba algas","c/h",2,null,null,0,null,null,0,0,0,0,0,0]
[136,null,"12.3. Zemes nodauzīšana no celma ar celmotāja-savācēja traktoru","100gab.",2.49,null,null,0,null,null,0,0,0,0,0,0]
[137,null,"12.4. Izrok vienrindas dzīvžoga standarta stādījumu ar ekskavatoru, tranšeja 0,5x0,5m, dziļumā līdz 1m, pieved auglīgo augsni līdz 25%, sagatavo bedri stādīšanai","m",68,null,null,0,null,null,0,0,0,0,0,0]
[138,null,"Darba algas","c/h",1.84,null,null,0,null,null,0,0,0,0,0,0]
[139,null,"Melnzeme","m³",0.1,null,null,0,null,null,0,0,0,0,0,0]
[140,null,"12.5. Atrok vienrindas dzīvžoga krūmu (3gb.) stādījuma vietu, iestāda eglītes stādus (50cm), aizber un blietē bedrītes, aplaista","m",68,null,null,0,null,null,0,0,0,0,0,0]
[141,null,"Darba algas","c/h",0.6,null,null,0,null,null,0,0,0,0,0,0]
[142,null,"Eglītes","1000 gab.",0.004,null,null,0,null,null,0,0,0,0,0,0]
[143,null,"13. Koku vainagu veidošana"]
[144,null,"13.1. Koku vainaga apzāģēšana","vien.",16]
[145,null,"Darba algas","c/h",1.5,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"12","index":13,"n_rows":48,"n_cols":17,"rows_kept":48,"cut":false,"hidden":false,"merged":[[45,0,45,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[15,2,15,10],[19,2,19,10]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 12"]
["Ceļi un laukumi",{"$nulls":15},"Ceļi un laukumi"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"1. Demontāžas darbi."]
[2,null,"1.1. Teritorijas ap ēku attīrīšana no laika gaitā izveidotā kultūrslāņa \"uzauguma\" ar tehniku un piepalīdzot roku darbā lieko grunts masu iekraut autransportā ","m³",108]
[3,null,"Darba algas","c/h",1.75]
[4,null,"1.2. Noņemtā \"kultūrslāņa\" nodošana atkritumu izgāztuvē","t",189]
[5,null,"2. Jauna seguma izbūve ap ēku."]
[6,null,"2.1. Laukuma nospraušana dabā","100m²",2.55]
[7,null,"Darba algas","c/h",7.65]
[8,null,"2.2. Laukuma gultnes izveidošana mehanizēti","1000m²",0.26]
[9,null,"Darba algas","c/h",26]
[10,null,"2.3. Smilts pamatojuma izbūve, blīvējot ~15cm","m³",39.1]
[11,null,"Darba algas","c/h",0.43]
[12,null,"Smilts","m³",1.05]
[13,null,"2.4. Šķembu segums (12-20mm) piebraucamajam ceļam b=15cm","m²",100]
[14,null,"Darba algas","c/h",0.22]
[15,null,"Šķembas","m³",0.165]
[16,null,"2.5. Dolomīta šķembu pamatnes izbūve, blīvējot ~15m","m³",23.3,null,null,0,null,null,0,0,0,0,0,0]
[17,null,"Darba algas","c/h",0.41,null,null,0,null,null,0,0,0,0,0,0]
[18,null,"Dolomīta šķembas 0-40","t",1.37,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"2.6. Akmens bruģa segums (100-150)","m²",126.6,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"Darba algas","c/h",1.6,null,null,0,null,null,0,0,0,0,0,0]
[21,null,"Akmens bruģis","m²",1.05,null,null,0,null,null,0,0,0,0,0,0]
[22,null,"Smilts","m³",0.03,null,null,0,null,null,0,0,0,0,0,0]
[23,null,"2.7. Plēsta akmens bruģa segums ","m²",26.7,null,null,0,null,null,0,0,0,0,0,0]
[24,null,"Darba algas","c/h",1.6,null,null,0,null,null,0,0,0,0,0,0]
[25,null,"Plēsts akmens bruģis","m²",1.05,null,null,0,null,null,0,0,0,0,0,0]
[26,null,"Smilts","m³",0.03,null,null,0,null,null,0,0,0,0,0,0]
[27,null,"2.8. Augsnes slāņa atjaunošana un zālāju iesēšana ap bruģa malām b~15cm","100m²",5,null,null,0,null,null,0,0,0,0,0,0]
[28,null,"Darba algas","c/h",34,null,null,0,null,null,0,0,0,0,0,0]
[29,null,"Melnzeme","m³",15.75,null,null,0,null,null,0,0,0,0,0,0]
[30,null,"Zālāju sēklas","kg",3.9,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"13","index":14,"n_rows":32,"n_cols":17,"rows_kept":32,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[29,0,29,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 13"]
["Ārējais ūdenvads",{"$nulls":15},"Ārējais ūdenvads"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Ūdensvada caurule PE Pn 10 D 32","m",30,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Ūdensvada caurule PE Pn 10 D 25","m",15,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Veidgabali,pieslēguma armatūra","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Iegremdējamais sūknis Subinox","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Sūkņa vadība","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Stiprinājumi akā","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Pretvārsts Dn 25","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Tranšejas rakšana cauruļvadu montāžai mehanizēti","m³",36.4,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Pamatojums zem caurules: smilts h=0.15m","m³",2.6,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Grunts blietēšana","m³",2.6,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"Ievada izveidošana ēkā","vieta",2,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Tranšejas aizbēršana ","m³",33,null,null,0,null,null,0,0,0,0,0,0]
[13,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[14,null,"Digitālā uzmērīšana","m",26,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"14","index":15,"n_rows":29,"n_cols":17,"rows_kept":29,"cut":false,"hidden":false,"merged":[[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15],[26,0,26,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 14"]
["Ārējā saimnieciskā kanalizācija",{"$nulls":15},"Ārējā saimnieciskā kanalizācija"]
["Būves nosaukums:",null,"Teritorijas labiekārtošanas darbi un renovācijas darbi Kubalu skolas - muzeja saimniecības ēkā , atjaunojot vēsturiskos elementus"]
["Objekta nosaukums:",null,"Kubalu skolas - muzeja saimniecības ēka ar teritoriju"]
["Objekta adrese:",null,"\"Kubalu skola\", Dundagas pagasts, Dundagas novads"]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[]
[1,null,"Caurule PE Pn 10 40x3,7","m",40,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Individuālā izgatavojuma PEH skataka D 400 ar čuguna vāku","kts",2,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Uponor sūknētava 0,5 m3","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Drenāžas sūkņa uzstādīšana, pieslēgumi.","kts",1,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Lodveida pretvārsts Dn 32-piev.","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Tranšejas rakšana cauruļvadu montāžai mehanizēti","m³",40,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Pamatojums zem caurules: smilts h=0.15m","m³",6,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Grunts blietēšana","m³",6,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Pievienošanas pie esošā tīkla  ","vieta",1,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Tranšejas aizbēršana ","m³",34,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"Digitālā uzmērīšana","aka",3,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]