{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Finansu piedavajums"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Finansu piedavajums","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[[3,0,3,6],[36,4,36,5],[37,4,37,5],[35,4,35,5]],"flags":["formulas_cached_only"]}
[null,"Dundagas novada Dundagas pagasta Dundagas ciemata ielas Nr.16"]
[null,"E. Dinsberga iela km 0,046 - 0,167 remonta"]
[]
["Finanšu piedāvājums"]
[]
["Izmaksu pozīcija","Specifik. Nr.","Darba nosaukums","Mēr- vienība","Darba daudzums","Vienības cena                 LVL","Kopējā izmaksa LVL"]
["1.","3.","Sagatavošanas darbi"]
["1.1.","3.1.","Uzmērīšana un nospraušana","km",0.125]
["1.2.","3.7.","Asfalta seguma savienojumu frēzēšana","m2",11.9]
["1.3.","3.7.","Asfalta seguma safrēzēšana","m2",696.8]
["1.4.","3.7.","Cementbetona seguma frēzēšana","m2",2.7]
["2.","4.","Zemes klātne"]
["2.1.","4.1.","Ielas  un ietves segas pamata nojaukšana, materiālu aizvedot uz atbērtni","m3",193.8]
["2.2.","4.1.","Ielas klātnes profilēšana ierakumā","m2",872]
["2.3.","4.2.","Nostiprināšana ar augu zemi 15cm biezumā","m2",70.4]
["3.","5.","Ar saistvielām nesaistītas konstruktīvas kārtas"]
["3.1.","5.2","Šķembu 0/32 pamata izbūve 20cm biezumā ielai","m2",872]
["4.","6.","Ar saistvielām saistītas konstruktīvas kārtas"]
["4.1.","6.1.","Gruntēšana","m2",57.8]
["4.2.","6.2.","Karstā asfalta apakškārtas izbūve  no  ACb-16  4cm biezumā","m2",961]
["4.3.","6.2.","Karstā asfalta virskārtas izbūve  no  AC-11  6cm biezumā","m2",1018]
["5.","7.","Caurtekas un konstrukcijas"]
["5.1.","7.1."," Gūlijas diam.560mm, augstums ~2m iebūve","kompl.",2]
["5.2.","7.1.","Novadcaurles diam.110mm iebūve no gūlijas ~1,5m dziļumā","m",25]
["5.3.","7.1. ","Virsūdeņu novadaku vāku līmeņa paaugstināšana","gab.",3]
["5.4.","7.2.","Betona apmaļu BR 100.30.15 demontāža gar ielas malu","m",94.5]
["5.5.","7.2.","Betona apmaļu BR 100.20.8 demontāža ietvei","m",67]
["5.6.","7.2. ","Virsūdeņu novadakas nojaukšana","kompl.",1]
["5.7.","7.3.","Grants/šķembu 0/32 pamata izbūve ietvei","m3",17.8]
["5.8.","7.3.","Smilts virskārtas ietves pamatam izbūve 3cm biezumā","m2",119.9]
["5.9.","7.3.","Divkrāsaina (pelēks : brūms = 1:5 6cm bieza betona bruģakmeņa ietves seguma izbūve","m2",119.9]
["5.10.","7.4.","Betona apmaļu BR 100.30.15 uz betona pamatnes uzstādīšana","m",95]
["5.11.","7.4.","Betona apmaļu BR 100.20.8 uz betona pamatnes ietvei uzstādīšana","m",77]
["5.12.","7.4.","Betona apmaļu BR 100.30.15 K ; L uz betona pamatnes ietvei uzstādīšana","m",4]
["5.13.","7.4.","Pazemināto betona apmaļu BR 100.22.15 uz betona pamatnes ietvei uzstādīšana","m",26]
[null,null,null,"A","Kopā:"]
[null,null,null,"B","PVN (21% no A):"]
[{"$nulls":4},"Pavisam kopā (A + B):"]
[]
[null,null,"Pilnvarotās personas paraksts :"]