{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":1218,"n_cols":15,"rows_kept":1218,"cut":false,"hidden":false,"merged":[[1221,1,1221,7],[1222,1,1222,3],[7,9,10,9],[7,10,10,10],[7,6,10,6],[7,7,10,7],[7,8,10,8],[1220,1,1220,7],[0,1,0,14],[4,0,4,3],[1,7,1,12],[3,0,3,1],[7,11,10,11],[7,13,10,13],[7,12,10,12],[6,0,10,0],[6,1,10,1],[6,2,10,2],[7,14,10,14],[6,10,6,14],[7,4,10,4],[7,5,10,5],[2,0,2,14],[6,3,10,3],[6,4,6,9]],"flags":["formulas_cached_only"]}
[null,"Tāme \"Mazirbes speciālās internātpamatskolas telpu vienkāršotā renovācija mācību telpu uzlabošanai\""]
[{"$nulls":7},"Identifikācijas Nr. DND-2010/13/ERAF"]
["TĀME"]
["Būves nosaukums: Mācību telpas"]
["Objekta nosaukums: Mazirbes speciālā internātpamatskola"]
["Objekta adrese: „Mazirbes speciālā internātskola”, Mazirbes ciems, Dundagas novads"]
["N.p.k.","Darbu,materiālu un citu izdevumu nosaukums","Mērvienība","Daudzums","Vienības izmaksas,tai skaitā",{"$nulls":5},"Kopējās izmaksas,tai skaitā"]
[{"$nulls":4},"Laika norma C/st","Darba samaksa likme Ls","Darba alga Ls","Materiāli Ls","Mehanismi Ls","Kopā Ls","Darbietilpība C/st","Darba alga Ls","Materiāli Ls","Mehanismi Ls","Kopā Ls"]
[]
[]
[]
[1,2,3,4,5,5,7,8,9,10,11,12,13,14,15]
[null,"MĀCĪBU TELPA NR.1"]
[1,"Dēļu grīdas klāja izjaukšana","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[2,"Dēļu grīdas gulšņu izjaukšana","m",70,{"$nulls":5},0,0,0,null,0,0]
[3,"Būvgružu savākšana","m3",2.65,{"$nulls":5},0,0,0,null,0,0]
[4,"Smilšu pamatkārtas izveidošana līdz 100 mm biezumā","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[5,"smilts","m3",4.4,{"$nulls":5},0,null,null,0,null,0]
[6,"Tvaikizolācijas plēves uzstādīšana,salaidumvietas sastiprinot ar līmlenti","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[7,"polietlēna plēve","m2",54.89,{"$nulls":5},0,null,null,0,null,0]
[8,"līmlenta","m",17,{"$nulls":5},0,null,null,0,null,0]
[9,"Cieto siltumizolācijas plātņu ieklāšana","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[10,"ekstrudētais putupolistirols 50 mm","m2",50.9,{"$nulls":5},0,null,null,0,null,0]
[11,"Betona grīdas ieklāšana","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[12,"betons B 15","m3",3.05,{"$nulls":5},0,null,null,0,null,0]
[13,"betonēšanas siets 4x150x150 mm","m2",59.88,{"$nulls":5},0,null,null,0,null,0]
[14,"distanceri","gb",100,{"$nulls":5},0,null,null,0,null,0]
[15,"Betona grīdas virsmas špaktelēšana un slīpēšana","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[16,"bodenfinish špaktele","kg",80,{"$nulls":5},0,null,null,0,null,0]
[17,"Betona grīdas virsmas gruntēšana","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[18,"grunts","l",15,{"$nulls":5},0,null,null,0,null,0]
[19,"Linoleja ieklāšana pielīmējot visā platībā","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[20,"linolejs 34 klase","m2",52.39,{"$nulls":5},0,null,null,0,null,0]
[21,"linoleja līme","kg",25,{"$nulls":5},0,null,null,0,null,0]
[22,"šuvju kausēšanas diegs","m",17.4,{"$nulls":5},0,null,null,0,null,0]
[23,"Koka grīdlīstu uzstādīšana","m",28,{"$nulls":5},0,0,0,null,0,0]
[24,"koka grīdlīste,krāsota","m",32.3,{"$nulls":5},0,null,null,0,null,0]
[25,"Griestu krāsošana","m2",49.9,{"$nulls":5},0,0,0,null,0,0]
[26,"grunts","l",6.2,{"$nulls":5},0,null,null,0,null,0]
[27,"krāsa","l",10,{"$nulls":5},0,null,null,0,null,0]
[28,"Saplaisājušas un bojātas krāsas noņemšana","m2",21,{"$nulls":5},0,0,0,null,0,0]
[29,"Sienu virsmu gruntēšana","m2",77,{"$nulls":5},0,0,0,null,0,0]
[30,"grunts","l",11,{"$nulls":5},0,null,null,0,null,0]
[31,"Sienu virsmu špaktelēšana","m2",77,{"$nulls":5},0,0,0,null,0,0]
[32,"špaktele","kg",93,{"$nulls":5},0,null,null,0,null,0]
[33,"gatavā špakteļmasa","kg",123,{"$nulls":5},0,null,null,0,null,0]
[34,"Sienu virsmu krāsošana","m2",77,{"$nulls":5},0,0,0,null,0,0]
[35,"grunts","l",7.7,{"$nulls":5},0,null,null,0,null,0]
[36,"krāsa tonēta","l",25,{"$nulls":5},0,null,null,0,null,0]
[37,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,0,0,0]
[38,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,null,null,0,null,0]
[39,"Esošo durvju špaktelēšana un slīpēšana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[40,"špakteļtepe","l",1.5,{"$nulls":5},0,null,null,0,null,0]
[41,"smilšpapīrs","m",1.1,{"$nulls":5},0,null,null,0,null,0]
[42,"Augstvērtīga krāsojuma uzklāšana durvīm","gb",1,{"$nulls":5},0,0,0,null,0,0]
[43,"krāsa kokam","l",0.6,{"$nulls":5},0,null,null,0,null,0]
[44,"Gaismas ķermeņu noņemšana","gb",8,{"$nulls":5},0,0,0,null,0,0]
[45,"Elektroinstalācijas montāža","m",42,{"$nulls":5},0,0,0,null,0,0]
[46,"kabelis","m",42,{"$nulls":5},0,null,null,0,null,0]
[47,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[48,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[49,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[50,"Gaismas ķermeņu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[51,"dienasgaismas lampas","gb",8,{"$nulls":5},0,null,null,0,null,0]
[52,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[53,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[54,"MĀCĪBU TELPA NR.2"]
[55,"Dēļu grīdas klāja izjaukšana","m2",54.7,{"$nulls":5},0,0,0,null,0,0]
[56,"Dēļu grīdas gulšņu izjaukšana","m",78,{"$nulls":5},0,0,0,null,0,0]
[57,"Būvgružu savākšana","m3",2.83,{"$nulls":5},0,0,0,null,0,0]
[58,"Smilšu pamatkārtas izveidošana līdz 100 mm biezumā","m2",54.7,{"$nulls":5},0,0,0,null,0,0]
[59,"smilts","m3",4.8,{"$nulls":5},0,null,null,0,null,0]
[60,"Tvaikizolācijas plēves uzstādīšana,salaidumvietas sastiprinot ar līmlenti","m2",54.7,{"$nulls":5},0,0,0,null,0,0]
[61,"polietlēna plēve","m2",60.17,{"$nulls":5},0,null,null,0,null,0]
[62,"līmlenta","m",19,{"$nulls":5},0,null,null,0,null,0]
[63,"Cieto siltumizolācijas plātņu ieklāšana","m2",54.7,{"$nulls":5},0,0,0,null,0,0]
[64,"ekstrudētais putupolistirols 50 mm","m2",55.79,{"$nulls":5},0,null,null,0,null,0]
[65,"Betona grīdas ieklāšana","m2",54.7,{"$nulls":5},0,0,0,null,0,0]
[66,"betons B 15","m3",3.35,{"$nulls":5},0,null,null,0,null,0]
[67,"betonēšanas siets 4x150x150 mm","m2",65.64,{"$nulls":5},0,null,null,0,null,0]
[68,"distanceri","gb",110,{"$nulls":5},0,null,null,0,null,0]
[69,"Betona grīdas virsmas špaktelēšana un slīpēšana","m2",54.7,{"$nulls":5},0,0,0,0,0,0]
[70,"bodenfinish špaktele","kg",87.5,{"$nulls":5},0,null,null,0,null,0]
[71,"Betona grīdas virsmas gruntēšana","m2",54.7,{"$nulls":5},0,0,0,null,0,0]
[72,"grunts","l",16.5,{"$nulls":5},0,null,null,0,null,0]
[73,"Linoleja ieklāšana pielīmējot visā platībā","m2",54.7,{"$nulls":5},0,0,0,null,0,0]
[74,"linolejs 34 klase","m2",55.8,{"$nulls":5},0,null,null,0,null,0]
[75,"linoleja līme","kg",27.35,{"$nulls":5},0,null,null,0,null,0]
[76,"šuvju kausēšanas diegs","m",19,{"$nulls":5},0,null,null,0,null,0]
[77,"Koka grīdlīstu uzstādīšana","m",29.2,{"$nulls":5},0,0,0,null,0,0]
[78,"koka grīdlīste,krāsota","m",32.3,{"$nulls":5},0,null,null,0,null,0]
[79,"Griestu krāsošana","m2",54.7,{"$nulls":5},0,0,0,null,0,0]
[80,"grunts","l",9,{"$nulls":5},0,null,null,0,null,0]
[81,"krāsa","l",12.5,{"$nulls":5},0,null,null,0,null,0]
[82,"Saplaisājušas un bojātas krāsas noņemšana","m2",26,{"$nulls":5},0,0,0,null,0,0]
[83,"Sienu virsmu gruntēšana","m2",82,{"$nulls":5},0,0,0,null,0,0]
[84,"grunts","l",12.3,{"$nulls":5},0,null,null,0,null,0]
[85,"Sienu virsmu špaktelēšana","m2",82,{"$nulls":5},0,0,0,null,0,0]
[86,"špaktele","kg",98.4,{"$nulls":5},0,null,null,0,null,0]
[87,"gatavā špakteļmasa","kg",131,{"$nulls":5},0,null,null,0,null,0]
[88,"Sienu virsmu krāsošana","m2",82,{"$nulls":5},0,0,0,null,0,0]
[89,"grunts","l",12.3,{"$nulls":5},0,null,null,0,null,0]
[90,"krāsa tonēta","l",27.5,{"$nulls":5},0,null,null,0,null,0]
[91,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,null,0,0]
[92,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,null,null,0,null,0]
[93,"Esošo durvju špaktelēšana un slīpēšana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[94,"špakteļtepe","l",1.6,{"$nulls":5},0,null,null,0,null,0]
[95,"smilšpapīrs","m",1,{"$nulls":5},0,null,null,0,null,0]
[96,"Augstvērtīga krāsojuma uzklāšana durvīm","gb",1,{"$nulls":5},0,0,0,null,0,0]
[97,"krāsa kokam","l",0.6,{"$nulls":5},0,null,null,0,null,0]
[98,"Gaismas ķermeņu noņemšana","gb",8,{"$nulls":5},0,0,0,null,0,0]
[99,"Elektroinstalācijas montāža","m",45.3,{"$nulls":5},0,0,0,null,0,0]
[100,"kabelis","m",45.3,{"$nulls":5},0,null,null,0,null,0]
[101,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[102,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[103,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[104,"Gaismas ķermeņu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[105,"dienasgaismas lampas","gb",8,{"$nulls":5},0,null,null,0,null,0]
[106,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[107,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[108,"MĀCĪBU TELPA NR.3"]
[109,"Dēļu grīdas klāja izjaukšana","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[110,"Dēļu grīdas gulšņu izjaukšana","m",50.5,{"$nulls":5},0,0,0,null,0,0]
[111,"Būvgružu savākšana","m3",1.83,{"$nulls":5},0,0,0,null,0,0]
[112,"Smilšu pamatkārtas izveidošana līdz 100 mm biezumā","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[113,"smilts","m3",3.1,{"$nulls":5},0,null,null,0,null,0]
[114,"Tvaikizolācijas plēves uzstādīšana,salaidumvietas sastiprinot ar līmlenti","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[115,"polietlēna plēve","m2",38.72,{"$nulls":5},0,null,null,0,null,0]
[116,"līmlenta","m",13,{"$nulls":5},0,null,null,0,null,0]
[117,"Cieto siltumizolācijas plātņu ieklāšana","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[118,"ekstrudētais putupolistirols 50 mm","m2",35.9,{"$nulls":5},0,null,null,0,null,0]
[119,"Betona grīdas ieklāšana","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[120,"betons B 15","m3",2.15,{"$nulls":5},0,null,null,0,null,0]
[121,"betonēšanas siets 4x150x150 mm","m2",42.24,{"$nulls":5},0,null,null,0,null,0]
[122,"distanceri","gb",70,{"$nulls":5},0,null,null,0,null,0]
[123,"Betona grīdas virsmas špaktelēšana un slīpēšana","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[124,"bodenfinish špaktele","kg",56.32,{"$nulls":5},0,null,null,0,null,0]
[125,"Betona grīdas virsmas gruntēšana","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[126,"grunts","l",10.6,{"$nulls":5},0,null,null,0,null,0]
[127,"Linoleja ieklāšana pielīmējot visā platībā","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[128,"linolejs 34 klase","m2",36.96,{"$nulls":5},0,null,null,0,null,0]
[129,"linoleja līme","kg",17.6,{"$nulls":5},0,null,null,0,null,0]
[130,"šuvju kausēšanas diegs","m",13,{"$nulls":5},0,null,null,0,null,0]
[131,"Koka grīdlīstu uzstādīšana","m",22.8,{"$nulls":5},0,0,0,null,0,0]
[132,"koka grīdlīste,krāsota","m",25.1,{"$nulls":5},0,null,null,0,null,0]
[133,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[134,"UD profils","m",24,{"$nulls":5},0,null,null,0,null,0]
[135,"CD profils","m",135,{"$nulls":5},0,null,null,0,null,0]
[136,"U veida skava","gb",30,{"$nulls":5},0,null,null,0,null,0]
[137,"CD profilu savienotājs","gb",15,{"$nulls":5},0,null,null,0,null,0]
[138,"CD profilu šķērssavienotājs","gb",35,{"$nulls":5},0,null,null,0,null,0]
[139,"ģipškartons","m2",37,{"$nulls":5},0,null,null,0,null,0]
[140,"apšuvuma skrūves","gb",530,{"$nulls":5},0,null,null,0,null,0]
[141,"dībeļnaglas","gb",60,{"$nulls":5},0,null,null,0,null,0]
[142,"Gipškartona šuvju špaktelēšana","m",42,{"$nulls":5},0,0,0,null,0,0]
[143,"grunts","l",0.5,{"$nulls":5},0,null,null,0,null,0]
[144,"špaktele","kg",10.5,{"$nulls":5},0,null,null,0,null,0]
[145,"Griestu gruntēšana","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[146,"grunts","l",6,{"$nulls":5},0,null,null,0,null,0]
[147,"Griestu krāsošana","m2",35.2,{"$nulls":5},0,0,0,null,0,0]
[148,"krāsa","l",11.8,{"$nulls":5},0,null,null,0,null,0]
[149,"Saplaisājušas un bojātas krāsas noņemšana","m2",17,{"$nulls":5},0,0,0,null,0,0]
[150,"Sienu virsmu gruntēšana","m2",66,{"$nulls":5},0,0,0,null,0,0]
[151,"grunts","l",9.9,{"$nulls":5},0,null,null,0,null,0]
[152,"Sienu virsmu špaktelēšana","m2",66,{"$nulls":5},0,0,0,null,0,0]
[153,"špaktele","kg",80,{"$nulls":5},0,null,null,0,null,0]
[154,"gatavā špakteļmasa","kg",105,{"$nulls":5},0,null,null,0,null,0]
[155,"Sienu virsmu krāsošana","m2",66,{"$nulls":5},0,0,0,null,0,0]
[156,"grunts","l",9.9,{"$nulls":5},0,null,null,0,null,0]
[157,"krāsa tonēta","l",22,{"$nulls":5},0,null,null,0,null,0]
[158,"Radiatoru krāsošana","gb",2,{"$nulls":5},0,0,0,null,0,0]
[159,"krāsa radiatoriem","l",1.8,{"$nulls":5},0,null,null,0,null,0]
[160,"Esošo durvju špaktelēšana un slīpēšana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[161,"špakteļtepe","l",1.6,{"$nulls":5},0,null,null,0,null,0]
[162,"smilšpapīrs","m",1,{"$nulls":5},0,null,null,0,null,0]
[163,"Augstvērtīga krāsojuma uzklāšana durvīm","gb",1,{"$nulls":5},0,0,0,null,0,0]
[164,"krāsa kokam","l",0.6,{"$nulls":5},0,null,null,0,null,0]
[165,"Gaismas ķermeņu noņemšana","gb",6,{"$nulls":5},0,0,0,null,0,0]
[166,"Elektroinstalācijas montāža","m",33,{"$nulls":5},0,0,0,null,0,0]
[167,"kabelis","m",33,{"$nulls":5},0,null,null,0,null,0]
[168,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[169,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[170,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[171,"Gaismas ķermeņu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[172,"dienasgaismas lampas","gb",6,{"$nulls":5},0,null,null,0,null,0]
[173,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[174,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[175,"ĒDAMZĀLE TELPA NR.4"]
[176,"Esošās grīdas sagatavošana","m2",76.8,{"$nulls":5},0,0,0,null,0,0]
[177,"grunts","l",23.04,{"$nulls":5},0,null,null,0,null,0]
[178,"Izlīdzinošā grīdas sastāva iestrāde","m2",76.8,{"$nulls":5},0,0,0,null,0,0]
[179,"pašizlīdzinošais maisījums","kg",368.64,{"$nulls":5},0,null,null,0,null,0]
[180,"Betona grīdas virsmas gruntēšana","m2",76.8,{"$nulls":5},0,0,0,null,0,0]
[181,"grunts","l",23.04,{"$nulls":5},0,null,null,0,null,0]
[182,"Linoleja ieklāšana pielīmējot visā platībā","m2",76.8,{"$nulls":5},0,0,0,null,0,0]
[183,"linolejs 34 klase","m2",80.64,{"$nulls":5},0,null,null,0,null,0]
[184,"linoleja līme","kg",38.4,{"$nulls":5},0,null,null,0,null,0]
[185,"šuvju kausēšanas diegs","m",33.7,{"$nulls":5},0,null,null,0,null,0]
[186,"Koka grīdlīstu uzstādīšana","m",37.4,{"$nulls":5},0,0,0,null,0,0]
[187,"koka grīdlīste,krāsota","m",39.27,{"$nulls":5},0,null,null,0,null,0]
[188,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",76.8,{"$nulls":5},0,0,0,null,0,0]
[189,"UD profils","m",38,{"$nulls":5},0,null,null,0,null,0]
[190,"CD profils","m",212,{"$nulls":5},0,null,null,0,null,0]
[191,"U veida skava","gb",56,{"$nulls":5},0,null,null,0,null,0]
[192,"CD profilu savienotājs","gb",22,{"$nulls":5},0,null,null,0,null,0]
[193,"CD profilu šķērssavienotājs","gb",40,{"$nulls":5},0,null,null,0,null,0]
[194,"ģipškartons","m2",78.34,{"$nulls":5},0,null,null,0,null,0]
[195,"apšuvuma skrūves","gb",1160,{"$nulls":5},0,null,null,0,null,0]
[196,"dībeļnaglas","gb",112,{"$nulls":5},0,null,null,0,null,0]
[197,"Gipškartona šuvju špaktelēšana","m",100.4,{"$nulls":5},0,0,0,null,0,0]
[198,"grunts","l",1.2,{"$nulls":5},0,null,null,0,null,0]
[199,"špaktele","kg",25,{"$nulls":5},0,null,null,0,null,0]
[200,"Griestu gruntēšana","m2",76.8,{"$nulls":5},0,0,0,null,0,0]
[201,"grunts","l",12.8,{"$nulls":5},0,null,null,0,null,0]
[202,"Griestu krāsošana","m2",76.8,{"$nulls":5},0,0,0,null,0,0]
[203,"krāsa","l",26,{"$nulls":5},0,null,null,0,null,0]
[204,"Saplaisājušas un bojātas krāsas noņemšana","m2",26,{"$nulls":5},0,0,0,null,0,0]
[205,"Sienu virsmu gruntēšana","m2",99.11,{"$nulls":5},0,0,0,null,0,0]
[206,"grunts","l",14.87,{"$nulls":5},0,null,null,0,null,0]
[207,"Sienu virsmu špaktelēšana","m2",99.11,{"$nulls":5},0,0,0,null,0,0]
[208,"špaktele","kg",119,{"$nulls":5},0,null,null,0,null,0]
[209,"gatavā špakteļmasa","kg",158,{"$nulls":5},0,null,null,0,null,0]
[210,"Sienu virsmu krāsošana","m2",99.11,{"$nulls":5},0,0,0,null,0,0]
[211,"grunts","l",14.87,{"$nulls":5},0,null,null,0,null,0]
[212,"krāsa tonēta","l",33,{"$nulls":5},0,null,null,0,null,0]
[213,"Radiatoru krāsošana","gb",4,{"$nulls":5},0,0,0,null,0,0]
[214,"krāsa radiatoriem","l",3.6,{"$nulls":5},0,null,null,0,null,0]
[215,"Esošo durvju špaktelēšana un slīpēšana","gb",2,{"$nulls":5},0,0,0,null,0,0]
[216,"špakteļtepe","l",3,{"$nulls":5},0,null,null,0,null,0]
[217,"smilšpapīrs","m",2,{"$nulls":5},0,null,null,0,null,0]
[218,"Augstvērtīga krāsojuma uzklāšana durvīm","gb",2,{"$nulls":5},0,0,0,null,0,0]
[219,"krāsa kokam","l",1.2,{"$nulls":5},0,null,null,0,null,0]
[220,"Gaismas ķermeņu noņemšana","gb",12,{"$nulls":5},0,0,0,null,0,0]
[221,"Elektroinstalācijas montāža","m",74.4,{"$nulls":5},0,0,0,null,0,0]
[222,"kabelis","m",74.4,{"$nulls":5},0,null,null,0,null,0]
[223,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[224,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[225,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[226,"Gaismas ķermeņu montāža","gb",12,{"$nulls":5},0,0,0,null,0,0]
[227,"dienasgaismas lampas","gb",12,{"$nulls":5},0,null,null,0,null,0]
[228,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[229,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[230,"GUĻAMTELPA TELPA NR.5"]
[231,"Dēļu grīdas klāja izjaukšana","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[232,"Dēļu grīdas gulšņu izjaukšana","m",71,{"$nulls":5},0,0,0,null,0,0]
[233,"Starpsienas nojaukšana","m2",14.5,{"$nulls":5},0,0,0,null,0,0]
[234,"Būvgružu savākšana","m3",4.77,{"$nulls":5},0,0,0,null,0,0]
[235,"Smilšu pamatkārtas izveidošana līdz 100 mm biezumā","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[236,"smilts","m3",4,{"$nulls":5},0,null,null,0,null,0]
[237,"Tvaikizolācijas plēves uzstādīšana,salaidumvietas sastiprinot ar līmlenti","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[238,"polietlēna plēve","m2",54.56,{"$nulls":5},0,null,null,0,null,0]
[239,"līmlenta","m",9.5,{"$nulls":5},0,null,null,0,null,0]
[240,"Cieto siltumizolācijas plātņu ieklāšana","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[241,"ekstrudētais putupolistirols 50 mm","m2",52.08,{"$nulls":5},0,null,null,0,null,0]
[242,"Betona grīdas ieklāšana","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[243,"betons B 15","m3",3.03,{"$nulls":5},0,null,null,0,null,0]
[244,"betonēšanas siets 4x150x150 mm","m2",59.52,{"$nulls":5},0,null,null,0,null,0]
[245,"distanceri","gb",100,{"$nulls":5},0,null,null,0,null,0]
[246,"Betona grīdas virsmas špaktelēšana un slīpēšana","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[247,"bodenfinish špaktele","kg",79.4,{"$nulls":5},0,null,null,0,null,0]
[248,"Betona grīdas virsmas gruntēšana","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[249,"grunts","l",14.88,{"$nulls":5},0,null,null,0,null,0]
[250,"Metāla profilu karkasa starpsienu izbūve,apšujot no abām pusēm ar ģipškartona loksnēm","m2",14.5,{"$nulls":5},0,0,0,null,0,0]
[251,"starpsienu profils UW 100 mm","m",18,{"$nulls":5},0,null,null,0,null,0]
[252,"starpsienu profils CW 100 mm","m",36.25,{"$nulls":5},0,null,null,0,null,0]
[253,"skaņas izolācija 100 mm","m2",14.5,{"$nulls":5},0,null,null,0,null,0]
[254,"ģipškartons","m2",58,{"$nulls":5},0,null,null,0,null,0]
[255,"apšuvuma skrūves","gb",700,{"$nulls":5},0,null,null,0,null,0]
[256,"amortizējošā blīvlenta","m",12,{"$nulls":5},0,null,null,0,null,0]
[257,"Linoleja ieklāšana pielīmējot visā platībā","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[258,"linolejs 34 klase","m2",52.08,{"$nulls":5},0,null,null,0,null,0]
[259,"linoleja līme","kg",24.8,{"$nulls":5},0,null,null,0,null,0]
[260,"šuvju kausēšanas diegs","m",24,{"$nulls":5},0,null,null,0,null,0]
[261,"Koka grīdlīstu uzstādīšana","m",41,{"$nulls":5},0,0,0,null,0,0]
[262,"koka grīdlīste,krāsota","m",43.05,{"$nulls":5},0,null,null,0,null,0]
[263,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[264,"UD profils","m",41,{"$nulls":5},0,null,null,0,null,0]
[265,"CD profils","m",205,{"$nulls":5},0,null,null,0,null,0]
[266,"U veida skava","gb",48,{"$nulls":5},0,null,null,0,null,0]
[267,"CD profilu savienotājs","gb",20,{"$nulls":5},0,null,null,0,null,0]
[268,"CD profilu šķērssavienotājs","gb",36,{"$nulls":5},0,null,null,0,null,0]
[269,"ģipškartons","m2",52.08,{"$nulls":5},0,null,null,0,null,0]
[270,"apšuvuma skrūves","gb",645,{"$nulls":5},0,null,null,0,null,0]
[271,"dībeļnaglas","gb",110,{"$nulls":5},0,null,null,0,null,0]
[272,"Gipškartona šuvju špaktelēšana","m",63.6,{"$nulls":5},0,0,0,null,0,0]
[273,"grunts","l",0.6,{"$nulls":5},0,null,null,0,null,0]
[274,"špaktele","kg",16,{"$nulls":5},0,null,null,0,null,0]
[275,"Griestu gruntēšana","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[276,"grunts","l",8.3,{"$nulls":5},0,null,null,0,null,0]
[277,"Griestu krāsošana","m2",49.6,{"$nulls":5},0,0,0,null,0,0]
[278,"krāsa","l",16.55,{"$nulls":5},0,null,null,0,null,0]
[279,"Saplaisājušas un bojātas krāsas noņemšana","m2",13,{"$nulls":5},0,0,0,null,0,0]
[280,"Sienu virsmu gruntēšana","m2",82,{"$nulls":5},0,0,0,null,0,0]
[281,"grunts","l",12.3,{"$nulls":5},0,null,null,0,null,0]
[282,"Sienu virsmu špaktelēšana","m2",82,{"$nulls":5},0,0,0,null,0,0]
[283,"špaktele","kg",98.5,{"$nulls":5},0,null,null,0,null,0]
[284,"gatavā špakteļmasa","kg",131.2,{"$nulls":5},0,null,null,0,null,0]
[285,"Sienu virsmu krāsošana","m2",82,{"$nulls":5},0,0,0,null,0,0]
[286,"grunts","l",12.3,{"$nulls":5},0,null,null,0,null,0]
[287,"krāsa tonēta","l",27,{"$nulls":5},0,null,null,0,null,0]
[288,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,null,0,0]
[289,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,{"$nulls":4},0]
[290,"Gaismas ķermeņu noņemšana","gb",8,{"$nulls":5},0,0,0,null,0,0]
[291,"Elektroinstalācijas montāža","m",56,{"$nulls":5},0,0,0,null,0,0]
[292,"kabelis","m",56,{"$nulls":5},0,null,null,0,null,0]
[293,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[294,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[295,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[296,"Gaismas ķermeņu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[297,"dienasgaismas lampas","gb",8,{"$nulls":5},0,null,null,0,null,0]
[298,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[299,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[300,"GUĻAMTELPA TELPA NR.6"]
[301,"Dēļu grīdas klāja izjaukšana","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[302,"Dēļu grīdas gulšņu izjaukšana","m",46.35,{"$nulls":5},0,0,0,null,0,0]
[303,"Būvgružu savākšana","m3",1.7,{"$nulls":5},0,0,0,null,0,0]
[304,"Grīdas gulšņu uzstādīšana","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[305,"kokmateriāls","m3",0.45,{"$nulls":5},0,null,null,0,null,0]
[306,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",27.33,{"$nulls":5},0,0,0,null,0,0]
[307,"antiseptiķis","l",11,{"$nulls":5},0,null,null,0,null,0]
[308,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[309,"keramzīts","m3",3.32,{"$nulls":5},0,null,null,0,null,0]
[310,"Grīdas klāja-melnās grīdas ierīkošana ","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[311,"apzāģēti dēļi","m3",0.28,{"$nulls":5},0,null,null,0,null,0]
[312,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[313,"spundēta plāksne 22 mm","m2",35.86,{"$nulls":5},0,null,null,0,null,0]
[314,"skrūves","gb",450,{"$nulls":5},0,null,null,0,null,0]
[315,"Grīdas virsmas gruntēšana","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[316,"grunts","l",9.78,{"$nulls":5},0,null,null,0,null,0]
[317,"Linoleja ieklāšana pielīmējot visā platībā","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[318,"linolejs 34 klase","m2",34.23,{"$nulls":5},0,null,null,0,null,0]
[319,"linoleja līme","kg",16.3,{"$nulls":5},0,null,null,0,null,0]
[320,"šuvju kausēšanas diegs","m",15,{"$nulls":5},0,null,null,0,null,0]
[321,"Koka grīdlīstu uzstādīšana","m",23,{"$nulls":5},0,0,0,null,0,0]
[322,"koka grīdlīste,krāsota","m",25.3,{"$nulls":5},0,null,null,0,null,0]
[323,"Gipškartona šuvju špaktelēšana","m",41.8,{"$nulls":5},0,0,0,null,0,0]
[324,"grunts","l",0.4,{"$nulls":5},0,null,null,0,null,0]
[325,"špaktele","kg",10.25,{"$nulls":5},0,null,null,0,null,0]
[326,"sietlenta","m",43,{"$nulls":5},0,null,null,0,null,0]
[327,"Griestu gruntēšana","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[328,"grunts","l",5.53,{"$nulls":5},0,null,null,0,null,0]
[329,"Griestu krāsošana","m2",32.6,{"$nulls":5},0,0,0,null,0,0]
[330,"krāsa","l",11,{"$nulls":5},0,null,null,0,null,0]
[331,"Saplaisājušas un bojātas krāsas noņemšana","m2",14,{"$nulls":5},0,0,0,null,0,0]
[332,"Sienu virsmu gruntēšana","m2",49,{"$nulls":5},0,0,0,null,0,0]
[333,"grunts","l",7.35,{"$nulls":5},0,null,null,0,null,0]
[334,"Sienu virsmu špaktelēšana","m2",49,{"$nulls":5},0,0,0,null,0,0]
[335,"špaktele","kg",59,{"$nulls":5},0,null,null,0,null,0]
[336,"gatavā špakteļmasa","kg",78.5,{"$nulls":5},0,null,null,0,null,0]
[337,"Sienu virsmu krāsošana","m2",49,{"$nulls":5},0,0,0,null,0,0]
[338,"grunts","l",7.35,{"$nulls":5},0,null,null,0,null,0]
[339,"krāsa tonēta","l",16.3,{"$nulls":5},0,null,null,0,null,0]
[340,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,0,0,0]
[341,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,null,null,0,null,0]
[342,"Gaismas ķermeņu noņemšana","gb",6,{"$nulls":5},0,0,0,null,0,0]
[343,"Elektroinstalācijas montāža","m",45.6,{"$nulls":5},0,0,0,null,0,0]
[344,"kabelis","m",45.6,{"$nulls":5},0,null,null,0,null,0]
[345,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[346,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[347,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[348,"Gaismas ķermeņu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[349,"dienasgaismas lampas","gb",6,{"$nulls":5},0,null,null,0,null,0]
[350,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[351,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[352,"GAITEŅA TELPA  NR.7"]
[353,"Saplaisājušas un bojātas krāsas noņemšana","m2",90,{"$nulls":5},0,0,0,null,0,0]
[354,"Sienu virsmu gruntēšana","m2",238,{"$nulls":5},0,0,0,null,0,0]
[355,"grunts","l",49,{"$nulls":5},0,null,null,0,null,0]
[356,"Griestu gruntēšana","m2",117.4,{"$nulls":5},0,0,0,null,0,0]
[357,"grunts","l",20,{"$nulls":5},0,null,null,0,null,0]
[358,"Griestu krāsošana","m2",117.4,{"$nulls":5},0,0,0,null,0,0]
[359,"krāsa","l",39,{"$nulls":5},0,null,null,0,null,0]
[360,"Sienu virsmu špaktelēšana","m2",238,{"$nulls":5},0,0,0,0,0,0]
[361,"špaktele","kg",333,{"$nulls":5},0,null,null,0,null,0]
[362,"gatavā špakteļmasa","kg",381,{"$nulls":5},0,null,null,0,null,0]
[363,"Sienu virsmu krāsošana","m2",238,{"$nulls":5},0,0,0,0,0,0]
[364,"grunts","l",35.8,{"$nulls":5},0,null,null,0,null,0]
[365,"krāsa tonēta","l",80,{"$nulls":5},0,null,null,0,null,0]
[366,"Koridora grīdas flīžu šuvju pildījuma atjaunošana","m2",49.25,{"$nulls":5},0,0,0,null,0,0]
[367,"grunts","l",6.85,{"$nulls":5},0,null,null,0,null,0]
[368,"šuvju pildviela","kg",24.6,{"$nulls":5},0,null,null,0,null,0]
[369,"Betona pamatojuma gruntēšana","m2",16,{"$nulls":5},0,0,0,null,0,0]
[370,"grunts","l",5,{"$nulls":5},0,null,null,0,null,0]
[371,"Betona pamatojuma špaktelēšana","m2",16,{"$nulls":5},0,0,0,null,0,0]
[372,"betona špaktele","kg",26,{"$nulls":5},0,null,null,0,null,0]
[373,"Betona pamatojuma krāsošana","m2",16,{"$nulls":5},0,0,0,null,0,0]
[374,"krāsa","l",6.5,{"$nulls":5},0,null,null,0,null,0]
[375,"Gaismas ķermeņu noņemšana","gb",8,{"$nulls":5},0,0,0,null,0,0]
[376,"Elektroinstalācijas montāža","m",88,{"$nulls":5},0,0,0,null,0,0]
[377,"kabelis","m",88,{"$nulls":5},0,null,null,0,null,0]
[378,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[379,"slēdzis ar montāžas kārbu","gb",6,{"$nulls":5},0,null,null,0,null,0]
[380,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[381,"Gaismas ķermeņu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[382,"dienasgaismas lampas","gb",8,{"$nulls":5},0,null,null,0,null,0]
[383,"TUALETES TELPA CILVĒKIEM AR ĪPAŠĀM VAJADZĪBĀM "]
[384,"Santehnisko ierīču demontāža","gb",3,{"$nulls":5},0,0,0,null,0,0]
[385,"Esošo durvju izņemšana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[386,"Durvju ailas paplašināšana līdz 1,1m","gb",1,{"$nulls":5},0,0,0,null,0,0]
[387,"Sienas apšuvuma daļēja nojaukšana","m2",4,{"$nulls":5},0,0,0,null,0,0]
[388,"Cauruļvadu montāža lodējot","m",6,{"$nulls":5},0,0,0,null,0,0]
[389,"Cu cietā caurule 18x1,0 mm","m",6,{"$nulls":5},0,null,null,0,null,0]
[390,"Cu veidgabali 18 mm","gb",8,{"$nulls":5},0,null,null,0,null,0]
[391,"izolācija 18/13","m",6,{"$nulls":5},0,null,null,0,null,0]
[392,"Lodveida ventiļu montāža","gb",2,{"$nulls":5},0,0,0,null,0,0]
[393,"lodveida ventilis 3/4\"","gab.",2,{"$nulls":5},0,null,null,0,null,0]
[394,"Kanalizācijas cauruļvadu ar veidgabaliem montāža","m",3,{"$nulls":5},0,0,0,null,0,0]
[395,"caurule DN 50mm","m",3,{"$nulls":5},0,null,null,0,null,0]
[396,"veidgabali","gb",3,{"$nulls":5},0,null,null,0,null,0]
[397,"Durvju uzstādīšana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[398,"durvju vērtne ar kārbu","gb",1,{"$nulls":5},0,null,null,0,null,0]
[399,"WC mehānisms,rokturi","kpl.",1,{"$nulls":5},0,null,null,0,null,0]
[400,"Durvju apmaļu uzstādīšana","m",5.2,{"$nulls":5},0,0,0,null,0,0]
[401,"durvju kleidas","m",5.2,{"$nulls":5},0,null,null,0,null,0]
[402,"Izlietnes uzstādīšana","gb",1,{"$nulls":5},0,0,0,0,0,0]
[403,"Cesabo izlietne ","gb",1,{"$nulls":5},0,null,null,0,null,0]
[404,"jaucējkrāns","gb",1,{"$nulls":5},0,null,null,0,null,0]
[405,"sifons","gb",1,{"$nulls":5},0,null,null,0,null,0]
[406,"Atbalsta roktura montāža pie izlietnes","gb",1,{"$nulls":5},0,0,0,null,0,0]
[407,"atbalsta rokturis","gb",1,{"$nulls":5},0,null,null,0,null,0]
[408,"Tualetes poda uzstādīšana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[409,"Cesabo keramikas WC pods ","gab.",1,{"$nulls":5},0,null,null,0,null,0]
[410,"pieslēgšanās komplekts","gab.",1,{"$nulls":5},0,null,null,0,null,0]
[411,"Paceļama roktura montāža","gb",2,{"$nulls":5},0,0,0,null,0,0]
[412,"Mediclinics paceļams rokturis 80 cm","gb",2,{"$nulls":5},0,null,null,0,null,0]
[413,"Sienas flīzēšana","m2",1,{"$nulls":5},0,0,0,null,0,0]
[414,"sienu flīzes","m2",1.05,{"$nulls":5},0,null,null,0,null,0]
[415,"flīžu līme","kg",5,{"$nulls":5},0,null,null,0,null,0]
[416,"šuvju pildviela","kg",1,{"$nulls":5},0,null,null,0,null,0]
[417,"Grīdas flīzēšana","m2",1,{"$nulls":5},0,0,0,null,0,0]
[418,"grīdas flīzes","m2",1.05,{"$nulls":5},0,null,null,0,null,0]
[419,"flīžu līme","kg",5,{"$nulls":5},0,null,null,0,null,0]
[420,"šuvju pildviela","kg",1,{"$nulls":5},0,null,null,0,null,0]
[421,"Esošo durvju špaktelēšana un slīpēšana","gb",2,{"$nulls":5},0,0,0,null,0,0]
[422,"špakteļtepe","l",2.4,{"$nulls":5},0,null,null,0,null,0]
[423,"smilšpapīrs","m",2,{"$nulls":5},0,null,null,0,null,0]
[424,"Augstvērtīga krāsojuma uzklāšana durvīm","gb",2,{"$nulls":5},0,0,0,null,0,0]
[425,"krāsa kokam","l",1.2,{"$nulls":5},0,null,null,0,null,0]
[426," MĀCĪBU TELPA NR.8 (2.ST)"]
[427,"Dēļu grīdas klāja izjaukšana","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[428,"Dēļu grīdas gulšņu izjaukšana","m",72,{"$nulls":5},0,0,0,null,0,0]
[429,"Būvgružu savākšana","m3",2.6,{"$nulls":5},0,0,0,null,0,0]
[430,"Grīdas gulšņu uzstādīšana","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[431,"kokmateriāls","m3",0.71,{"$nulls":5},0,null,null,0,null,0]
[432,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",41,{"$nulls":5},0,0,0,null,0,0]
[433,"antiseptiķis","l",9,{"$nulls":5},0,null,null,0,null,0]
[434,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[435,"skaņas izolācija 100 mm","m2",50.1,{"$nulls":5},0,null,null,0,null,0]
[436,"Grīdas klāja-melnās grīdas ierīkošana ","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[437,"apzāģēti dēļi","m3",0.41,{"$nulls":5},0,null,null,0,null,0]
[438,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[439,"spundēta plāksne 22 mm","m2",52.6,{"$nulls":5},0,null,null,0,null,0]
[440,"skrūves","gb",750,{"$nulls":5},0,null,null,0,null,0]
[441,"Grīdas virsmas gruntēšana","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[442,"grunts","l",12.5,{"$nulls":5},0,null,null,0,null,0]
[443,"Linoleja ieklāšana pielīmējot visā platībā","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[444,"linolejs 34 klase","m2",52.6,{"$nulls":5},0,null,null,0,null,0]
[445,"linoleja līme","kg",25,{"$nulls":5},0,null,null,0,null,0]
[446,"šuvju kausēšanas diegs","m",21,{"$nulls":5},0,null,null,0,null,0]
[447,"Koka grīdlīstu uzstādīšana","m",28,{"$nulls":5},0,0,0,null,0,0]
[448,"koka grīdlīste,krāsota","m",30.8,{"$nulls":5},0,null,null,0]
[449,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[450,"UD profils","m",28,{"$nulls":5},0,null,null,0,null,0]
[451,"CD profils","m",140,{"$nulls":5},0,null,null,0,null,0]
[452,"U veida skava","gb",45,{"$nulls":5},0,null,null,0,null,0]
[453,"CD profilu savienotājs","gb",21,{"$nulls":5},0,null,null,0,null,0]
[454,"CD profilu šķērssavienotājs","gb",39,{"$nulls":5},0,null,null,0,null,0]
[455,"ģipškartons","m2",52.5,{"$nulls":5},0,null,null,0,null,0]
[456,"apšuvuma skrūves","gb",850,{"$nulls":5},0,null,null,0,null,0]
[457,"dībeļnaglas","gb",90,{"$nulls":5},0,null,null,0,null,0]
[458,"Gipškartona šuvju špaktelēšana","m",64,{"$nulls":5},0,0,0,null,0,0]
[459,"grunts","l",0.6,{"$nulls":5},0,null,null,0,null,0]
[460,"špaktele","kg",16,{"$nulls":5},0,null,null,0,null,0]
[461,"Griestu gruntēšana","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[462,"grunts","l",8.3,{"$nulls":5},0,null,null,0,null,0]
[463,"Griestu krāsošana","m2",50.1,{"$nulls":5},0,0,0,null,0,0]
[464,"krāsa","l",16.7,{"$nulls":5},0,null,null,0,null,0]
[465,"Virsmu apšūšana ar riģipša plāksnēm,tās piestiprinot ar līmjavu","m2",18.9,{"$nulls":5},0,0,0,null,0,0]
[466,"ģipškartona līme","kg",113.4,{"$nulls":5},0,null,null,0,null,0]
[467,"ģipškartons","m2",19.84,{"$nulls":5},0,0,0,0,0,0]
[468,"Gipškartona šuvju špaktelēšana","m",16,{"$nulls":5},0,0,0,null,0,0]
[469,"grunts","l",0.2,{"$nulls":5},0,null,null,0,null,0]
[470,"špaktele","kg",4,{"$nulls":5},0,null,null,0,null,0]
[471,"Saplaisājušas un bojātas krāsas noņemšana","m2",20,{"$nulls":5},0,0,0,null,0,0]
[472,"Sienu virsmu gruntēšana","m2",78.3,{"$nulls":5},0,0,0,null,0,0]
[473,"grunts","l",11.75,{"$nulls":5},0,null,null,0,null,0]
[474,"Sienu virsmu špaktelēšana","m2",78.3,{"$nulls":5},0,0,0,null,0,0]
[475,"špaktele","kg",94,{"$nulls":5},0,null,null,0,null,0]
[476,"gatavā špakteļmasa","kg",125.28,{"$nulls":5},0,null,null,0,null,0]
[477,"Sienu virsmu krāsošana","m2",78.3,{"$nulls":5},0,0,0,null,0,0]
[478,"grunts","l",11.75,{"$nulls":5},0,null,null,0,null,0]
[479,"krāsa tonēta","l",26,{"$nulls":5},0,null,null,0,null,0]
[480,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,null,0,0]
[481,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,null,null,0,null,0]
[482,"Gaismas ķermeņu noņemšana","gb",10,{"$nulls":5},0,0,0,null,0,0]
[483,"Elektroinstalācijas montāža","m",43.2,{"$nulls":5},0,0,0,null,0,0]
[484,"kabelis","m",43.2,{"$nulls":5},0,null,null,0,null,0]
[485,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[486,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[487,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[488,"Gaismas ķermeņu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[489,"dienasgaismas lampas","gb",8,{"$nulls":5},0,null,null,0,null,0]
[490,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[491,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[492," MĀCĪBU TELPA NR.9 (2.ST)"]
[493,"Dēļu grīdas klāja izjaukšana","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[494,"Dēļu grīdas gulšņu izjaukšana","m",74,{"$nulls":5},0,0,0,null,0,0]
[495,"Būvgružu savākšana","m3",2.77,{"$nulls":5},0,0,0,null,0,0]
[496,"Grīdas gulšņu uzstādīšana","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[497,"kokmateriāls","m3",0.77,{"$nulls":5},0,null,null,0,null,0]
[498,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",42,{"$nulls":5},0,0,0,null,0,0]
[499,"antiseptiķis","l",9.2,{"$nulls":5},0,null,null,0,null,0]
[500,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[501,"skaņas izolācija 100 mm","m2",51.61,{"$nulls":5},0,null,null,0,null,0]
[502,"Grīdas klāja-melnās grīdas ierīkošana ","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[503,"apzāģēti dēļi","m3",0.44,{"$nulls":5},0,null,null,0,null,0]
[504,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[505,"spundēta plāksne 22 mm","m2",53.13,{"$nulls":5},0,null,null,0,null,0]
[506,"skrūves","gb",760,{"$nulls":5},0,null,null,0,null,0]
[507,"Grīdas virsmas gruntēšana","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[508,"grunts","l",12.7,{"$nulls":5},0,null,null,0,null,0]
[509,"Linoleja ieklāšana pielīmējot visā platībā","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[510,"linolejs 34 klase","m2",53.13,{"$nulls":5},0,null,null,0,null,0]
[511,"linoleja līme","kg",25.3,{"$nulls":5},0,null,null,0,null,0]
[512,"šuvju kausēšanas diegs","m",21.7,{"$nulls":5},0,null,null,0,null,0]
[513,"Koka grīdlīstu uzstādīšana","m",28.8,{"$nulls":5},0,0,0,null,0,0]
[514,"koka grīdlīste,krāsota","m",21.7,{"$nulls":5},0,null,null,0,null,0]
[515,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",50.6,{"$nulls":5},0,0,0,0,0,0]
[516,"UD profils","m",28.4,{"$nulls":5},0,null,null,0,null,0]
[517,"CD profils","m",141,{"$nulls":5},0,null,null,0,null,0]
[518,"U veida skava","gb",46,{"$nulls":5},0,null,null,0,null,0]
[519,"CD profilu savienotājs","gb",22,{"$nulls":5},0,null,null,0,null,0]
[520,"CD profilu šķērssavienotājs","gb",40,{"$nulls":5},0,null,null,0,null,0]
[521,"ģipškartons","m2",53.15,{"$nulls":5},0,null,null,0,null,0]
[522,"apšuvuma skrūves","gb",855,{"$nulls":5},0,null,null,0,null,0]
[523,"dībeļnaglas","gb",92,{"$nulls":5},0,null,null,0,null,0]
[524,"Gipškartona šuvju špaktelēšana","m",64.4,{"$nulls":5},0,0,0,null,0,0]
[525,"grunts","l",0.62,{"$nulls":5},0,null,null,0,null,0]
[526,"špaktele","kg",16.3,{"$nulls":5},0,null,null,0,null,0]
[527,"Griestu gruntēšana","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[528,"grunts","l",8.4,{"$nulls":5},0,null,null,0,null,0]
[529,"Griestu krāsošana","m2",50.6,{"$nulls":5},0,0,0,null,0,0]
[530,"krāsa","l",16.8,{"$nulls":5},0,null,null,0,null,0]
[531,"Virsmu apšūšana ar riģipša plāksnēm,tās piestiprinot ar līmjavu","m2",37.8,{"$nulls":5},0,0,0,null,0,0]
[532,"ģipškartona līme","kg",226.8,{"$nulls":5},0,null,null,0,null,0]
[533,"ģipškartons","m2",39.69,{"$nulls":5},0,null,null,0,null,0]
[534,"Gipškartona šuvju špaktelēšana","m",33,{"$nulls":5},0,0,0,null,0,0]
[535,"grunts","l",0.4,{"$nulls":5},0,null,null,0,null,0]
[536,"špaktele","kg",8.25,{"$nulls":5},0,null,null,0,null,0]
[537,"Saplaisājušas un bojātas krāsas noņemšana","m2",16,{"$nulls":5},0,0,0,null,0,0]
[538,"Sienu virsmu gruntēšana","m2",84.2,{"$nulls":5},0,0,0,null,0,0]
[539,"grunts","l",12.63,{"$nulls":5},0,null,null,0,null,0]
[540,"Sienu virsmu špaktelēšana","m2",84.2,{"$nulls":5},0,0,0,null,0,0]
[541,"špaktele","kg",101,{"$nulls":5},0,null,null,0,null,0]
[542,"gatavā špakteļmasa","kg",134.7,{"$nulls":5},0,null,null,0,null,0]
[543,"Sienu virsmu krāsošana","m2",84.2,{"$nulls":5},0,0,0,null,0,0]
[544,"grunts","l",12.63,{"$nulls":5},0,null,null,0,null,0]
[545,"krāsa tonēta","l",28,{"$nulls":5},0,null,null,0,null,0]
[546,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,0,0,0]
[547,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,null,null,0,null,0]
[548,"Gaismas ķermeņu noņemšana","gb",10,{"$nulls":5},0,0,0,null,0,0]
[549,"Elektroinstalācijas montāža","m",43.2,{"$nulls":5},0,0,0,null,0,0]
[550,"kabelis","m",43.2,{"$nulls":5},0,null,null,0,null,0]
[551,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[552,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[553,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[554,"Gaismas ķermeņu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[555,"dienasgaismas lampas","gb",8,{"$nulls":5},0,null,null,0,null,0]
[556,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[557,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[558," MĀCĪBU TELPA NR.10 (2.ST)"]
[559,"Dēļu grīdas klāja izjaukšana","m2",54,{"$nulls":5},0,0,0,null,0,0]
[560,"Dēļu grīdas gulšņu izjaukšana","m",77,{"$nulls":5},0,0,0,null,0,0]
[561,"Būvgružu savākšana","m3",2.8,{"$nulls":5},0,0,0,null,0,0]
[562,"Grīdas gulšņu uzstādīšana","m2",54,{"$nulls":5},0,0,0,null,0,0]
[563,"kokmateriāls","m3",0.81,{"$nulls":5},0,null,null,0,null,0]
[564,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",40.45,{"$nulls":5},0,0,0,null,0,0]
[565,"antiseptiķis","l",11,{"$nulls":5},0,null,null,0,null,0]
[566,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",54,{"$nulls":5},0,0,0,null,0,0]
[567,"skaņas izolācija 100 mm","m2",55.08,{"$nulls":5},0,null,null,0,null,0]
[568,"Grīdas klāja-melnās grīdas ierīkošana ","m2",54,{"$nulls":5},0,0,0,null,0,0]
[569,"apzāģēti dēļi","m3",0.44,{"$nulls":5},0,null,null,0,null,0]
[570,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",54,{"$nulls":5},0,0,0,null,0,0]
[571,"spundēta plāksne 22 mm","m2",56.7,{"$nulls":5},0,null,null,0,null,0]
[572,"skrūves","gb",810,{"$nulls":5},0,null,null,0,null,0]
[573,"Grīdas virsmas gruntēšana","m2",54,{"$nulls":5},0,0,0,null,0,0]
[574,"grunts","l",16.2,{"$nulls":5},0,null,null,0,null,0]
[575,"Linoleja ieklāšana pielīmējot visā platībā","m2",54,{"$nulls":5},0,0,0,null,0,0]
[576,"linolejs 34 klase","m2",56.7,{"$nulls":5},0,null,null,0,null,0]
[577,"linoleja līme","kg",27,{"$nulls":5},0,null,null,0,null,0]
[578,"šuvju kausēšanas diegs","m",25,{"$nulls":5},0,null,null,0,null,0]
[579,"Koka grīdlīstu uzstādīšana","m",29,{"$nulls":5},0,0,0,null,0,0]
[580,"koka grīdlīste,krāsota","m",31.9,{"$nulls":5},0,null,null,0,null,0]
[581,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",54,{"$nulls":5},0,0,0,null,0,0]
[582,"UD profils","m",29,{"$nulls":5},0,null,null,0,null,0]
[583,"CD profils","m",144,{"$nulls":5},0,null,null,0,null,0]
[584,"U veida skava","gb",48,{"$nulls":5},0,null,null,0,null,0]
[585,"CD profilu savienotājs","gb",25,{"$nulls":5},0,null,null,0,null,0]
[586,"CD profilu šķērssavienotājs","gb",42,{"$nulls":5},0,null,null,0,null,0]
[587,"ģipškartons","m2",56.7,{"$nulls":5},0,null,null,0,null,0]
[588,"apšuvuma skrūves","gb",920,{"$nulls":5},0,null,null,0,null,0]
[589,"dībeļnaglas","gb",96,{"$nulls":5},0,null,null,0,null,0]
[590,"Gipškartona šuvju špaktelēšana","m",69,{"$nulls":5},0,0,0,null,0,0]
[591,"grunts","l",0.65,{"$nulls":5},0,null,null,0,null,0]
[592,"špaktele","kg",17.25,{"$nulls":5},0,null,null,0,null,0]
[593,"Griestu gruntēšana","m2",54,{"$nulls":5},0,0,0,null,0,0]
[594,"grunts","l",9,{"$nulls":5},0,null,null,0,null,0]
[595,"Griestu krāsošana","m2",54,{"$nulls":5},0,0,0,null,0,0]
[596,"krāsa","l",18,{"$nulls":5},0,null,null,0,null,0]
[597,"Virsmu apšūšana ar riģipša plāksnēm,tās piestiprinot ar līmjavu","m2",18.9,{"$nulls":5},0,0,0,null,0,0]
[598,"ģipškartona līme","kg",113.4,{"$nulls":5},0,null,null,0,null,0]
[599,"ģipškartons","m2",19.84,{"$nulls":5},0,0,0,0,0,0]
[600,"Gipškartona šuvju špaktelēšana","m",16,{"$nulls":5},0,0,0,null,0,0]
[601,"grunts","l",0.2,{"$nulls":5},0,null,null,0,null,0]
[602,"špaktele","kg",4,{"$nulls":5},0,null,null,0,null,0]
[603,"Saplaisājušas un bojātas krāsas noņemšana","m2",20.5,{"$nulls":5},0,0,0,null,0,0]
[604,"Sienu virsmu gruntēšana","m2",82.1,{"$nulls":5},0,0,0,null,0,0]
[605,"grunts","l",12.31,{"$nulls":5},0,null,null,0,null,0]
[606,"Sienu virsmu špaktelēšana","m2",82.1,{"$nulls":5},0,0,0,null,0,0]
[607,"špaktele","kg",98.5,{"$nulls":5},0,null,null,0,null,0]
[608,"gatavā špakteļmasa","kg",131.36,{"$nulls":5},0,null,null,0,null,0]
[609,"Sienu virsmu krāsošana","m2",82.1,{"$nulls":5},0,0,0,null,0,0]
[610,"grunts","l",12.31,{"$nulls":5},0,null,null,0,null,0]
[611,"krāsa tonēta","l",27.3,{"$nulls":5},0,null,null,0,null,0]
[612,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,null,0,0]
[613,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,null,null,0,null,0]
[614,"Gaismas ķermeņu noņemšana","gb",10,{"$nulls":5},0,0,0,null,0,0]
[615,"Elektroinstalācijas montāža","m",45.2,{"$nulls":5},0,0,0,null,0,0]
[616,"kabelis","m",45.2,{"$nulls":5},0,null,null,0,null,0]
[617,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[618,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[619,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[620,"Gaismas ķermeņu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[621,"dienasgaismas lampas","gb",8,{"$nulls":5},0,null,null,0,null,0]
[622,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[623,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[624," MĀCĪBU TELPA NR.11 (2.ST)"]
[625,"Dēļu grīdas klāja izjaukšana","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[626,"Dēļu grīdas gulšņu izjaukšana","m",67,{"$nulls":5},0,0,0,null,0,0]
[627,"Būvgružu savākšana","m3",2.47,{"$nulls":5},0,0,0,null,0,0]
[628,"Grīdas gulšņu uzstādīšana","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[629,"kokmateriāls","m3",1.28,{"$nulls":5},0,null,null,0,null,0]
[630,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",51.94,{"$nulls":5},0,0,0,null,0,0]
[631,"antiseptiķis","l",12,{"$nulls":5},0,null,null,0,null,0]
[632,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[633,"skaņas izolācija 100 mm","m2",49.24,{"$nulls":5},0,null,null,0,null,0]
[634,"Grīdas klāja-melnās grīdas ierīkošana ","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[635,"apzāģēti dēļi","m3",0.39,{"$nulls":5},0,null,null,0,null,0]
[636,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[637,"spundēta plāksne 22 mm","m2",49.24,{"$nulls":5},0,null,null,0,null,0]
[638,"skrūves","gb",715,{"$nulls":5},0,null,null,0,null,0]
[639,"Grīdas virsmas gruntēšana","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[640,"grunts","l",14.1,{"$nulls":5},0,null,null,0,null,0]
[641,"Linoleja ieklāšana pielīmējot visā platībā","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[642,"linolejs 34 klase","m2",49.24,{"$nulls":5},0,null,null,0,null,0]
[643,"linoleja līme","kg",23.45,{"$nulls":5},0,null,null,0,null,0]
[644,"šuvju kausēšanas diegs","m",19,{"$nulls":5},0,null,null,0,null,0]
[645,"Koka grīdlīstu uzstādīšana","m",26,{"$nulls":5},0,0,0,null,0,0]
[646,"koka grīdlīste,krāsota","m",28.6,{"$nulls":5},0,null,null,0,null,0]
[647,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[648,"UD profils","m",28,{"$nulls":5},0,null,null,0,null,0]
[649,"CD profils","m",140,{"$nulls":5},0,null,null,0,null,0]
[650,"CD profilu ātrā enkuriekare","gb",42,{"$nulls":5},0,null,null,0,null,0]
[651,"enkuriekares stieple ar cilpu","gb",42,{"$nulls":5},0,null,null,0,null,0]
[652,"CD profilu savienotājs","gb",24,{"$nulls":5},0,null,null,0,null,0]
[653,"CD profilu šķērssavienotājs","gb",40,{"$nulls":5},0,null,null,0,null,0]
[654,"ģipškartons","m2",49.24,{"$nulls":5},0,null,null,0,null,0]
[655,"apšuvuma skrūves","gb",615,{"$nulls":5},0,null,null,0,null,0]
[656,"dībeļnaglas","gb",84,{"$nulls":5},0,null,null,0,null,0]
[657,"Gipškartona šuvju špaktelēšana","m",60,{"$nulls":5},0,0,0,null,0,0]
[658,"grunts","l",0.54,{"$nulls":5},0,null,null,0,null,0]
[659,"špaktele","kg",15,{"$nulls":5},0,null,null,0,null,0]
[660,"Griestu gruntēšana","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[661,"grunts","l",7.8,{"$nulls":5},0,null,null,0,null,0]
[662,"Griestu krāsošana","m2",46.9,{"$nulls":5},0,0,0,null,0,0]
[663,"krāsa","l",15.6,{"$nulls":5},0,null,null,0,null,0]
[664,"Virsmu apšūšana ar riģipša plāksnēm,tās piestiprinot ar līmjavu","m2",24.25,{"$nulls":5},0,0,0,null,0,0]
[665,"ģipškartona līme","kg",144,{"$nulls":5},0,null,null,0,null,0]
[666,"ģipškartons","m2",25.46,{"$nulls":5},0,null,null,0,null,0]
[667,"Gipškartona šuvju špaktelēšana","m",19,{"$nulls":5},0,0,0,null,0,0]
[668,"grunts","l",0.2,{"$nulls":5},0,null,null,0,null,0]
[669,"špaktele","kg",4.75,{"$nulls":5},0,null,null,0,null,0]
[670,"Saplaisājušas un bojātas krāsas noņemšana","m2",20,{"$nulls":5},0,0,0,null,0,0]
[671,"Sienu virsmu gruntēšana","m2",79.56,{"$nulls":5},0,0,0,null,0,0]
[672,"grunts","l",12,{"$nulls":5},0,null,null,0,null,0]
[673,"Uzlabots cementa-kaļķu javas apmetums","m2",13,{"$nulls":5},0,0,0,null,0,0]
[674,"apmetuma java","kg",130,{"$nulls":5},0,null,null,0,null,0]
[675,"Sienu virsmu izlīdzināšana līdz 10mm","m2",13,{"$nulls":5},0,0,0,null,0,0]
[676,"ģipšapmetums","kg",79,{"$nulls":5},0,null,null,0,null,0]
[677,"stiklašķiedras siets ","m2",14.3,{"$nulls":5},0,null,null,0,null,0]
[678,"Sienu virsmu špaktelēšana","m2",79.56,{"$nulls":5},0,0,0,null,0,0]
[679,"špaktele","kg",96,{"$nulls":5},0,null,null,0,null,0]
[680,"gatavā špakteļmasa","kg",128,{"$nulls":5},0,null,null,0,null,0]
[681,"Sienu virsmu krāsošana","m2",79.56,{"$nulls":5},0,0,0,null,0,0]
[682,"grunts","l",12,{"$nulls":5},0,null,null,0,null,0]
[683,"krāsa tonēta","l",26.7,{"$nulls":5},0,null,null,0,null,0]
[684,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,null,0,0]
[685,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,null,null,0,null,0]
[686,"Durvju ailas aizšūšana ar ģipškartonu","m2",2.1,{"$nulls":5},0,0,0,null,0,0]
[687,"ģipškartons","m2",4.41,{"$nulls":5},0,null,null,0,null,0]
[688,"skaņas izolācija 200 mm","m2",4.41,{"$nulls":5},0,null,null,0,null,0]
[689,"UD profils","m",12,{"$nulls":5},0,null,null,0,null,0]
[690,"CD profils","m",10,{"$nulls":5},0,null,null,0,null,0]
[691,"Jaunas durvju ailas izveidošana","m2",2.1,{"$nulls":5},0,0,0,null,0,0]
[692,"Durvju uzstādīšana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[693,"montāžas putas","gb",1,{"$nulls":5},0,null,null,0,null,0]
[694,"Esošās elektroinstalācijas demontāža","m",42,{"$nulls":5},0,0,0,null,0,0]
[695,"Esošo gaismas ķermeņu noņemšana","gb",6,{"$nulls":5},0,0,0,null,0,0]
[696,"Apgaismes elektrosadales demontāža","gb",2,{"$nulls":5},0,0,0,null,0,0]
[697,"Kabeļu iefrēzēšana sienā","m",90,{"$nulls":5},0,0,0,null,0,0]
[698,"kabelis 3x1,5 mm2","m",55,{"$nulls":5},0,null,null,0,null,0]
[699,"kabelis 3x2,5 mm2","m",35,{"$nulls":5},0,null,null,0,null,0]
[700,"Apgaismes elektrosadales montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[701,"elektrosadale","gb",1,{"$nulls":5},0,null,null,0,null,0]
[702,"Vienpola automātisko slēdžu montāža","gb",10,{"$nulls":5},0,0,0,null,0,0]
[703,"automātiskais slēdzis","gb",10,{"$nulls":5},0,null,null,0,null,0]
[704,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[705,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[706,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[707,"Gaismas ķermeņu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[708,"dienasgaismas lampas","gb",6,{"$nulls":5},0,null,null,0,null,0]
[709," MĀCĪBU TELPA NR.12 (2.ST)"]
[710,"Dēļu grīdas klāja izjaukšana","m2",52,{"$nulls":5},0,0,0,null,0,0]
[711,"Dēļu grīdas gulšņu izjaukšana","m",74,{"$nulls":5},0,0,0,null,0,0]
[712,"Būvgružu savākšana","m3",2.6,{"$nulls":5},0,0,0,null,0,0]
[713,"Grīdas gulšņu uzstādīšana","m2",52,{"$nulls":5},0,0,0,null,0,0]
[714,"kokmateriāls","m3",0.77,{"$nulls":5},0,null,null,0,null,0]
[715,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",42.5,{"$nulls":5},0,0,0,null,0,0]
[716,"antiseptiķis","l",9,{"$nulls":5},0,null,null,0,null,0]
[717,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",52,{"$nulls":5},0,0,0,null,0,0]
[718,"skaņas izolācija 100 mm","m2",54.6,{"$nulls":5},0,null,null,0,null,0]
[719,"Grīdas klāja-melnās grīdas ierīkošana ","m2",54,{"$nulls":5},0,0,0,null,0,0]
[720,"apzāģēti dēļi","m3",0.42,{"$nulls":5},0,null,null,0,null,0]
[721,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",52,{"$nulls":5},0,0,0,null,0,0]
[722,"spundēta plāksne 22 mm","m2",54.6,{"$nulls":5},0,null,null,0,null,0]
[723,"skrūves","gb",780,{"$nulls":5},0,null,null,0,null,0]
[724,"Grīdas virsmas gruntēšana","m2",52,{"$nulls":5},0,0,0,null,0,0]
[725,"grunts","l",15.6,{"$nulls":5},0,null,null,0,null,0]
[726,"Linoleja ieklāšana pielīmējot visā platībā","m2",52,{"$nulls":5},0,0,0,null,0,0]
[727,"linolejs 34 klase","m2",54.6,{"$nulls":5},0,null,null,0,null,0]
[728,"linoleja līme","kg",26,{"$nulls":5},0,null,null,0,null,0]
[729,"šuvju kausēšanas diegs","m",19,{"$nulls":5},0,null,null,0,null,0]
[730,"Koka grīdlīstu uzstādīšana","m",28,{"$nulls":5},0,0,0,null,0,0]
[731,"koka grīdlīste,krāsota","m",30.8,{"$nulls":5},0,null,null,0,null,0]
[732,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",52,{"$nulls":5},0,0,0,null,0,0]
[733,"UD profils","m",28,{"$nulls":5},0,null,null,0,null,0]
[734,"CD profils","m",141,{"$nulls":5},0,null,null,0,null,0]
[735,"U veida skava","gb",46,{"$nulls":5},0,null,null,0,null,0]
[736,"CD profilu savienotājs","gb",24,{"$nulls":5},0,null,null,0,null,0]
[737,"CD profilu šķērssavienotājs","gb",40,{"$nulls":5},0,null,null,0,null,0]
[738,"ģipškartons","m2",54.6,{"$nulls":5},0,null,null,0,null,0]
[739,"apšuvuma skrūves","gb",740,{"$nulls":5},0,null,null,0,null,0]
[740,"dībeļnaglas","gb",92,{"$nulls":5},0,null,null,0,null,0]
[741,"Gipškartona šuvju špaktelēšana","m",66,{"$nulls":5},0,0,0,null,0,0]
[742,"grunts","l",0.59,{"$nulls":5},0,null,null,0,null,0]
[743,"špaktele","kg",16.5,{"$nulls":5},0,null,null,0,null,0]
[744,"Griestu gruntēšana","m2",52,{"$nulls":5},0,0,0,null,0,0]
[745,"grunts","l",8.6,{"$nulls":5},0,null,null,0,null,0]
[746,"Griestu krāsošana","m2",52,{"$nulls":5},0,0,0,null,0,0]
[747,"krāsa","l",17.2,{"$nulls":5},0,null,null,0,null,0]
[748,"Saplaisājušas un bojātas krāsas noņemšana","m2",19,{"$nulls":5},0,0,0,null,0,0]
[749,"Sienu virsmu gruntēšana","m2",79.9,{"$nulls":5},0,0,0,null,0,0]
[750,"grunts","l",12,{"$nulls":5},0,null,null,0,null,0]
[751,"Sienu virsmu špaktelēšana","m2",79.9,{"$nulls":5},0,0,0,null,0,0]
[752,"špaktele","kg",96,{"$nulls":5},0,null,null,0,null,0]
[753,"gatavā špakteļmasa","kg",128,{"$nulls":5},0,null,null,0,null,0]
[754,"Sienu virsmu krāsošana","m2",79.9,{"$nulls":5},0,0,0,null,0,0]
[755,"grunts","l",12,{"$nulls":5},0,null,null,0,null,0]
[756,"krāsa tonēta","l",26.7,{"$nulls":5},0,null,null,0,null,0]
[757,"Radiatoru krāsošana","gb",3,{"$nulls":5},0,0,0,0,0,0]
[758,"krāsa radiatoriem","l",2.7,{"$nulls":5},0,null,null,0,null,0]
[759,"Gaismas ķermeņu noņemšana","gb",10,{"$nulls":5},0,0,0,null,0,0]
[760,"Elektroinstalācijas montāža","m",46.1,{"$nulls":5},0,0,0,null,0,0]
[761,"kabelis","m",46.1,{"$nulls":5},0,null,null,0,null,0]
[762,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[763,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[764,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[765,"Gaismas ķermeņu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[766,"dienasgaismas lampas","gb",8,{"$nulls":5},0,null,null,0,null,0]
[767,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[768,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[769," DIREKTORES KABINETS TELPA NR.13 (2.ST)"]
[770,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",18.2,{"$nulls":5},0,0,0,null,0,0]
[771,"spundēta plāksne 22 mm","m2",19.11,{"$nulls":5},0,null,null,0,null,0]
[772,"skrūves","gb",280,{"$nulls":5},0,null,null,0,null,0]
[773,"Grīdas virsmas gruntēšana","m2",18.2,{"$nulls":5},0,0,0,null,0,0]
[774,"grunts","l",5.46,{"$nulls":5},0,null,null,0,null,0]
[775,"Linoleja ieklāšana pielīmējot visā platībā","m2",18.2,{"$nulls":5},0,0,0,null,0,0]
[776,"linolejs 34 klase","m2",19.11,{"$nulls":5},0,null,null,0,null,0]
[777,"linoleja līme","kg",9.1,{"$nulls":5},0,null,null,0,null,0]
[778,"šuvju kausēšanas diegs","m",10,{"$nulls":5},0,null,null,0,null,0]
[779,"Koka grīdlīstu uzstādīšana","m",18.5,{"$nulls":5},0,0,0,null,0,0]
[780,"koka grīdlīste,krāsota","m",20.35,{"$nulls":5},0,null,null,0,null,0]
[781,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",18.2,{"$nulls":5},0,0,0,null,0,0]
[782,"UD profils","m",18,{"$nulls":5},0,null,null,0,null,0]
[783,"CD profils","m",64,{"$nulls":5},0,null,null,0,null,0]
[784,"U veida skava","gb",20,{"$nulls":5},0,null,null,0,null,0]
[785,"CD profilu savienotājs","gb",15,{"$nulls":5},0,null,null,0,null,0]
[786,"CD profilu šķērssavienotājs","gb",18,{"$nulls":5},0,null,null,0,null,0]
[787,"ģipškartons","m2",19.11,{"$nulls":5},0,null,null,0,null,0]
[788,"apšuvuma skrūves","gb",288,{"$nulls":5},0,null,null,0,null,0]
[789,"dībeļnaglas","gb",60,{"$nulls":5},0,null,null,0,null,0]
[790,"Gipškartona šuvju špaktelēšana","m",23,{"$nulls":5},0,0,0,null,0,0]
[791,"grunts","l",0.2,{"$nulls":5},0,null,null,0,null,0]
[792,"špaktele","kg",5.75,{"$nulls":5},0,null,null,0,null,0]
[793,"Griestu gruntēšana","m2",18.2,{"$nulls":5},0,0,0,0,0,0]
[794,"grunts","l",3.1,{"$nulls":5},0,null,null,0,null,0]
[795,"Griestu krāsošana","m2",18.2,{"$nulls":5},0,0,0,null,0,0]
[796,"krāsa","l",6.2,{"$nulls":5},0,null,null,0,null,0]
[797,"Saplaisājušas un bojātas krāsas noņemšana","m2",10.7,{"$nulls":5},0,0,0,null,0,0]
[798,"Sienu virsmu gruntēšana","m2",43.44,{"$nulls":5},0,0,0,null,0,0]
[799,"grunts","l",6.51,{"$nulls":5},0,null,null,0,null,0]
[800,"Sienu virsmu špaktelēšana","m2",43.44,{"$nulls":5},0,0,0,null,0,0]
[801,"špaktele","kg",53,{"$nulls":5},0,null,null,0,null,0]
[802,"gatavā špakteļmasa","kg",69,{"$nulls":5},0,null,null,0,null,0]
[803,"Sienu virsmu krāsošana","m2",43.44,{"$nulls":5},0,0,0,null,0,0]
[804,"grunts","l",6.51,{"$nulls":5},0,null,null,0,null,0]
[805,"krāsa tonēta","l",14.3,{"$nulls":5},0,null,null,0,null,0]
[806,"Radiatoru krāsošana","gb",2,{"$nulls":5},0,0,0,null,0,0]
[807,"krāsa radiatoriem","l",1.8,{"$nulls":5},0,null,null,0,null,0]
[808,"Gaismas ķermeņu noņemšana","gb",3,{"$nulls":5},0,0,0,null,0,0]
[809,"Elektroinstalācijas montāža","m",27,{"$nulls":5},0,0,0,null,0,0]
[810,"kabelis","m",27,{"$nulls":5},0,null,null,0,null,0]
[811,"Slēdžu un kontaktu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[812,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[813,"kontaktligzda ar montāžas kārbu","gb",4,{"$nulls":5},0,null,null,0,null,0]
[814,"Gaismas ķermeņu montāža","gb",18,{"$nulls":5},0,0,0,null,0,0]
[815,"iebūvējamie gaismas ķermeņi","gb",18,{"$nulls":5},0,null,null,0,null,0]
[816," DIREKTORES VIETNIEKU KABINETS TELPA NR.14 (2.ST)"]
[817,"Dēļu grīdas klāja izjaukšana","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[818,"Dēļu grīdas gulšņu izjaukšana","m",40,{"$nulls":5},0,0,0,null,0,0]
[819,"Būvgružu savākšana","m3",1.43,{"$nulls":5},0,0,0,null,0,0]
[820,"Grīdas gulšņu uzstādīšana","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[821,"kokmateriāls","m3",0.39,{"$nulls":5},0,null,null,0,null,0]
[822,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",23,{"$nulls":5},0,0,0,null,0,0]
[823,"antiseptiķis","l",6,{"$nulls":5},0,null,null,0,null,0]
[824,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[825,"skaņas izolācija 100 mm","m2",28.05,{"$nulls":5},0,null,null,0,null,0]
[826,"Grīdas klāja-melnās grīdas ierīkošana ","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[827,"apzāģēti dēļi","m3",0.23,{"$nulls":5},0,null,null,0,null,0]
[828,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[829,"spundēta plāksne 22 mm","m2",28.87,{"$nulls":5},0,null,null,0,null,0]
[830,"skrūves","gb",405,{"$nulls":5},0,null,null,0,null,0]
[831,"Grīdas virsmas gruntēšana","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[832,"grunts","l",8.25,{"$nulls":5},0,null,null,0,null,0]
[833,"Linoleja ieklāšana pielīmējot visā platībā","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[834,"linolejs 34 klase","m2",28.87,{"$nulls":5},0,null,null,0,null,0]
[835,"linoleja līme","kg",13.75,{"$nulls":5},0,null,null,0,null,0]
[836,"šuvju kausēšanas diegs","m",11,{"$nulls":5},0,null,null,0,null,0]
[837,"Koka grīdlīstu uzstādīšana","m",21,{"$nulls":5},0,0,0,null,0,0]
[838,"koka grīdlīste,krāsota","m",23.1,{"$nulls":5},0,null,null,0,null,0]
[839,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[840,"UD profils","m",21,{"$nulls":5},0,null,null,0,null,0]
[841,"CD profils","m",68,{"$nulls":5},0,null,null,0,null,0]
[842,"U veida skava","gb",28,{"$nulls":5},0,null,null,0,null,0]
[843,"CD profilu savienotājs","gb",12,{"$nulls":5},0,null,null,0,null,0]
[844,"CD profilu šķērssavienotājs","gb",30,{"$nulls":5},0,null,null,0,null,0]
[845,"ģipškartons","m2",28.87,{"$nulls":5},0,null,null,0,null,0]
[846,"apšuvuma skrūves","gb",467,{"$nulls":5},0,null,null,0,null,0]
[847,"dībeļnaglas","gb",56,{"$nulls":5},0,null,null,0,null,0]
[848,"Gipškartona šuvju špaktelēšana","m",36,{"$nulls":5},0,0,0,null,0,0]
[849,"grunts","l",0.32,{"$nulls":5},0,null,null,0,null,0]
[850,"špaktele","kg",9,{"$nulls":5},0,null,null,0,null,0]
[851,"Griestu gruntēšana","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[852,"grunts","l",4.6,{"$nulls":5},0,null,null,0,null,0]
[853,"Griestu krāsošana","m2",27.5,{"$nulls":5},0,0,0,null,0,0]
[854,"krāsa","l",9.1,{"$nulls":5},0,null,null,0,null,0]
[855,"Virsmu apšūšana ar riģipša plāksnēm,tās piestiprinot ar līmjavu","m2",15.95,{"$nulls":5},0,0,0,null,0,0]
[856,"ģipškartona līme","kg",96,{"$nulls":5},0,null,null,0,null,0]
[857,"ģipškartons","m2",16.74,{"$nulls":5},0,null,null,0,null,0]
[858,"Gipškartona šuvju špaktelēšana","m",15.8,{"$nulls":5},0,0,0,null,0,0]
[859,"grunts","l",0.15,{"$nulls":5},0,null,null,0,null,0]
[860,"špaktele","kg",4,{"$nulls":5},0,null,null,0,null,0]
[861,"Saplaisājušas un bojātas krāsas noņemšana","m2",14,{"$nulls":5},0,0,0,null,0,0]
[862,"Sienu virsmu gruntēšana","m2",56,{"$nulls":5},0,0,0,null,0,0]
[863,"grunts","l",8.4,{"$nulls":5},0,null,null,0,null,0]
[864,"Sienu virsmu špaktelēšana","m2",56,{"$nulls":5},0,0,0,null,0,0]
[865,"špaktele","kg",67.2,{"$nulls":5},0,null,null,0,null,0]
[866,"gatavā špakteļmasa","kg",89.6,{"$nulls":5},0,null,null,0,null,0]
[867,"Sienu virsmu krāsošana","m2",56,{"$nulls":5},0,0,0,0,0,0]
[868,"grunts","l",8.4,{"$nulls":5},0,null,null,0,null,0]
[869,"krāsa tonēta","l",18,{"$nulls":5},0,null,null,0,null,0]
[870,"Radiatoru krāsošana","gb",2,{"$nulls":5},0,0,0,null,0,0]
[871,"krāsa radiatoriem","l",1.8,{"$nulls":5},0,null,null,0,null,0]
[872,"Gaismas ķermeņu noņemšana","gb",3,{"$nulls":5},0,0,0,null,0,0]
[873,"Elektroinstalācijas montāža","m",32,{"$nulls":5},0,0,0,null,0,0]
[874,"kabelis","m",32,{"$nulls":5},0,null,null,0,null,0]
[875,"Slēdžu un kontaktu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[876,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[877,"kontaktligzda ar montāžas kārbu","gb",6,{"$nulls":5},0,null,null,0,null,0]
[878,"Gaismas ķermeņu montāža","gb",10,{"$nulls":5},0,0,0,null,0,0]
[879,"iebūvējamie gaismas ķermeņi","gb",10,{"$nulls":5},0,null,null,0,null,0]
[880," SKOLOTĀJU ISTABA TELPA NR.15 (2.ST)"]
[881,"Dēļu grīdas klāja izjaukšana","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[882,"Dēļu grīdas gulšņu izjaukšana","m",25,{"$nulls":5},0,0,0,null,0,0]
[883,"Būvgružu savākšana","m3",0.92,{"$nulls":5},0,0,0,null,0,0]
[884,"Grīdas gulšņu uzstādīšana","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[885,"kokmateriāls","m3",0.25,{"$nulls":5},0,null,null,0,null,0]
[886,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",14.3,{"$nulls":5},0,0,0,null,0,0]
[887,"antiseptiķis","l",3,{"$nulls":5},0,null,null,0,null,0]
[888,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[889,"skaņas izolācija 100 mm","m2",18.05,{"$nulls":5},0,null,null,0,null,0]
[890,"Grīdas klāja-melnās grīdas ierīkošana ","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[891,"apzāģēti dēļi","m3",0.14,{"$nulls":5},0,null,null,0,null,0]
[892,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[893,"spundēta plāksne 22 mm","m2",18.58,{"$nulls":5},0,null,null,0,null,0]
[894,"skrūves","gb",265,{"$nulls":5},0,null,null,0,null,0]
[895,"Grīdas virsmas gruntēšana","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[896,"grunts","l",5.3,{"$nulls":5},0,null,null,0,null,0]
[897,"Linoleja ieklāšana pielīmējot visā platībā","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[898,"linolejs 34 klase","m2",18.58,{"$nulls":5},0,null,null,0,null,0]
[899,"linoleja līme","kg",8.85,{"$nulls":5},0,null,null,0,null,0]
[900,"šuvju kausēšanas diegs","m",7,{"$nulls":5},0,null,null,0,null,0]
[901,"Koka grīdlīstu uzstādīšana","m",17,{"$nulls":5},0,0,0,null,0,0]
[902,"koka grīdlīste,krāsota","m",18.7,{"$nulls":5},0,null,null,0,null,0]
[903,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[904,"UD profils","m",17,{"$nulls":5},0,null,null,0,null,0]
[905,"CD profils","m",38,{"$nulls":5},0,null,null,0,null,0]
[906,"U veida skava","gb",18,{"$nulls":5},0,null,null,0,null,0]
[907,"CD profilu savienotājs","gb",14,{"$nulls":5},0,null,null,0,null,0]
[908,"CD profilu šķērssavienotājs","gb",16,{"$nulls":5},0,null,null,0,null,0]
[909,"ģipškartons","m2",18.58,{"$nulls":5},0,null,null,0,null,0]
[910,"apšuvuma skrūves","gb",270,{"$nulls":5},0,null,null,0,null,0]
[911,"dībeļnaglas","gb",40,{"$nulls":5},0,null,null,0,null,0]
[912,"Gipškartona šuvju špaktelēšana","m",23,{"$nulls":5},0,0,0,null,0,0]
[913,"grunts","l",0.21,{"$nulls":5},0,null,null,0,null,0]
[914,"špaktele","kg",5.75,{"$nulls":5},0,null,null,0,null,0]
[915,"Griestu gruntēšana","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[916,"grunts","l",3,{"$nulls":5},0,null,null,0,null,0]
[917,"Griestu krāsošana","m2",17.7,{"$nulls":5},0,0,0,null,0,0]
[918,"krāsa","l",11.5,{"$nulls":5},0,null,null,0,null,0]
[919,"Virsmu apšūšana ar riģipša plāksnēm,tās piestiprinot ar līmjavu","m2",17.95,{"$nulls":5},0,0,0,null,0,0]
[920,"ģipškartona līme","kg",108,{"$nulls":5},0,null,null,0,null,0]
[921,"ģipškartons","m2",18.85,{"$nulls":5},0,null,null,0,null,0]
[922,"Gipškartona šuvju špaktelēšana","m",19.8,{"$nulls":5},0,0,0,null,0,0]
[923,"grunts","l",0.18,{"$nulls":5},0,null,null,0,null,0]
[924,"špaktele","kg",5,{"$nulls":5},0,null,null,0,null,0]
[925,"Saplaisājušas un bojātas krāsas noņemšana","m2",11,{"$nulls":5},0,0,0,null,0,0]
[926,"Sienu virsmu gruntēšana","m2",45,{"$nulls":5},0,0,0,null,0,0]
[927,"grunts","l",6.75,{"$nulls":5},0,null,null,0,null,0]
[928,"Sienu virsmu špaktelēšana","m2",45,{"$nulls":5},0,0,0,null,0,0]
[929,"špaktele","kg",54,{"$nulls":5},0,null,null,0,null,0]
[930,"gatavā špakteļmasa","kg",72,{"$nulls":5},0,null,null,0,null,0]
[931,"Sienu virsmu krāsošana","m2",45,{"$nulls":5},0,0,0,null,0,0]
[932,"grunts","l",6.75,{"$nulls":5},0,null,null,0,null,0]
[933,"krāsa tonēta","l",15,{"$nulls":5},0,null,null,0,null,0]
[934,"Radiatoru krāsošana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[935,"krāsa radiatoriem","l",0.9,{"$nulls":5},0,null,null,0,null,0]
[936,"Gaismas ķermeņu noņemšana","gb",4,{"$nulls":5},0,0,0,null,0,0]
[937,"Elektroinstalācijas montāža","m",34,{"$nulls":5},0,0,0,null,0,0]
[938,"kabelis","m",34,{"$nulls":5},0,null,null,0,null,0]
[939,"Slēdžu un kontaktu montāža","gb",14,{"$nulls":5},0,0,0,null,0,0]
[940,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[941,"kontaktligzda ar montāžas kārbu","gb",12,{"$nulls":5},0,null,null,0,null,0]
[942,"Gaismas ķermeņu montāža","gb",18,{"$nulls":5},0,0,0,null,0,0]
[943,"iebūvējamie gaismas ķermeņi","gb",18,{"$nulls":5},0,null,null,0,null,0]
[944," MĀCĪBU TELPA NR.16 (2.ST)"]
[945,"Dēļu grīdas klāja izjaukšana","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[946,"Dēļu grīdas gulšņu izjaukšana","m",46,{"$nulls":5},0,0,0,null,0,0]
[947,"Būvgružu savākšana","m3",1.67,{"$nulls":5},0,0,0,null,0,0]
[948,"Grīdas gulšņu uzstādīšana","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[949,"kokmateriāls","m3",0.45,{"$nulls":5},0,null,null,0,null,0]
[950,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",26.4,{"$nulls":5},0,0,0,null,0,0]
[951,"antiseptiķis","l",7,{"$nulls":5},0,null,null,0,null,0]
[952,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[953,"skaņas izolācija 100 mm","m2",32.23,{"$nulls":5},0,null,null,0,null,0]
[954,"Grīdas klāja-melnās grīdas ierīkošana ","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[955,"apzāģēti dēļi","m3",0.26,{"$nulls":5},0,null,null,0,null,0]
[956,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[957,"spundēta plāksne 22 mm","m2",33.18,{"$nulls":5},0,null,null,0,null,0]
[958,"skrūves","gb",480,{"$nulls":5},0,null,null,0,null,0]
[959,"Grīdas virsmas gruntēšana","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[960,"grunts","l",9.48,{"$nulls":5},0,null,null,0,null,0]
[961,"Linoleja ieklāšana pielīmējot visā platībā","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[962,"linolejs 34 klase","m2",33.18,{"$nulls":5},0,null,null,0,null,0]
[963,"linoleja līme","kg",15.8,{"$nulls":5},0,null,null,0,null,0]
[964,"šuvju kausēšanas diegs","m",12,{"$nulls":5},0,null,null,0,null,0]
[965,"Koka grīdlīstu uzstādīšana","m",21,{"$nulls":5},0,0,0,null,0,0]
[966,"koka grīdlīste,krāsota","m",23.1,{"$nulls":5},0,null,null,0,null,0]
[967,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[968,"UD profils","m",21,{"$nulls":5},0,null,null,0,null,0]
[969,"CD profils","m",64,{"$nulls":5},0,null,null,0,null,0]
[970,"U veida skava","gb",28,{"$nulls":5},0,null,null,0,null,0]
[971,"CD profilu savienotājs","gb",16,{"$nulls":5},0,null,null,0,null,0]
[972,"CD profilu šķērssavienotājs","gb",20,{"$nulls":5},0,null,null,0,null,0]
[973,"ģipškartons","m2",33.18,{"$nulls":5},0,null,null,0,null,0]
[974,"apšuvuma skrūves","gb",480,{"$nulls":5},0,null,null,0,null,0]
[975,"dībeļnaglas","gb",56,{"$nulls":5},0,null,null,0,null,0]
[976,"Gipškartona šuvju špaktelēšana","m",40,{"$nulls":5},0,0,0,null,0,0]
[977,"grunts","l",0.36,{"$nulls":5},0,null,null,0,null,0]
[978,"špaktele","kg",10,{"$nulls":5},0,null,null,0,null,0]
[979,"Griestu gruntēšana","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[980,"grunts","l",5.3,{"$nulls":5},0,null,null,0,null,0]
[981,"Griestu krāsošana","m2",31.6,{"$nulls":5},0,0,0,null,0,0]
[982,"krāsa","l",10.6,{"$nulls":5},0,0,0,0,0,0]
[983,"Virsmu apšūšana ar riģipša plāksnēm,tās piestiprinot ar līmjavu","m2",18.27,{"$nulls":5},0,0,0,null,0,0]
[984,"ģipškartona līme","kg",109.8,{"$nulls":5},0,null,null,0,null,0]
[985,"ģipškartons","m2",19.18,{"$nulls":5},0,null,null,0,null,0]
[986,"Gipškartona šuvju špaktelēšana","m",16,{"$nulls":5},0,0,0,null,0,0]
[987,"grunts","l",0.14,{"$nulls":5},0,null,null,0,null,0]
[988,"špaktele","kg",4,{"$nulls":5},0,null,null,0,null,0]
[989,"Saplaisājušas un bojātas krāsas noņemšana","m2",15,{"$nulls":5},0,0,0,null,0,0]
[990,"Sienu virsmu gruntēšana","m2",60.2,{"$nulls":5},0,0,0,null,0,0]
[991,"grunts","l",9,{"$nulls":5},0,null,null,0,null,0]
[992,"Sienu virsmu špaktelēšana","m2",60.2,{"$nulls":5},0,0,0,null,0,0]
[993,"špaktele","kg",72,{"$nulls":5},0,null,null,0,null,0]
[994,"gatavā špakteļmasa","kg",96.32,{"$nulls":5},0,null,null,0,null,0]
[995,"Sienu virsmu krāsošana","m2",60.2,{"$nulls":5},0,0,0,null,0,0]
[996,"grunts","l",9,{"$nulls":5},0,null,null,0,null,0]
[997,"krāsa tonēta","l",20,{"$nulls":5},0,null,null,0,null,0]
[998,"Radiatoru krāsošana","gb",2,{"$nulls":5},0,0,0,null,0,0]
[999,"krāsa radiatoriem","l",1.8,{"$nulls":5},0,null,null,0,null,0]
[1000,"Gaismas ķermeņu noņemšana","gb",6,{"$nulls":5},0,0,0,null,0,0]
[1001,"Elektroinstalācijas montāža","m",37,{"$nulls":5},0,0,0,null,0,0]
[1002,"kabelis","m",37,{"$nulls":5},0,null,null,0,null,0]
[1003,"Slēdžu un kontaktu montāža","gb",7,{"$nulls":5},0,0,0,null,0,0]
[1004,"slēdzis ar montāžas kārbu","gb",1,{"$nulls":5},0,null,null,0,null,0]
[1005,"kontaktligzda ar montāžas kārbu","gb",6,{"$nulls":5},0,null,null,0,null,0]
[1006,"Gaismas ķermeņu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[1007,"dienasgaismas lampas","gb",6,{"$nulls":5},0,null,null,0,null,0]
[1008,"Ventilācijas restes montāža","gb",1,{"$nulls":5},0,0,0,null,0,0]
[1009,"ventilācijas reste","gb",1,{"$nulls":5},0,null,null,0,null,0]
[1010," MĀCĪBU TELPA NR.17 (2.ST)"]
[1011,"Dēļu grīdas klāja izjaukšana","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1012,"Dēļu grīdas gulšņu izjaukšana","m",24,{"$nulls":5},0,0,0,null,0,0]
[1013,"Būvgružu savākšana","m3",0.82,{"$nulls":5},0,0,0,null,0,0]
[1014,"Grīdas gulšņu uzstādīšana","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1015,"kokmateriāls","m3",0.24,{"$nulls":5},0,null,null,0,null,0]
[1016,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",14.3,{"$nulls":5},0,0,0,null,0,0]
[1017,"antiseptiķis","l",2.8,{"$nulls":5},0,null,null,0,null,0]
[1018,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1019,"skaņas izolācija 100 mm","m2",18.67,{"$nulls":5},0,null,null,0,null,0]
[1020,"Grīdas klāja-melnās grīdas ierīkošana ","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1021,"apzāģēti dēļi","m3",0.15,{"$nulls":5},0,null,null,0,null,0]
[1022,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1023,"spundēta plāksne 22 mm","m2",19.21,{"$nulls":5},0,null,null,0,null,0]
[1024,"skrūves","gb",275,{"$nulls":5},0,null,null,0,null,0]
[1025,"Grīdas virsmas gruntēšana","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1026,"grunts","l",5.5,{"$nulls":5},0,null,null,0,null,0]
[1027,"Linoleja ieklāšana pielīmējot visā platībā","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1028,"linolejs 34 klase","m2",19.21,{"$nulls":5},0,null,null,0,null,0]
[1029,"linoleja līme","kg",9.15,{"$nulls":5},0,null,null,0,null,0]
[1030,"šuvju kausēšanas diegs","m",5.1,{"$nulls":5},0,null,null,0,null,0]
[1031,"Koka grīdlīstu uzstādīšana","m",16,{"$nulls":5},0,0,0,null,0,0]
[1032,"koka grīdlīste,krāsota","m",17.6,{"$nulls":5},0,null,null,0,null,0]
[1033,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1034,"UD profils","m",18,{"$nulls":5},0,null,null,0,null,0]
[1035,"CD profils","m",40,{"$nulls":5},0,null,null,0,null,0]
[1036,"U veida skava","gb",20,{"$nulls":5},0,null,null,0,null,0]
[1037,"CD profilu savienotājs","gb",15,{"$nulls":5},0,null,null,0,null,0]
[1038,"CD profilu šķērssavienotājs","gb",18,{"$nulls":5},0,null,null,0,null,0]
[1039,"ģipškartons","m2",19.21,{"$nulls":5},0,null,null,0,null,0]
[1040,"apšuvuma skrūves","gb",275,{"$nulls":5},0,null,null,0,null,0]
[1041,"dībeļnaglas","gb",44,{"$nulls":5},0,null,null,0,null,0]
[1042,"Gipškartona šuvju špaktelēšana","m",23.5,{"$nulls":5},0,0,0,null,0,0]
[1043,"grunts","l",0.24,{"$nulls":5},0,null,null,0,null,0]
[1044,"špaktele","kg",5.87,{"$nulls":5},0,null,null,0,null,0]
[1045,"Griestu gruntēšana","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1046,"grunts","l",3.05,{"$nulls":5},0,null,null,0,null,0]
[1047,"Griestu krāsošana","m2",18.3,{"$nulls":5},0,0,0,null,0,0]
[1048,"krāsa","l",6.1,{"$nulls":5},0,null,null,0,null,0]
[1049,"Saplaisājušas un bojātas krāsas noņemšana","m2",11,{"$nulls":5},0,0,0,null,0,0]
[1050,"Sienu virsmu gruntēšana","m2",44.8,{"$nulls":5},0,0,0,null,0,0]
[1051,"grunts","l",6.72,{"$nulls":5},0,null,null,0,null,0]
[1052,"Sienu virsmu špaktelēšana","m2",44.8,{"$nulls":5},0,0,0,null,0,0]
[1053,"špaktele","kg",58,{"$nulls":5},0,null,null,0,null,0]
[1054,"gatavā špakteļmasa","kg",71.7,{"$nulls":5},0,null,null,0,null,0]
[1055,"Sienu virsmu krāsošana","m2",44.8,{"$nulls":5},0,0,0,null,0,0]
[1056,"grunts","l",6.72,{"$nulls":5},0,null,null,0,null,0]
[1057,"krāsa tonēta","l",14.9,{"$nulls":5},0,null,null,0,null,0]
[1058,"Radiatoru krāsošana","gb",1,{"$nulls":5},0,0,0,0,0,0]
[1059,"krāsa radiatoriem","l",0.9,{"$nulls":5},0,0,0,0,0,0]
[1060,"Gaismas ķermeņu noņemšana","gb",4,{"$nulls":5},0,0,0,null,0,0]
[1061,"Elektroinstalācijas montāža","m",27,{"$nulls":5},0,0,0,null,0,0]
[1062,"kabelis","m",27,{"$nulls":5},0,null,null,0,null,0]
[1063,"Slēdžu un kontaktu montāža","gb",7,{"$nulls":5},0,0,0,null,0,0]
[1064,"slēdzis ar montāžas kārbu","gb",1,{"$nulls":5},0,null,null,0,null,0]
[1065,"kontaktligzda ar montāžas kārbu","gb",6,{"$nulls":5},0,null,null,0,null,0]
[1066,"Gaismas ķermeņu montāža","gb",4,{"$nulls":5},0,0,0,null,0,0]
[1067,"gaismeklis","gb",4,{"$nulls":5},0,null,null,0,null,0]
[1068," MĀCĪBU TELPA NR.18 UN 19 (2.ST)"]
[1069,"Dēļu grīdas klāja izjaukšana","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1070,"Dēļu grīdas gulšņu izjaukšana","m",37,{"$nulls":5},0,0,0,null,0,0]
[1071,"Būvgružu savākšana","m3",0.88,{"$nulls":5},0,0,0,null,0,0]
[1072,"Grīdas gulšņu uzstādīšana","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1073,"kokmateriāls","m3",0.37,{"$nulls":5},0,null,null,0,null,0]
[1074,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1075,"antiseptiķis","l",2.9,{"$nulls":5},0,null,null,0,null,0]
[1076,"Siltumizolācijas ieklāšana uz grīdas starpklāja","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1077,"skaņas izolācija 100 mm","m2",14.89,{"$nulls":5},0,null,null,0,null,0]
[1078,"Grīdas klāja-melnās grīdas ierīkošana ","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1079,"apzāģēti dēļi","m3",0.24,{"$nulls":5},0,null,null,0,null,0]
[1080,"Grīdas klāja ierīkošana no kokskaidu plātnēm","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1081,"spundēta plāksne 22 mm","m2",15.33,{"$nulls":5},0,null,null,0,null,0]
[1082,"skrūves","gb",224,{"$nulls":5},0,null,null,0,null,0]
[1083,"Grīdas virsmas gruntēšana","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1084,"grunts","l",4.4,{"$nulls":5},0,null,null,0,null,0]
[1085,"Linoleja ieklāšana pielīmējot visā platībā","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1086,"linolejs 34 klase","m2",16.06,{"$nulls":5},0,null,null,0,null,0]
[1087,"linoleja līme","kg",7.3,{"$nulls":5},0,null,null,0,null,0]
[1088,"šuvju kausēšanas diegs","m",8,{"$nulls":5},0,null,null,0,null,0]
[1089,"Koka grīdlīstu uzstādīšana","m",17,{"$nulls":5},0,0,0,null,0,0]
[1090,"koka grīdlīste,krāsota","m",18.7,{"$nulls":5},0,null,null,0,null,0]
[1091,"Griestu apšūšana ar ģipškartona loksnēm,veidojot iekārtu divkārtu metāla profilu latojumu","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1092,"UD profils","m",17,{"$nulls":5},0,null,null,0,null,0]
[1093,"CD profils","m",60,{"$nulls":5},0,null,null,0,null,0]
[1094,"U veida skava","gb",22,{"$nulls":5},0,null,null,0,null,0]
[1095,"CD profilu savienotājs","gb",18,{"$nulls":5},0,null,null,0,null,0]
[1096,"CD profilu šķērssavienotājs","gb",16,{"$nulls":5},0,null,null,0,null,0]
[1097,"ģipškartons","m2",15.33,{"$nulls":5},0,null,null,0,null,0]
[1098,"apšuvuma skrūves","gb",220,{"$nulls":5},0,null,null,0,null,0]
[1099,"dībeļnaglas","gb",44,{"$nulls":5},0,null,null,0,null,0]
[1100,"Gipškartona šuvju špaktelēšana","m",19,{"$nulls":5},0,0,0,null,0,0]
[1101,"grunts","l",0.2,{"$nulls":5},0,null,null,0,null,0]
[1102,"špaktele","kg",4.75,{"$nulls":5},0,null,null,0,null,0]
[1103,"Griestu gruntēšana","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1104,"grunts","l",2.45,{"$nulls":5},0,null,null,0,null,0]
[1105,"Griestu krāsošana","m2",14.6,{"$nulls":5},0,0,0,null,0,0]
[1106,"krāsa","l",4.9,{"$nulls":5},0,null,null,0,null,0]
[1107,"Saplaisājušas un bojātas krāsas noņemšana","m2",14,{"$nulls":5},0,0,0,null,0,0]
[1108,"Sienu virsmu gruntēšana","m2",57,{"$nulls":5},0,0,0,null,0,0]
[1109,"grunts","l",8.55,{"$nulls":5},0,null,null,0,null,0]
[1110,"Sienu virsmu špaktelēšana","m2",45,{"$nulls":5},0,0,0,null,0,0]
[1111,"špaktele","kg",54,{"$nulls":5},0,null,null,0,null,0]
[1112,"gatavā špakteļmasa","kg",86.4,{"$nulls":5},0,null,null,0,null,0]
[1113,"Sienu virsmu krāsošana","m2",45,{"$nulls":5},0,0,0,null,0,0]
[1114,"grunts","l",6.75,{"$nulls":5},0,null,null,0,null,0]
[1115,"krāsa tonēta","l",15,{"$nulls":5},0,null,null,0,null,0]
[1116,"Radiatoru krāsošana","gb",2,{"$nulls":5},0,0,0,null,0,0]
[1117,"krāsa radiatoriem","l",1.8,{"$nulls":5},0,null,null,0,null,0]
[1118,"Sienu flīzēšana","m2",12,{"$nulls":5},0,0,0,null,0,0]
[1119,"sienu flīzes","m2",12.6,{"$nulls":5},0,null,null,0,null,0]
[1120,"flīžu līme","kg",60,{"$nulls":5},0,null,null,0,null,0]
[1121,"šuvju pildviela","kg",5,{"$nulls":5},0,null,null,0,null,0]
[1122,"Gaismas ķermeņu noņemšana","gb",2,{"$nulls":5},0,0,0,null,0,0]
[1123,"Elektroinstalācijas montāža","m",33,{"$nulls":5},0,0,0,null,0,0]
[1124,"kabelis","m",33,{"$nulls":5},0,null,null,0,null,0]
[1125,"Slēdžu un kontaktu montāža","gb",8,{"$nulls":5},0,0,0,null,0,0]
[1126,"slēdzis ar montāžas kārbu","gb",2,{"$nulls":5},0,null,null,0,null,0]
[1127,"kontaktligzda ar montāžas kārbu","gb",6,{"$nulls":5},0,null,null,0,null,0]
[1128,"Gaismas ķermeņu montāža","gb",6,{"$nulls":5},0,0,0,null,0,0]
[1129,"gaismeklis","gb",6,{"$nulls":5},0,null,null,0,null,0]
[1130," KORIDORS UN KĀPŅU LAUKUMS (2.ST)"]
[1131,"Koridora grīdas flīžu šuvju pildījuma atjaunošana","m2",28.3,{"$nulls":5},0,0,0,null,0,0]
[1132,"grunts","l",4.25,{"$nulls":5},0,null,null,0,null,0]
[1133,"šuvju pildviela","kg",14,{"$nulls":5},0,null,null,0,null,0]
[1134,"KĀPŅU TELPA"]
[1135,"Saplaisājušas un bojātas krāsas noņemšana","m2",35,{"$nulls":5},0,0,0,null,0,0]
[1136,"Sienu virsmu gruntēšana","m2",175,{"$nulls":5},0,0,0,null,0,0]
[1137,"grunts","l",26.25,{"$nulls":5},0,null,null,0,null,0]
[1138,"Sienu virsmu špaktelēšana","m2",175,{"$nulls":5},0,0,0,null,0,0]
[1139,"špaktele","kg",840,{"$nulls":5},0,null,null,0,null,0]
[1140,"gatavā špakteļmasa","kg",280,{"$nulls":5},0,null,null,0,null,0]
[1141,"Sienu virsmu krāsošana","m2",175,{"$nulls":5},0,0,0,null,0,0]
[1142,"grunts","l",26.25,{"$nulls":5},0,null,null,0,null,0]
[1143,"krāsa tonēta","l",58.3,{"$nulls":5},0,null,null,0,null,0]
[1144,"IEEJAS MEZGLA PIELĀGOŠANA CILVĒKIEM AR ĪPAŠĀM VAJADZĪBĀM"]
[1145,"Betona pakāpienu nojaukšana","m",12,{"$nulls":5},0,0,0,null,0,0]
[1146,"Betona laukuma nojaukšana","m2",4,{"$nulls":5},0,0,0,null,0,0]
[1147,"Būvgružu savākšana","m3",1.2,{"$nulls":5},0,0,0,null,0,0]
[1148,"Pakāpienu pamatojuma sagatavošana","m2",2.2,{"$nulls":5},0,0,0,null,0,0]
[1149,"betons izgatavots būvlaukumā","m3",0.4,{"$nulls":5},0,null,null,0,null,0]
[1150,"Kāpņu laukuma betonēšana","m3",0.6,{"$nulls":5},0,0,0,null,0,0]
[1151,"betons izgatavots būvlaukumā","m3",0.61,{"$nulls":5},0,null,null,0,null,0]
[1152,"stiegras diam.10 mm","m",20,{"$nulls":5},0,null,null,0,null,0]
[1153,"Kāpņu atbalsta sienu apmešana","m2",3.5,{"$nulls":5},0,0,0,null,0,0]
[1154,"apmetuma java","kg",46,{"$nulls":5},0,null,null,0,null,0]
[1155,"Gatavu pakāpienu uzstādīšana","gb",6,{"$nulls":5},0,0,0,null,0,0]
[1156,"betona pakāpieni","gb",6,{"$nulls":5},0,null,null,0,null,0]
[1157,"Melnzemes izņemšana","m2",4.8,{"$nulls":5},0,0,0,null,0,0]
[1158,"Pamata rakšana zem atbalsta sienas","m3",1.2,{"$nulls":5},0,0,0,null,0,0]
[1159,"Šķembu slāņa iestrādāšana","m3",0.24,{"$nulls":5},0,0,0,null,0,0]
[1160,"grants-šķembu maisījums","m3",0.26,{"$nulls":5},0,null,null,0,null,0]
[1161,"Veidņu uzstādīšana pamatu pēdai","m2",3.2,{"$nulls":5},0,0,0,null,0,0]
[1162,"veidņu materiāls","m2",3.52,{"$nulls":5},0,null,null,0,null,0]
[1163,"Pamata pēdas betonēšana","m3",0.64,{"$nulls":5},0,0,0,null,0,0]
[1164,"betons izgatavots būvlaukumā","m3",0.65,{"$nulls":5},0,null,null,0,null,0]
[1165,"stiegras diam.10 mm","m",16,{"$nulls":5},0,null,null,0,null,0]
[1166,"Uzbrauktuves atbalsta sienas veidņošana","m2",3,{"$nulls":5},0,0,0,null,0,0]
[1167,"veidņu materiāls","m2",6,{"$nulls":5},0,null,null,0,null,0]
[1168,"Atbalsta sienas betonēšana","m3",1.41,{"$nulls":5},0,0,0,null,0,0]
[1169,"betons izgatavots būvlaukumā","m3",1.44,{"$nulls":5},0,null,null,0,null,0]
[1170,"stiegras diam.10 mm","m",24,{"$nulls":5},0,null,null,0,null,0]
[1171,"Uzbrauktuves slīpuma veidošana","m2",4.8,{"$nulls":5},0,0,0,null,0,0]
[1172,"smilts-grants maisījums","m3",3.17,{"$nulls":5},0,null,null,0,null,0]
[1173,"mazgāta smilts","m3",0.58,{"$nulls":5},0,null,null,0,null,0]
[1174,"Bruģa  seguma ieklāšana","m2",4.8,{"$nulls":5},0,0,0,null,0,0]
[1175,"bruģakmens h=6cm","m2",5.04,{"$nulls":5},0,null,null,0,null,0]
[1176,"Atbalsta margu uzstādīšana","m",24,{"$nulls":5},0,0,0,null,0,0]
[1177,"metāla caurule diam.32 mm","m",26,{"$nulls":5},0,null,null,0,null,0]
[1178,"stiprinājumi","gb",15,{"$nulls":5},0,null,null,0,null,0]
[1179,"Atbalsta margu krāsošana","m",24,{"$nulls":5},0,0,0,null,0,0]
[1180,"Hammerit krāsa","l",0.75,{"$nulls":5},0,null,null,0,null,0]
[1181,"Durvju zvana uzstādīšana","gb",1,{"$nulls":5},0,0,0,null,0,0]
[1182,"duurvju zvans","gb",1,{"$nulls":5},0,null,null,0,null,0]
[1183,"instalācijas materiāli","kompl.",1,{"$nulls":5},0,null,null,0,null,0]
[1184,"2. STĀVA GRIESTU PĀRSEGUMA SILTINĀŠANA"]
[1185,"Starpsiju dēļu klāja apšuvuma nomaiņa","m2",115.5,{"$nulls":5},0,0,0,null,0,0]
[1186,"apzāģēti dēļi","m3",3.85,{"$nulls":5},0,null,null,0,null,0]
[1187,"Būvgružu savākšana","m3",3.49,{"$nulls":5},0,0,0,null,0,0]
[1188,"Koka virsmu antiseptēšana,uzklājot ar otu","m2",140,{"$nulls":5},0,0,0,null,0,0]
[1189,"antiseptiķis","l",30,{"$nulls":5},0,null,null,0,null,0]
[1190,"Pārseguma siltināšana ar siltumizolācijas plāksnēm","m2",270,{"$nulls":5},0,0,0,null,0,0]
[1191," izolācija 150 mm","m2",275.4,{"$nulls":5},0,null,null,0,null,0]
[1192,"Vēja izolācijas plākšņu uzklāšana","m2",270,{"$nulls":5},0,0,0,null,0,0]
[1193,"vēja izolācijas plāksne 30 mm","m2",275.4,{"$nulls":5},0,null,null,0,null,0]
[1194,"Koka laipu izbūve bēniņos","m2",67.5,{"$nulls":5},0,0,0,null,0,0]
[1195,"apzāģēti dēļi","m3",0.38,{"$nulls":5},0,null,null,0,null,0]
[null,"Kopā:"]
[null,"Transporta un sagādes izdevumi 8%",{"$nulls":12},0]
[null,"Kopā:",{"$nulls":12},0]
[null,"Neparedzētie darbi un izdevumi 4%",{"$nulls":12},0]
[null,"Virsizdevumi 6%",{"$nulls":12},0]
[null,"Plānotā peļņa 4%",{"$nulls":12},0]
[null,"Sociālais nodoklis 24,09%",{"$nulls":12},0]
[null,"Kopā bez PVN",{"$nulls":12},0]
[null,"PVN 21%",{"$nulls":12},0]
[null,"Kopā ar PVN",{"$nulls":12},0]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}