{"text_format":"2","workbook":"xls","n_sheets":17,"sheets":["Kopā","Savilkums","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Kopā","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[[7,0,7,4],[15,2,16,3],[17,2,17,3],[17,0,17,1],[15,0,16,1],[15,4,16,4]],"flags":["formulas_cached_only"]}
[null,null,"APSTIPRINU:"]
[]
[{"$nulls":4},"/______________/___________________/"]
[null,null,null,"             Paraksts                             atšifrējums"]
[{"$nulls":4},"z.v."]
[{"$nulls":4},"2010. g. \"_____  \"________________"]
[]
["Būvniecības koptāme"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[]
[null,null,"Cilvēkstundas: ",null,0]
[null,null,"Tāme sastādīta:",null,0]
["Tāmes nr.",null,"Tāmes nosaukums",null,"Izmaksas BEZ PVN 21% Ls"]
[]
["1",null,"Tautas nama vienkāršotā rekonstrukcija",null,0]
[null,null,null,"Kopā bez PVN Ls:",0]
[null,null,null,"PVN 21% Ls:",0]
[null,null,null,"Kopā ar PVN Ls:",0]

{"sheet":"Savilkums","index":1,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[[6,0,6,7],[16,0,16,1],[14,0,15,1],[14,2,15,2],[14,3,15,3],[17,0,17,1],[18,0,18,1],[19,0,19,1],[20,0,20,1],[14,4,15,4],[14,5,14,7],[29,0,29,1],[30,0,30,1],[21,0,21,1],[22,0,22,1],[23,0,23,1],[24,0,24,1],[25,0,25,1],[26,0,26,1],[27,0,27,1],[28,0,28,1]],"flags":["formulas_cached_only"]}
[{"$nulls":5},"APSTIPRINU:"]
[]
[{"$nulls":5},"/______________/___________________/"]
[{"$nulls":5},"     Paraksts                             atšifrējums"]
[{"$nulls":7},"z.v."]
[{"$nulls":5},"2010. g.","\"_____  \"________________"]
["Kopsavilkums"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[]
[null,null,"Cilvēkstundas: ",0]
[null,null,"Tāme sastādīta:"]
["Tāmes nr.",null,"Tāmes nosaukums","Tiešās izmaksas BEZ PVN 21% Ls","Darba ietilpība C/st","Kopējās izmaksas, tai skaitā"]
[{"$nulls":5},"Dalba alga Ls","Materiāli Ls","Mehanismi Ls"]
["1",null,"Jumta seguma rekontsrukcija",0,0,0,0,0]
[2,null,"Zāles priekštelpa",0,0,0,0,0]
[3,null,"Zāle",0,0,0,0,0]
[4,null,"Aktieru telpas",0,0,0,0,0]
[5,null,"Invalīdu uzbrauktuve, bruģis",0,0,0,0,0]
[6,null,"Invalīdu tualete",0,0,0,0,0]
[7,null,"Invalīdu tualetes aprīkojums",0,0,0,0,0]
[8,null,"Mūzikas skola",0,0,0,0,0]
[9,null,"UAS izbūve",0,0,0,0,0]
[10,null,"Apsardzes sistēma",0,0,0,0,0]
[11,null,"Elektromontāžas darbi",0,0,0,0,0]
[12,null,"Zibens aizsardzība",0,0,0,0,0]
[13,null,"Katlu māja",0,0,0,0,0]
[14,null,"Apkures sistēmas izbūve",0,0,0,0,0]
[15,null,"Ventilācijas sistēma",0,0,0,0,0]
[null,null,"Tiešās izmaksas kopā Ls:",0,0,0,0,0]
[null,null,"Materiālu sagāde, transports ...% Ls:"]
[null,null,"Uzņēmuma virsizdevumi ...% Ls:"]
[null,null,"Plānotie uzkrājumi ...% Ls:"]
[null,null,"Neparedzētie izdevumi 4% Ls:"]
[null,null,"Darba devēja sociālais nodoklis 24.09% Ls:",0]
[null,null,"Kopā bez PVN 21% Ls:",0]

{"sheet":"1","index":2,"n_rows":76,"n_cols":17,"rows_kept":76,"cut":false,"hidden":false,"merged":[[0,0,0,15],[1,0,1,15],[7,11,7,12],[8,0,8,2],[8,11,8,12],[6,11,6,12],[73,0,73,4],[9,7,9,10],[9,16,12,16],[10,7,10,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 1"]
["Jumta seguma rekontsrukcija",{"$nulls":15},"Jumta seguma rekontsrukcija"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"11-81","Jumta seguma, noteksistēmas demontāža, saglabājot",{"$nulls":4},0,null,null,0,0,0,0,0,0]
[2,null,"apakšējo dēļu klāju","m2",977,null,null,0,null,null,0,0,0,0,0,0]
[3,"5-72","Antikondensāta plēves ieklāšana","m2",977,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Jutacom 130","m2","1180",null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Skavas","kompl","2",null,null,0,null,null,0,0,0,0,0,0]
[6,"6-80","Dubultais latojums uz dēļu klāja  seguma","m2",977,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Antiseptizētas līstes 28 x 100","m3","13,4",null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Naglas 75 mm","kg",60,null,null,0,null,null,0,0,0,0,0,0]
[9,"5-27","Jumta seguma ieklāšana","m2",977,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Dakstiņveida profils PE 0,45mm","m2",1110,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"jumta skrūve ar bīvgumiju","gb",7800,null,null,0,null,null,0,0,0,0,0,0]
[12,"5-60","Jumta kores uzstādīšana","t.m.",69,null,null,0,null,null,0,0,0,0,0,0]
[13,null,"Kore PE ","t.m.",76,null,null,0,null,null,0,0,0,0,0,0]
[14,null,"jumta skrūve ar bīvgumiju","gb",550,null,null,0,null,null,0,0,0,0,0,0]
[15,"5-60","karnīzes uzstādīšana","t.m.",97,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"Karnīze PE","t.m.",106,null,null,0,null,null,0,0,0,0,0,0]
[17,"5-60","Pieslēgums mūra sienai","t.m.",19,null,null,0,null,null,0,0,0,0,0,0]
[18,null,"Atloks PE","t.m.",23,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"jumta skrūve ar bīvgumiju","gb",90,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"Dībeļi","gb",90,null,null,0,null,null,0,0,0,0,0,0]
[21,"5-60","Sateces uzstādīšana","t.m.",45.5,null,null,0,null,null,0,0,0,0,0,0]
[22,null,"Sateka PE","t.m.",50,null,null,0,null,null,0,0,0,0,0,0]
[23,null,"jumta skrūve ar bīvgumiju","gb.",300,null,null,0,null,null,0,0,0,0,0,0]
[24,"5-60","Sniega aiztures uzstādīšana","t.m.",8,null,null,0,null,null,0,0,0,0,0,0]
[25,null,"Sateka PE","t.m.",8,null,null,0,null,null,0,0,0,0,0,0]
[26,null,"jumta skrūve ar bīvgumiju","gb.",96,null,null,0,null,null,0,0,0,0,0,0]
[27,"Normat.","Vēja dēļa uzstādīšana","t.m.",74,null,null,0,null,null,0,0,0,0,0,0]
[28,null,"Krāsots dēlis PE","t.m.",82,null,null,0,null,null,0,0,0,0,0,0]
[29,null,"Skārda vējdēlis","t.m.",82,null,null,0,null,null,0,0,0,0,0,0]
[30,null,"jumta skrūve ar bīvgumiju","gb.",320,null,null,0,null,null,0,0,0,0,0,0]
[31,"Normat.","Jumta lūkas uzstād.un iestrāde ar skārdu","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[32,null,"Jumta lūka PE ovāla","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[33,null,"jumta skrūve ar bīvgumiju","gb.",30,null,null,0,null,null,0,0,0,0,0,0]
[34,null,"Silikons","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[35,"Normat.","Skursteņu iestrāde ar ruļļu skārdu","m",19.2,null,null,0,null,null,0,0,0,0,0,0]
[36,null,"Skārds PE","m2",19.2,null,null,0,null,null,0,0,0,0,0,0]
[37,null,"jumta skrūve ar bīvgumiju","gb",130,null,null,0,null,null,0,0,0,0,0,0]
[38,null,"Dībeļi","gb",65,null,null,0,null,null,0,0,0,0,0,0]
[39,null,"Silikons","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[40,"Normat.","Lietusūdens notekrenes montāža","m",97.4,null,null,0,null,null,0,0,0,0,0,0]
[41,null,"PE skārda apaļā rene dm115","m",106,null,null,0,null,null,0,0,0,0,0,0]
[42,null,"PE cietie gali","gb",14,null,null,0,null,null,0,0,0,0,0,0]
[43,null,"teknes āķis","gb",126,null,null,0,null,null,0,0,0,0,0,0]
[44,null,"PE stūris iekšējais","gb",4,null,null,0,null,null,0,0,0,0,0,0]
[45,null,"PE piltuves","gb",11,null,null,0,null,null,0,0,0,0,0,0]
[46,"Normat.","Lietusūdens notekcaurules montāža","m",33,null,null,0,null,null,0,0,0,0,0,0]
[47,null,"PE skārda apaļā caurule dm89","m",36,null,null,0,null,null,0,0,0,0,0,0]
[48,null,"PE līkumu komplekti- augšējie","kpl",11,null,null,0,null,null,0,0,0,0,0,0]
[49,null,"PE iztece","gb",11,null,null,0,null,null,0,0,0,0,0,0]
[50,null,"aptveres, dībelis 10*80","gb",38,null,null,0,null,null,0,0,0,0,0,0]
[51,"Normat.","Pārkares krāsojums ar toni 2x","m2",85.5,null,null,0,null,null,0,0,0,0,0,0]
[52,null,"Villa aqua","litri",25,null,null,0,null,null,0,0,0,0,0,0]
[53,null,"tonēšana","litri",25,null,null,0,null,null,0,0,0,0,0,0]
[54,"Normat.","Bēniņu pārseguma dēļu seguma nomaiņa","m2",4,null,null,0,null,null,0,0,0,0,0,0]
[55,null,"Kokmateriāli","m3",0.1,null,null,0,null,null,0,0,0,0,0,0]
[56,"Normat.","Akmens vates siltinājums 5cm + 5cm","m2",566,null,null,0,null,null,0,0,0,0,0,0]
[57,null,"Akmens vate  \"Isover\"","m3",59.45,null,null,0,null,null,0,0,0,0,0,0]
[58,"Normat.","Būvgruži- azbestcementa- debonēšana","tn",5,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"2","index":3,"n_rows":42,"n_cols":17,"rows_kept":42,"cut":false,"hidden":false,"merged":[[8,0,8,2],[9,7,9,10],[9,16,12,16],[10,7,10,10],[9,12,9,15],[10,12,10,15],[39,0,39,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 2"]
["Zāles priekštelpa",{"$nulls":15},"Zāles priekštelpa"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Demontēt logus, t.p. uzstādīt, ārējā 30cm, iekšējā  40cm palodzes montāža","gb.",4,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"PVC logs ar vērtni balts/balts 800*600","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"PVC logs  balts/balts 800*600","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"ārējā palodze PE 30cm","m",3.2,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"iekšējā palodze 40cm","m",3.2,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Palīgmateriāli","kompl",4,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Logu ailu apdare, krāsojums","m2",3.5,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Knauf GKBI","m2",4.2,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Vetonit LR","kg",9,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Krāsa \"Bindo 20\" ar toni","ltri",1,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[10,"Normat.","Krāsot ārdurvis","m2",6.4,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"Krāsa","li",2,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Demontēt vecos griestus","m2",109.9,null,null,0,null,null,0,0,0,0,0,0]
[14,"Normat.","Iekārtie griesti 600 x 600 mm","m2",109.9,null,null,0,null,null,0,0,0,0,0,0]
[15,null,"mitrumizturīgas plātnes 600 x 600 x 12 mm","m2",120.9,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"Nesošā līste 3,6m","gb.",30,null,null,0,null,null,0,0,0,0,0,0]
[17,null,"Perimetra līste 3m","gb.",32,null,null,0,null,null,0,0,0,0,0,0]
[18,null,"Šķērslīste 1,2m","gb.",160,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"Šķērslīste 0,6m","gb.",176,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"Dībeļi","gb.",220,null,null,0,null,null,0,0,0,0,0,0]
[21,null,"Piekāršanas komplekts 30cm, metāla dībeļnagla","gb.",88,null,null,0,null,null,0,0,0,0,0,0]
[22,"Normat.","Būvgruži","tn",0.4,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"3","index":4,"n_rows":65,"n_cols":17,"rows_kept":65,"cut":false,"hidden":false,"merged":[[9,16,12,16],[9,7,9,10],[10,7,10,10],[62,0,62,4],[9,12,9,15],[10,12,10,15],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 3"]
["Zāle",{"$nulls":15},"Zāle"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Demontēt logus, t.p. uzstādīt, ārējā 30cm, iekšējā  40cm palodzes montāža","gb.",11,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"PVC logs ar vērtni balts/balts 800*1900","gb.",4,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"PVC logs  balts/balts 800*1900","gb.",7,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"ārējā palodze PE 30cm","m",10,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"iekšējā palodze 40cm","m",10,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Palīgmateriāli","kompl",11,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Logu ailu apdare, krāsojums","m2",20.2,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Knauf GKBI","m2",24.3,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Vetonit LR","kg",48.6,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Krāsa \"Bindo 20\" ar toni","ltri",6,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[10,"Normat.","Durvju demontāža, uzstādīšana","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"PVC fasādes divviru durvis balts/balts 1400*2600","kpl",1,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Ailu apdare durvīm","m2",1.8,null,null,0,null,null,0,0,0,0,0,0]
[13,null,"Knauf GKBI","m2",2,null,null,0,null,null,0,0,0,0,0,0]
[14,"Normat.","Dekoratīvā paneļa demontāža","m2",92,null,null,0,null,null,0,0,0,0,0,0]
[15,null,"Caurumu aizdare ar \"Rotband\"","kg",150,null,null,0,null,null,0,0,0,0,0,0]
[16,"Normat.","Sienu attīrīt, gruntēt, špaktelēt 2 x","m2",225,null,null,0,null,null,0,0,0,0,0,0]
[17,null,"Izkalt rievas, aizdarīt ar sietu, 2 x krāsot","t.m.",42,null,null,0,null,null,0,0,0,0,0,0]
[18,null,"Siets","m2",7,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"Līmjava \"Perflix\"","maisi",2,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"\"Tiefgrund\" LF","li",100,null,null,0,null,null,0,0,0,0,0,0]
[21,null,"Vetonit LR","kg.",150,null,null,0,null,null,0,0,0,0,0,0]
[22,null,"Smilšpapīrs","m",50,null,null,0,null,null,0,0,0,0,0,0]
[23,null,"Krāsotāja lenta","gb.",20,null,null,0,null,null,0,0,0,0,0,0]
[24,null,"Hermētiķis","gb.",5,null,null,0,null,null,0,0,0,0,0,0]
[25,null,"Grunts \"Bindo\"","li",40,null,null,0,null,null,0,0,0,0,0,0]
[26,null,"Krāsa \"Bindo 20\" ar toni","li",40,null,null,0,null,null,0,0,0,0,0,0]
[27,"Normat.","Griestu attīrīšana no krāsas","m2",290,null,null,0,null,null,0,0,0,0,0,0]
[28,"Normat.","Rievu apdare ar sietu","m",50,null,null,0,null,null,0,0,0,0,0,0]
[29,null,"Siets","m2",8,null,null,0,null,null,0,0,0,0,0,0]
[30,null,"Līmjava \"Perflix\"","maisi",2,null,null,0,null,null,0,0,0,0,0,0]
[31,"Normat.","Griestus gruntēt, špaktelēt 2x, krāsot 2x","m2",290,null,null,0,null,null,0,0,0,0,0,0]
[32,null,"Tiefgrund LF","li",110,null,null,0,null,null,0,0,0,0,0,0]
[33,null,"Vetonit LR","kg",160,null,null,0,null,null,0,0,0,0,0,0]
[34,null,"Smilšpapīrs","m",60,null,null,0,null,null,0,0,0,0,0,0]
[35,null,"Hermētiķis","gb.",6,null,null,0,null,null,0,0,0,0,0,0]
[36,null,"Krāsotāja lenta","gb.",10,null,null,0,null,null,0,0,0,0,0,0]
[37,null,"Aizsargplēve","m2",50,null,null,0,null,null,0,0,0,0,0,0]
[38,null,"Aizsargplēve grīdām","m2",270,null,null,0,null,null,0,0,0,0,0,0]
[39,null,"Grunts \"Bindo\"","li",40,null,null,0,null,null,0,0,0,0,0,0]
[40,null,"Krāsa \"Bindo 7\"","li",40,null,null,0,null,null,0,0,0,0,0,0]
[41,"Normat.","Kājlīstu izgatav., krāsoš.,uzstād.   H=20cm","t.m.",62,null,null,0,null,null,0,0,0,0,0,0]
[42,null,"kok akājlīste, stiprinājumi, krāsojums","m",68,null,null,0,null,null,0,0,0,0,0,0]
[43,"Normat.","Sastatņu montāža, demontāža","100m2",2.9,null,null,0,null,null,0,0,0,0,0,0]
[44,null,"Sastaņu noma","m2",290,null,null,0,null,null,0,0,0,0,0,0]
[45,"Normat.","Būvgružu savākšana","to",2.3,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"4","index":5,"n_rows":45,"n_cols":17,"rows_kept":45,"cut":false,"hidden":false,"merged":[[42,0,42,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 4"]
["Aktieru telpas",{"$nulls":15},"Aktieru telpas"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Demontēt koka grīdu, lāgas","m2",12,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Izbūvēt OSB grīdu un koka lāgām, siltinājums","m2",12,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"OSB 22 mm (spundēts)","m2",13,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Kokmateriāli","m3",0.3,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Keramzīts 8-20mm","m3",1.2,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Betons B15","m3",0.6,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"ruberoīds","m2",8,null,null,0,null,null,0,0,0,0,0,0]
[8,"Normat.","Ieklāt linoleju","m2",12,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Līme Farbo","kg",3,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"PVC linolejs PUR pārklājums","m2",13,null,null,0,null,null,0,0,0,0,0,0]
[11,"Normat.","Kājlīstu montāža","m",16,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Kājlīstes","m",17,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Demontēt logus, t.p. uzstādīt, ārējā 30cm, iekšējā  40cm palodzes montāža","gb.",3,null,null,0,null,null,0,0,0,0,0,0]
[14,null,"PVC logs ar vērtni balts/balts 600*1900","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[15,null,"PVC logs  balts/balts 600*1900","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[15,null,"ārējā palodze PE 30cm","m",2.1,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"iekšējā palodze 40cm","m",2.1,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"Palīgmateriāli","kompl",3,null,null,0,null,null,0,0,0,0,0,0]
[17,"Normat.","Logu ailu apdare, krāsojums","m2",4.6,null,null,0,null,null,0,0,0,0,0,0]
[18,null,"Knauf GKBI","m2",5.5,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"Vetonit LR","kg",10,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"krāsa \"Vivaplast 20\" (tonis - Tikkurila Symphony Opus II F488) vai analogs","ltri",1.5,null,null,0,null,null,0,0,0,0,0,0]
[21,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[22,"Normat.","Krāsot ārdurvis","m2",13.5,null,null,0,null,null,0,0,0,0,0,0]
[23,null,"Krāsa kokam","litri",4,null,null,0,null,null,0,0,0,0,0,0]
[24,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[25,"Normat.","Būvgruži","tn",0.5,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"5","index":6,"n_rows":31,"n_cols":17,"rows_kept":31,"cut":false,"hidden":false,"merged":[[28,0,28,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 5"]
["Invalīdu uzbrauktuve, bruģis",{"$nulls":15},"Invalīdu uzbrauktuve, bruģis"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Demontēt  betona plāksnes","m2",10,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Ierīkot bruģi 60 mm un šķambu pamatojuma","m2",10,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Bruģis pelēks 60mm","m2",10.5,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"šķembas 15/32","m3",2,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Smilts 0-4mm","m3",2,null,null,0,null,null,0,0,0,0,0,0]
[6,"Normat.","Betona apmaļu uzstādīšana","m",10,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Betona apmales 80*200*1000","gb",10,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Betons B15","m3",0.5,null,null,0,null,null,0,0,0,0,0,0]
[9,"Normat.","Uzbrauktuves margu uzstādīsana","m",8.5,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"tērauda stabi dm60, krāsoti","gb",10,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"tērauda  dm50 marga, reliņi 3joslās","m",8.5,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Betons B15","m3",0.5,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Būvgružu savākšana","tn",2.2,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"6","index":7,"n_rows":87,"n_cols":17,"rows_kept":87,"cut":false,"hidden":false,"merged":[[84,0,84,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 6"]
["Invalīdu tualete",{"$nulls":15},"Invalīdu tualete"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Demontēt ķieģeļu sienas 25cm","m2",8,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Iebūvēt pārsedzi","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Pārsedze 2*U20, piebetonēta, apmesta ar javu","m",1.6,null,null,0,null,null,0,0,0,0,0,0]
[4,"Normat.","Izzāģēt grīdā šahtas, izkalt un iebet.pam.","t.m.",3.8,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Betons B15","m3",0.5,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Armatūra dm12","m",10,null,null,0,null,null,0,0,0,0,0,0]
[7,"Normat.","1/2 ķieģeļu mūris","m2",11,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Ķieģeļi 65mm","gb.",550,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Mūrjava","m3",0.35,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Pārsedze 100*185*1490","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[11,"Normat.","Apmetums","m2",22,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"\"Rotband\"","kg",616,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Apmetuma špaktelēšana","m2",22,null,null,0,null,null,0,0,0,0,0,0]
[14,null,"Vetonit LR","kg",44,null,null,0,null,null,0,0,0,0,0,0]
[15,"Normat.","Krāsot 2x","m2",15,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"Krāsa \"Bindo\"","li",5,null,null,0,null,null,0,0,0,0,0,0]
[17,null,"Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[18,"Normat.","Iekārtie griesti 600 x 600 mm","m2",5.3,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"mitrumizturīgas plātnes 600 x 600 x 12 mm","m2",5.8,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"Nesošā līste 3,6m","gb.",1.5,null,null,0,null,null,0,0,0,0,0,0]
[21,null,"Perimetra līste 3m","gb.",1.5,null,null,0,null,null,0,0,0,0,0,0]
[22,null,"Šķērslīste 1,2m","gb.",7,null,null,0,null,null,0,0,0,0,0,0]
[23,null,"Šķērslīste 0,6m","gb.",9,null,null,0,null,null,0,0,0,0,0,0]
[24,null,"Dībeļi","gb.",12,null,null,0,null,null,0,0,0,0,0,0]
[25,null,"Piekāršanas komplekts 30cm, metāla dībeļnagla","gb.",4,null,null,0,null,null,0,0,0,0,0,0]
[26,"Normat.","Sienu flīzēšana","m2",18,null,null,0,null,null,0,0,0,0,0,0]
[27,null,"Flīzes keramiskās 20*30cm","m2",19,null,null,0,null,null,0,0,0,0,0,0]
[28,null,"Flīžu līme","kg",50,null,null,0,null,null,0,0,0,0,0,0]
[29,null,"Šuvju pildviela","kg",4.5,null,null,0,null,null,0,0,0,0,0,0]
[30,"Normat.","Grīdas grunts, izlīdzināšana, flīzēšana","m2",4.9,null,null,0,null,null,0,0,0,0,0,0]
[31,null,"grunts","litri",2,null,null,0,null,null,0,0,0,0,0,0]
[32,null,"izlīdzinātājs","kg",150,null,null,0,null,null,0,0,0,0,0,0]
[33,null,"Flīzes 30*30cm akmens masas","m2",5.6,null,null,0,null,null,0,0,0,0,0,0]
[34,null,"Līme","kg",30,null,null,0,null,null,0,0,0,0,0,0]
[35,null,"Šuvju mastika","kg",2,null,null,0,null,null,0,0,0,0,0,0]
[36,"Normat.","Durvju montāža","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[37,null,"Durvis 1200 x 2100 mm koka, furnitūra, apdare","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[38,null,"Kleidu komplekts","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[39,null,"Montāžas putas","bal.",0.5,null,null,0,null,null,0,0,0,0,0,0]
[40,null,"Stiprinājumi","gb.",6,null,null,0,null,null,0,0,0,0,0,0]
[41,"Normat.","Izzāģēt, izkalt grīdu kanaliz.izbūvēšanai","t.m.",4,null,null,0,null,null,0,0,0,0,0,0]
[42,null,"Aizbetonēt šahtu","m",4,null,null,0,null,null,0,0,0,0,0,0]
[43,null,"Betons B15","m3",0.1,null,null,0,null,null,0,0,0,0,0,0]
[44,"Normat.","Izbūvēt reģ.sienu ar 2-kāršu reģ.iesegumu","m2",2.5,null,null,0,null,null,0,0,0,0,0,0]
[45,null,"UW100","m",8,null,null,0,null,null,0,0,0,0,0,0]
[46,null,"CW100","m",3,null,null,0,null,null,0,0,0,0,0,0]
[47,null,"amortizācijas lenta 9,5cm","m",8,null,null,0,null,null,0,0,0,0,0,0]
[48,null,"dībeļnagla 6*50mm","gb",20,null,null,0,null,null,0,0,0,0,0,0]
[49,null,"montāžas skrūves","gb",10,null,null,0,null,null,0,0,0,0,0,0]
[50,null,"minerālvate 10cm loksnēs","m",2.8,null,null,0,null,null,0,0,0,0,0,0]
[51,null,"reģipsis GKBI","m2",12,null,null,0,null,null,0,0,0,0,0,0]
[52,null,"skrūves reģipsism","gb",180,null,null,0,null,null,0,0,0,0,0,0]
[53,null,"dziļumgrunts","litri",2,null,null,0,null,null,0,0,0,0,0,0]
[54,null,"Unifloat","kg",10,null,null,0,null,null,0,0,0,0,0,0]
[55,null,"sietiņlenta","m",5,null,null,0,null,null,0,0,0,0,0,0]
[56,"Normat.","Reģipša sienu virsmu sagatavošana krāsošanai (grunts, špaktelēšana, gruntēšana u.c.)","m2",5,null,null,0,null,null,0,0,0,0,0,0]
[57,null,"dziļumgrunts","litri",0.6,null,null,0,null,null,0,0,0,0,0,0]
[58,null,"špaktele- nobeiguma","kg",9,null,null,0,null,null,0,0,0,0,0,0]
[59,"Normat.","Sienu krāsošana","m2",5,null,null,0,null,null,0,0,0,0,0,0]
[60,null,"Krāsa \"Bindo 20\" ar toni","litri",2,null,null,0,null,null,0,0,0,0,0,0]
[61,null,"palīgmateriāli (krāsotāju lente u.c.)","kpl",1,null,null,0,null,null,0,0,0,0,0,0]
[62,"Normat.","Nokalt flīžu grīdu WC","m2",6,null,null,0,null,null,0,0,0,0,0,0]
[63,"Normat.","Grīdas grunts, izlīdzināšana, flīzēšana","m2",6,null,null,0,null,null,0,0,0,0,0,0]
[64,null,"grunts","litri",2.4,null,null,0,null,null,0,0,0,0,0,0]
[65,null,"izlīdzinātājs","kg",200,null,null,0,null,null,0,0,0,0,0,0]
[66,null,"Flīzes 30*30cm akmens masas","m2",6.9,null,null,0,null,null,0,0,0,0,0,0]
[67,null,"Līme","kg",36,null,null,0,null,null,0,0,0,0,0,0]
[68,null,"Šuvju mastika","kg",2.5,null,null,0,null,null,0,0,0,0,0,0]
[69,"Normat.","Būvgruži","tn",5.5,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"7","index":8,"n_rows":44,"n_cols":17,"rows_kept":44,"cut":false,"hidden":false,"merged":[[41,0,41,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 7"]
["Invalīdu tualetes aprīkojums",{"$nulls":15},"Invalīdu tualetes aprīkojums"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Klozetpoda montāža ar lokano šļūteni,","gb",1,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Izlietne 480x230mm Kolo Nova Top Pico 61250 (Polija) komplektā ar jaucēkrānu, sifonu vai analogs","gb",1,null,null,0,null,null,0,0,0,0,0,0]
[3,"Normat.","Plastmasas kanalizācijas caurules PP «Uponor» Ø110","m",4,null,null,0,null,null,0,0,0,0,0,0]
[4,"Normat.","Revīzija ar vāku Ø110","gb",1,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Fasondaļas. Stiprinājuma tipu un veidgabalu","kpl.",1,null,null,0,null,null,0,0,0,0,0,0]
[6,"Normat.","Daudzslāņu caurules 25x2.5","m",12,null,null,0,null,null,0,0,0,0,0,0]
[7,"Normat.","Daudzslāņu caurules 20x2.5","m",6,null,null,0,null,null,0,0,0,0,0,0]
[8,"Normat.","Pretkondensāta izolācija ar biezumu  9 mm 25/9-DG","m",12,null,null,0,null,null,0,0,0,0,0,0]
[9,"Normat.","Pretkondensāta izolācija ar biezumu  9 mm  20/9-DG","m",6,null,null,0,null,null,0,0,0,0,0,0]
[10,"Normat.","Lodveida ventilis DN20","gb.",3,null,null,0,null,null,0,0,0,0,0,0]
[11,"Normat.","Palīgmateriāli","kpl.",1,null,null,0,null,null,0,0,0,0,0,0]
[12,"Normat.","Cinkotais gaisa vads Ø100","m",6,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Cinkotais gaisa vads Ø100","m",4,null,null,0,null,null,0,0,0,0,0,0]
[14,"Normat.","Kanāla ventilatorsTD500/160, Nel.=0,05kW, 200Pa, ","kpl.",1,null,null,0,null,null,0,0,0,0,0,0]
[15,"Normat.","Ātruma regulators  REGUL l2 (Montēt jaunprojektējamā elektrosadalē)","kpl.",1,null,null,0,null,null,0,0,0,0,0,0]
[16,"Normat.","Gaisa vadu veidgabali, stiprinājumi","kpl.",1,null,null,0,null,null,0,0,0,0,0,0]
[17,"Normat.","Difozori dm100","gb",5,null,null,0,null,null,0,0,0,0,0,0]
[18,"Normat.","Caurumu kalšana sienā dm160","gb",1,null,null,0,null,null,0,0,0,0,0,0]
[19,"Normat.","Āra restes montāža 200*200","gb",1,null,null,0,null,null,0,0,0,0,0,0]
[20,"Normat.","Droseļvārsts Ø100","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[21,"Normat.","Droseļvārsts Ø125","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[22,"Normat.","sienas rokturis L=600mm /Kolo Basic L2100105 (Polija) vai analogs/","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[23,"Normat.","nolaižamais rokturis L=700mm /Kolo Basic L2161205 (Polija) vai analogs/","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[24,"Normat.","WC papīra turētājs","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[25,"Normat.","šķidro ziepju trauks","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[26,"Normat.","atkritumu spainis","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"8","index":9,"n_rows":26,"n_cols":17,"rows_kept":26,"cut":false,"hidden":false,"merged":[[23,0,23,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 8"]
["Mūzikas skola",{"$nulls":15},"Mūzikas skola"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Iekārto griestu izbūve","m2",30,null,null,0,null,null,0,0,0,0,0,0]
[2,null,"Planet SK 600 x 600 x 12 mm","m2",33,null,null,0,null,null,0,0,0,0,0,0]
[3,null,"Nesošā līste 3,6m","gb.",9,null,null,0,null,null,0,0,0,0,0,0]
[4,null,"Perimetra līste 3m","gb.",12,null,null,0,null,null,0,0,0,0,0,0]
[5,null,"Šķērslīste 1,2m","gb.",44,null,null,0,null,null,0,0,0,0,0,0]
[6,null,"Šķērslīste 0,6m","gb.",48,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Dībeļi","gb.",60,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Piekāršanas komplekts 30cm, metāla dībeļnagla","gb.",25,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"9","index":10,"n_rows":34,"n_cols":17,"rows_kept":34,"cut":false,"hidden":false,"merged":[[31,0,31,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 9"]
["UAS izbūve",{"$nulls":15},"UAS izbūve"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Paplašinātājs BENTEL","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Raidītājs ar antenu (GSM)","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[3,"Normat.","Dūmu detektors NB 338-2","gab",8,null,null,0,null,null,0,0,0,0,0,0]
[4,"Normat.","Termiskais detektors NB 323-2","gab",5,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Staru dūmu detektors C-9105R","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[6,"Normat.","Ugunsdrošības rokas signāldevējs","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[7,"Normat.","Sirēna LD-FS 100","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[8,"Normat.","Sirēna MR 300","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[9,"Normat.","Akumolātoru baterijas ","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[10,"Normat.","Kabelis KLM 1x2x0,8","m",340,null,null,0,null,null,0,0,0,0,0,0]
[11,"Normat.","Kabelis Eurosafe 2x0,8","m",85,null,null,0,null,null,0,0,0,0,0,0]
[12,"Normat.","Kabeļu kanāls 9x18","m",85,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Aizsargrežģis staru dūmu det.","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[14,"Normat.","Palīgmateriāli","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[15,"Normat.","Iekārtas regulēšana, programēšana ","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[16,"Normat.","Nodošana ekspluatācijā","obj.",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"10","index":11,"n_rows":34,"n_cols":17,"rows_kept":34,"cut":false,"hidden":false,"merged":[[31,0,31,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 10"]
["Apsardzes sistēma",{"$nulls":15},"Apsardzes sistēma"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Kontroles panelis Cortex","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Zonu paplašinātājs","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[3,"Normat.","Raidītājs ar antenu (GSM)","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[4,"Normat.","Vadības pults","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Barošanas bloks PSU","gab",1,null,null,0,null,null,0,0,0,0,0,0]
[6,"Normat.","Kustību detektors RX-40","gab",16,null,null,0,null,null,0,0,0,0,0,0]
[7,"Normat.","Kustību detektors 360","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[8,"Normat.","Sirēna SEM 923","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[9,"Normat.","Stiklu plīšanas detektors GBD+","gab",9,null,null,0,null,null,0,0,0,0,0,0]
[10,"Normat.","Akumolātoru baterijas ","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[11,"Normat.","Kabelis 12x0,22","m",740,null,null,0,null,null,0,0,0,0,0,0]
[12,"Normat.","Kabelis 8x0,22","m",120,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Kabeļu kanāls 9x18","m",80,null,null,0,null,null,0,0,0,0,0,0]
[14,"Normat.","Palīgmateriāli","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[15,"Normat.","Iekārtas regulēšana, programēšana ","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[16,"Normat.","Nodošana ekspluatācijā","obj.",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"11","index":12,"n_rows":68,"n_cols":17,"rows_kept":68,"cut":false,"hidden":false,"merged":[[65,0,65,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 11"]
["Elektromontāžas darbi",{"$nulls":15},"Elektromontāžas darbi"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Apgaismojuma armatūras montāža","gab.",79,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Apgaismojuma armatūras restaurācija","gab.",12,null,null,0,null,null,0,0,0,0,0,0]
[3,"Normat.","Apgaismojuma regulatora montāža","gab.",3,null,null,0,null,null,0,0,0,0,0,0]
[4,"Normat.","Cauruļu montāža ","m",360,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Instalācijas demontāža","cilv. st.",16,null,null,0,null,null,0,0,0,0,0,0]
[6,"Normat.","Izpilddokumentācija, elektriskie mērījumi, projektēšana","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[7,"Normat.","Kabeļa montāža <50mm","m",1395,null,null,0,null,null,0,0,0,0,0,0]
[8,"Normat.","Kontaktu montāža","gab.",66,null,null,0,null,null,0,0,0,0,0,0]
[9,"Normat.","Kontaktu montāža 3-fāzu","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[10,"Normat.","Nozarkārbu montāža","gab.",125,null,null,0,null,null,0,0,0,0,0,0]
[11,"Normat.","Nozarkārbu savienošana","gab.",40,null,null,0,null,null,0,0,0,0,0,0]
[12,"Normat.","Rievu frēzēšana","m",260,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Sadales demontāža","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[14,"Normat.","Sadales montāža","gab.",3,null,null,0,null,null,0,0,0,0,0,0]
[15,"Normat.","Slēdžu montāža","gab.",18,null,null,0,null,null,0,0,0,0,0,0]
[16,null,"Apgaismojuma armatūra 2x36W IP56","gab.",51,null,null,0,null,null,0,0,0,0,0,0]
[17,null,"Apgaismojuma armatūra pie sienas 60W 220V IP56","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[18,null,"Apgaismojuma prožektors 500W","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[19,null,"Armatūra 2x 60W 220V IP 20 pie griestiem","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[20,null,"Armatūra ar akumulatoru 1h GEF 1x8w IP20 IZEJA","gab.",6,null,null,0,null,null,0,0,0,0,0,0]
[21,null,"Armatūra iebūvējama 60W 220V IP20 ar spuldzi","gab.",11,null,null,0,null,null,0,0,0,0,0,0]
[22,null,"Armatūra pie sienas 60W 220V IP20","gab.",3,null,null,0,null,null,0,0,0,0,0,0]
[23,null,"Armatūra pie sienas 60W 220V IP65","gab.",3,null,null,0,null,null,0,0,0,0,0,0]
[24,null,"Caurule cieta plastmasas JM 16","m",360,null,null,0,null,null,0,0,0,0,0,0]
[25,null,"Gaismas regulators elektroniskais ar pārslēdzi z/a IP20","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[26,null,"Gaismas regulators z/a IP20","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[27,null,"Kabelis PPJ (MMJ) 3x1.5","m",820,null,null,0,null,null,0,0,0,0,0,0]
[28,null,"Kabelis PPJ (MMJ) 3x2.5","m",450,null,null,0,null,null,0,0,0,0,0,0]
[29,null,"Kabelis PPJ (MMJ) 4x4","m",5,null,null,0,null,null,0,0,0,0,0,0]
[30,null,"Kabelis PPJ (MMJ) 4x6","m",60,null,null,0,null,null,0,0,0,0,0,0]
[31,null,"Kabelis PPJ (MMJ) 5x10","m",10,null,null,0,null,null,0,0,0,0,0,0]
[32,null,"Kabelis PPJ (MMJ) 5x2.5","m",50,null,null,0,null,null,0,0,0,0,0,0]
[33,null,"Akumulatru bloks ar pārslēdzi 1,5h 76W (iebūvēts)","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[34,null,"Kontakts 3 fāzu + 1fāzu","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[35,null,"Kontakts DOMINO z/a 1V","gab.",60,null,null,0,null,null,0,0,0,0,0,0]
[36,null,"Kontakts JUNG z/a+z 1V 16A IP54","gab.",6,null,null,0,null,null,0,0,0,0,0,0]
[37,null,"Nozarkārba v/a IP56 ","gab.",20,null,null,0,null,null,0,0,0,0,0,0]
[38,null,"Nozarkārba z/a","gab.",105,null,null,0,null,null,0,0,0,0,0,0]
[39,null,"Nozarkārbu vāks","gab.",20,null,null,0,null,null,0,0,0,0,0,0]
[40,null,"Palīgmateriāli","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[41,null,"Sadale apgaismojumam AS-1 v/a IP30","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[42,null,"Sadale spēka/apgaismojuma SS-2 z/a IP30","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[43,null,"Sadale spēka/apgaismojuma SS-1 v/a IP30","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[44,null,"Slēdzis DOMINO z/a 1P IP20","gab.",7,null,null,0,null,null,0,0,0,0,0,0]
[45,null,"Slēdzis DOMINO z/a 1P pārslēdzis IP20","gab.",7,null,null,0,null,null,0,0,0,0,0,0]
[46,null,"Slēdzis DOMINO z/a 2P IP20","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[47,null,"Slēdzis JUNG z/a 1P 10A IP55","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[48,null,"Slēdzis NIKO v/a 2P IP55","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[49,null,"Spuldze ekanomiskā 26W 220V","gab.",21,null,null,0,null,null,0,0,0,0,0,0]
[50,null,"Spuldze d.g. 36W","gab.",102,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"12","index":13,"n_rows":33,"n_cols":17,"rows_kept":33,"cut":false,"hidden":false,"merged":[[30,0,30,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 12"]
["Zibens aizsardzība",{"$nulls":15},"Zibens aizsardzība"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Stieples montāža uz jumta un sienas","m",225,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Stieples montāža tranšejā","m",152,null,null,0,null,null,0,0,0,0,0,0]
[3,"Normat.","Savienojumu montāža","gab.",10,null,null,0,null,null,0,0,0,0,0,0]
[4,"Normat.","Stieples taisnošana","m",225,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Tranšejas raksāna un aizbēršana","m",152,null,null,0,null,null,0,0,0,0,0,0]
[6,"Normat.","Zibens novadītāju montāža","gab.",12,null,null,0,null,null,0,0,0,0,0,0]
[7,null,"Apaļstieple Rd-8 St/Zn","m",225,null,null,0,null,null,0,0,0,0,0,0]
[8,null,"Apaļstieple cinkota 18mm","m",152,null,null,0,null,null,0,0,0,0,0,0]
[9,null,"Palīgmateriāli","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[10,null,"Jumta un notekrenes savienojumi ar zibensuztv.","gab.",12,null,null,0,null,null,0,0,0,0,0,0]
[11,null,"Stieples savstarpējie savienojumi \"Multi-Clamp\"","gab.",10,null,null,0,null,null,0,0,0,0,0,0]
[12,null,"Stieples turētājs uz sienas ","gab.",36,null,null,0,null,null,0,0,0,0,0,0]
[13,null,"Stieples turētājs uz jumta ar blīvējumu","gab.",122,null,null,0,null,null,0,0,0,0,0,0]
[14,null,"Zibens novadītājs ar spailēm","gab.",12,null,null,0,null,null,0,0,0,0,0,0]
[15,null,"Zibens novadītāja turētājs \"Rod Support\"","gab.",24,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"13","index":14,"n_rows":62,"n_cols":17,"rows_kept":62,"cut":false,"hidden":false,"merged":[[59,0,59,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 13"]
["Katlu māja",{"$nulls":15},"Katlu māja"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Granulu katls DRANDEG GD ECO 100","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Granulu uzkrāšanas tvertne ar pneimo padevi 7,1m3- silosss, brīvstāvošs, betonēta plāksne 2000*200*200, armējums 200*200*10 2kārtās, šķembu pamatojums 150mm","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[3,"Normat.","Reflex N 150 izplešanās trauks, 6bar","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[4,"Normat.","Automātiskais atgaisotājs ar ventili 1/2\"","gab.",4,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Manometra ventilis 1/2\"","gab.",5,null,null,0,null,null,0,0,0,0,0,0]
[6,"Normat.","Manometrs 0-4 bar","gab.",5,null,null,0,null,null,0,0,0,0,0,0]
[7,"Normat.","Termometrs 1/2\" 120o","gab.",6,null,null,0,null,null,0,0,0,0,0,0]
[8,"Normat.","Pretvārsts DN40","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[9,"Normat.","Pretvārsts DN32","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[10,"Normat.","Pretvārsts DN15","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[11,"Normat.","Pārplūdes vārsts ¾\" IG, PN 10","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[12,"Normat.","Sadales kolektors  2konturi+2katla izvadi,izolācijā (DN125)","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Sūknis cirk.  Wilo-TOP-RL  25/7  PN10","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[14,"Normat.","Sūknis cirk.  Wilo-STAR-RS 25/4 PN10","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[15,"Normat.","Dūmvada komplekts dm iekš.250,izolācija 50mm, H=8m, betonēts pamats 1800*1800*1600(h), armējums, iekiekamā detaļa- grozs","k-ts",1,null,null,0,null,null,0,0,0,0,0,0]
[16,"Normat.","Lodveida ventilis  DN50","gab.",3,null,null,0,null,null,0,0,0,0,0,0]
[17,"Normat.","Lodveida ventilis  DN40","gab.",4,null,null,0,null,null,0,0,0,0,0,0]
[18,"Normat.","Lodveida ventilis DN20","gab.",4,null,null,0,null,null,0,0,0,0,0,0]
[19,"Normat.","Uzpildes vārsts DN20","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[20,"Normat.","Regulējošs vārsts zāles apkurei VRG 25 ar el.piedziņu AMV 15","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[21,"Normat.","Regulējošs vārsts mūzikas skolas apkurei VRG 15 ar el.piedziņu AMV 15","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[22,"Normat.","ECL-300","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[23,"Normat.","Panelis uzstādīšanai pie sienas ","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[24,"Normat.","Ārgaisa sensors ESM-10","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[25,"Normat.","Virsmas sensors ESM-11","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[26,"Normat.","Programmu karte C66","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[27,"Normat.","Netīrumu ķērājs DN40","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[28,"Normat.","Netīrumu ķērājs DN20","gab.",1,null,null,0,null,null,0,0,0,0,0,0]
[29,"Normat.","Cauruļvadi veidgabali, siltumizolācija, montāžas palīgmateriāli","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[30,"Normat.","Griestiem karkass, 2x ugunsdrošs reģipša apšuvums, sagatave, krāsojums","m2",7,null,null,0,null,null,0,0,0,0,0,0]
[31,"Normat.","Grīdas demontāža, siltinājums 50mm, armējums 150*150*4, betonējums 70mm","m2",7,null,null,0,null,null,0,0,0,0,0,0]
[32,"Normat.","Durvju demontāža","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[33,"Normat.","Metāla RI30 durvju montāža ar ventilācijas pieplūdi 900*2100","gab.",2,null,null,0,null,null,0,0,0,0,0,0]
[34,"Normat.","Sienu sagatave,  javas apmetums","m2",30,null,null,0,null,null,0,0,0,0,0,0]
[35,"Normat.","Montēt logu, t.p. uzstādīt, ārējā 30cm, iekšējā  40cm palodzes montāža","gb.",2,null,null,0,null,null,0,0,0,0,0,0]
[36,"Normat.","PVC logs ar vērtni balts/balts 800*600","gb.",1,null,null,0,null,null,0,0,0,0,0,0]
[36,"Normat.","ārējā palodze PE 30cm","m",0.6,null,null,0,null,null,0,0,0,0,0,0]
[37,"Normat.","iekšējā palodze 40cm","m",0.6,null,null,0,null,null,0,0,0,0,0,0]
[37,"Normat.","Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[38,"Normat.","Logu ailu apdare, krāsojums","m2",0.9,null,null,0,null,null,0,0,0,0,0,0]
[39,"Normat.","Knauf GKBI","m2",1.05,null,null,0,null,null,0,0,0,0,0,0]
[40,"Normat.","Vetonit LR","kg",2.25,null,null,0,null,null,0,0,0,0,0,0]
[41,"Normat.","Krāsa \"Bindo 20\" ar toni","ltri",0.25,null,null,0,null,null,0,0,0,0,0,0]
[42,"Normat.","Palīgmateriāli","kompl",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"14","index":15,"n_rows":72,"n_cols":17,"rows_kept":72,"cut":false,"hidden":false,"merged":[[69,0,69,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 14"]
["Apkures sistēmas izbūve",{"$nulls":15},"Apkures sistēmas izbūve"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Esošās sistēmas demontāža","sisit.",1,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Uponor Unipipe PE-RT dauzdzslāņu caurule (stieņos), 16 x 2.0","m",150,null,null,0,null,null,0,0,0,0,0,0]
[3,"Normat.","Uponor Unipipe PE-RT dauzdzslāņu caurule (stieņos), 20 x 2.25","m",170,null,null,0,null,null,0,0,0,0,0,0]
[4,"Normat.","Uponor Unipipe PE-RT dauzdzslāņu caurule (stieņos), 25 x 2.5","m",100,null,null,0,null,null,0,0,0,0,0,0]
[5,"Normat.","Uponor Unipipe PE-RT dauzdzslāņu caurule (stieņos), 32 x 3.0","m",80,null,null,0,null,null,0,0,0,0,0,0]
[6,"Normat.","Uponor Unipipe PE-RT dauzdzslāņu caurule (stieņos), 40 x 4.0","m",50,null,null,0,null,null,0,0,0,0,0,0]
[7,"Normat.","Uponor Unipipe PE-RT dauzdzslāņu caurule (stieņos), 50 x 4.5","m",20,null,null,0,null,null,0,0,0,0,0,0]
[8,"Normat.","Uponor pāreja uz vītni, 40-1 1/2(ārējā)","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[9,"Normat.","Uponor pāreja, 20 - 16","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[10,"Normat.","Uponor pāreja, 25 - 20","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[11,"Normat.","Uponor pāreja, 32-25 ","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[12,"Normat.","Uponor pāreja, 32-25 ","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[13,"Normat.","Uponor pāreja, 40-25 ","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[14,"Normat.","Uponor pāreja, 40-32","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[15,"Normat.","Uponor pāreja, 50-40","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[16,"Normat.","Uponor līkums 90°, 16 - 16","gab",218,null,null,0,null,null,0,0,0,0,0,0]
[17,"Normat.","Uponor līkums 90°, 20 - 20","gab",52,null,null,0,null,null,0,0,0,0,0,0]
[18,"Normat.","Uponor līkums 90°, 25 - 25","gab",20,null,null,0,null,null,0,0,0,0,0,0]
[19,"Normat.","Uponor līkums 90°, 32 - 32","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[20,"Normat.","Uponor līkums 90°, 40-40","gab",20,null,null,0,null,null,0,0,0,0,0,0]
[21,"Normat.","Uponor līkums 90°, 50 - 50","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[22,"Normat.","Uponor  T-gabals, 16 - 16 - 16","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[23,"Normat.","Uponor  T-gabals, 16 - 20 - 16","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[24,"Normat.","Uponor  T-gabals, 20-16-20","gab",6,null,null,0,null,null,0,0,0,0,0,0]
[25,"Normat.","Uponor  T-gabals, 20 - 16 - 16","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[26,"Normat.","Uponor  T-gabals, 20 - 16 - 20","gab",10,null,null,0,null,null,0,0,0,0,0,0]
[27,"Normat.","Uponor  T-gabals, 25-16-20","gab",6,null,null,0,null,null,0,0,0,0,0,0]
[28,"Normat.","Uponor  T-gabals, 25-16-25","gab",8,null,null,0,null,null,0,0,0,0,0,0]
[29,"Normat.","Uponor  T-gabals, 32-16-32","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[30,"Normat.","Uponor  T-gabals, 32-16-25","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[31,"Normat.","Uponor  T-gabals, 32 - 25 - 20","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[32,"Normat.","Uponor  T-gabals, 40-16-40","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[33,"Normat.","Uponor  T-gabals, 40-16-32","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[34,"Normat.","Uponor  T-gabals, 40-40-25","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[35,"Normat.","Uponor  T-gabals, 50-25-50","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[36,"Normat.","Uponor  T-gabals, 50-40-40","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[37,"Normat.","Uponor  T-gabals ar vītni,50-1/2-50","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[38,"Normat.","Ventīlis DN 40 ar garo rokturi","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[39,"Normat.","Radiators  11k   500*600","gab",3,null,null,0,null,null,0,0,0,0,0,0]
[40,"Normat.","Radiators  22k   500*600","gab",3,null,null,0,null,null,0,0,0,0,0,0]
[41,"Normat.","Radiators  22k   500*1200","gab",4,null,null,0,null,null,0,0,0,0,0,0]
[42,"Normat.","Radiators  22k   500*800","gab",7,null,null,0,null,null,0,0,0,0,0,0]
[43,"Normat.","Radiators  22k   500*1400","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[44,"Normat.","Radiators  22k   500*1800","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[45,"Normat.","Radiators  33k   500*1200","gab",8,null,null,0,null,null,0,0,0,0,0,0]
[46,"Normat.","Radiators  33k   500*1400","gab",12,null,null,0,null,null,0,0,0,0,0,0]
[47,"Normat.","Termostata vārsts TS-90, leņķa,1/2\", ar 3/4\" ārējo vītni(ar eiro konusu D 16)","gab",41,null,null,0,null,null,0,0,0,0,0,0]
[48,"Normat.","Termostata galva ","gab",41,null,null,0,null,null,0,0,0,0,0,0]
[49,"Normat.","Bremzētājvārsts leņķa (ar eiro konusu D 16)","gab",41,null,null,0,null,null,0,0,0,0,0,0]
[50,"Normat.","Radiatoru kronšteini ","kom.",41,null,null,0,null,null,0,0,0,0,0,0]
[51,"Normat.","Automātiskie atgaisotāji","gab",2,null,null,0,null,null,0,0,0,0,0,0]
[52,"Normat.","Kronšteini","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[53,"Normat.","Caurumu aizdare","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[54,"Normat.","Palīgmateriāli","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]

{"sheet":"15","index":16,"n_rows":21,"n_cols":17,"rows_kept":21,"cut":false,"hidden":false,"merged":[[18,0,18,4],[0,0,0,15],[1,0,1,15],[8,11,8,12],[6,11,6,12],[7,11,7,12],[8,0,8,2],[10,7,10,10],[9,16,12,16],[9,7,9,10],[9,12,9,15],[10,12,10,15]],"flags":["formulas_cached_only"]}
["Lokālā tāme Nr. 15"]
["Ventilācijas sistēma",{"$nulls":15},"Ventilācijas sistēma"]
["Būves nosaukums:",null,"Tautas nams"]
["Objekta nosaukums:",null,"Kolkas Tautas nama vienkāršotā rekonstrukcija"]
["Objekta adrese:",null,"Dundagas novads, Kolka \"Tautas nams\""]
["Pasūtījuma Nr.",null,"Dundagas novada pašvaldība"]
[{"$nulls":10},"Cilvēkstundas: ",0]
[{"$nulls":10},"Tāme sastādīta:",0]
[{"$nulls":10},"Tiešās izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",{"$nulls":4},"Kopējās izmaksas"]
["Nr.","Normat.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"Darba","tai skaitā"]
["p.","pozic.","pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","ietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.","nr.",null,null,null,"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"I"]
[1,"Normat.","Ventilatora montāža bēniņstāvā AR 500E4","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[2,"Normat.","Ātruma regulators RTRD-2","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[3,"Normat.","Cauruļvadu veidgabali, siltumizolācija, montāžas palīgmateriāli","kompl.",1,null,null,0,null,null,0,0,0,0,0,0]
[{"$nulls":11},0,0,0,0,0]
[]
[{"$nulls":9},"Tiešās izmaksas:","Ls.",0,0,0,0,0]