{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Tāme"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tāme","index":0,"n_rows":90,"n_cols":17,"rows_kept":90,"cut":false,"hidden":false,"merged":[[3,0,3,15],[4,0,4,15],[8,11,8,12],[9,11,9,12],[10,11,10,12],[10,13,10,15],[80,11,80,15],[11,7,11,10],[11,11,11,15],[11,16,14,16],[12,7,12,10],[12,11,12,15],[74,11,74,15],[75,11,75,15],[76,11,76,15],[77,11,77,15],[78,11,78,15],[79,11,79,15]],"flags":["formulas_cached_only"]}
[]
[{"$nulls":8},"SASKAŅOTS:____________________/2013.g.     .                      /"]
[]
["Lokālā tāme Nr.4"]
["Dundagas mākslas, mūzikas skolas 3.stāva skolotāju istabas  remonta darbi (telpa Nr.141)"]
["Būves nosaukums:",null,"Dundagas mākslas, mūzikas skola"]
["Objekta nosaukums:",null,"3.stāva skolotāju istabas  remonta darbi (telpa Nr.141)"]
["Objekta adrese:",null,"Pils iela 14, Dundaga, Dundagas novads"]
["Pasūtījuma Nr.",null,"03.03.2013.",{"$nulls":7},"Darba ietilpība C/st:",0]
[{"$nulls":10},"Tāme sastādīta:"]
["Tāme sastādīta 2013.gada tirgus cenās, pamatojoties uz inventarizācijas lietu un uzmērījumiem dabā",{"$nulls":9},"Objekta izmaksas:",0]
[{"$nulls":7},"Vienības izmaksa",null,null,null,"Kopējā izmaksa"]
["Nr.","Pozic.","Darba un izdevumu nosaukums","Vienība","Daudz.","Laika","Darba ","tai skaitā",null,null,null,"tai skaitā"]
["p.",null,"pielietotie materiāli, to daudzums",null,null,"norma","samaksa","Darba alga","Materiāli","Mehanismi","Kopā","Darbietilpība","Darba alga","Materiāli","Mehanismi","Kopā"]
["k.",{"$nulls":4},"C/st","Ls","Ls","Ls","Ls","Ls","C/st","Ls","Ls","Ls","Ls"]
[1,2,3,4,5,6,7,"8","9","10","11","12","13","14","15","16"]
[null,"1","Remonta darbi"]
[1,"Normat.","Kājlīstu demontāža","m",22.7,{"$nulls":5},0,0,0,0,0,0]
[2,"Normat.","Krāsojuma attīrīšana griestiem","m2",32.4,{"$nulls":5},0,0,0,0,0,0]
[3,"Normat.","Krāsojuma, tapešu attīrīšana sienām","m2",79.2,{"$nulls":5},0,0,0,0,0,0]
[4,"Normat.","Būvgružu savākšana, utilizācija","m3",0.5,{"$nulls":5},0,0,0,0,0,0]
[5,"Normat.","Griestu gruntēšana, pilna špaktelēšana","m2",32.4,{"$nulls":5},0,0,0,0,0,0]
[6,"Normat.","Griestu krāsojums ar akrila krāsu 2x","m2",32.4,{"$nulls":5},0,0,0,0,0,0]
[7,"Normat.","Sienas gruntēšana, pilna špaktelēšana","m2",79.2,{"$nulls":5},0,0,0,0,0,0]
[8,"Normat.","Sienas krāsojums ar akrila, tonētu krāsu 2x","m2",79.2,{"$nulls":5},0,0,0,0,0,0]
[9,"Normat.","Grīdas virsmas gruntēšana","m2",32.4,{"$nulls":5},0,0,0,0,0,0]
[10,"Normat.","Virsmas izlīdzināšana līdz 10mm, stiprinot stiklšķiedras sietu 4*4mm, 160g/m2","m2",32.4,{"$nulls":5},0,0,0,0,0,0]
[11,"Normat.","Lamināta apakšklāja, lamināta ieklāšana 34.kl","m2",32.4,{"$nulls":5},0,0,0,0,0,0]
[12,"Normat.","Oša koka kājlīstes iebūve, vaskošana","m",22.7,{"$nulls":5},0,0,0,0,0,0]
[13,"Normat.","Alumīnija nosegslieksnis","m",1,{"$nulls":5},0,0,0,0,0,0]
[{"$nulls":10},"Kopā:",0,0,0,0,0]
[null,"2","Iekšējie elektrotīkli, apgaismojums"]
[1,"Normat.","Demontēt esošo elektroinstalāciju, utilizācija","kpl",1,{"$nulls":5},0,0,0,0,0,0]
[2,"Normat.","Apgaismojuma armatūras montāža 4*36w iekarināma, spuldzes","gb",2,{"$nulls":5},0,0,0,0,0,0]
[3,"Normat.","Automātiskā slēdža montāža B 1F 16A","gb",2,{"$nulls":5},0,0,0,0,0,0]
[4,"Normat.","Caurumu urbšana sienā instalācijai","gab.",1,{"$nulls":5},0,0,0,0,0,0]
[5,"Normat.","Kabeļa montāža  Kabelis PPJ 3*1.5","m",50,{"$nulls":5},0,0,0,0,0,0]
[6,"Normat.","Rievu frēzēšana mūrī","m",28,{"$nulls":5},0,0,0,0,0,0]
[7,"Normat.","Cauruļu montāža  pvc dm16-25mm","m",1,{"$nulls":5},0,0,0,0,0,0]
[8,"Normat.","Kārba betonam ar skruv. 60mm montāža","gb",12,{"$nulls":5},0,0,0,0,0,0]
[9,"Normat.","Nozarkārbu savienošana","gb",1,{"$nulls":5},0,0,0,0,0,0]
[10,"Normat.","Grupu slēdzis mehanisms 2P Siemens vai ekvivalents","gb",1,{"$nulls":5},0,0,0,0,0,0]
[11,"Normat.","Rozete mehanisms a/z balt. Siemens vai ekvivalents","gb",10,{"$nulls":5},0,0,0,0,0,0]
[12,"Normat."," Rāmitis 1d./balts Siemens vai ekvivalents","gb",3,{"$nulls":5},0,0,0,0,0,0]
[13,"Normat."," Rāmitis 5d./balts Siemens vai ekvivalents","gb",2,{"$nulls":5},0,0,0,0,0,0]
[14,"Normat.","Palīgmateriāli, stiprinājumi","k-ts",1,{"$nulls":5},0,0,0,0,0,0]
[{"$nulls":10},"Kopā:",0,0,0,0,0]
[null,"3","Iekšējie vājstrāvas tīkli"]
[1,"Normat.","Kabeļa motāža 5kat.","m",15,{"$nulls":5},0,0,0,0,0,0]
[2,"Normat.","Caurumu urbšana sienā instalācijai","gab.",1,{"$nulls":5},0,0,0,0,0,0]
[3,"Normat.","Rutenbeck Rozete 1xRJ45 5kat vai ekvivalents\nRutenbeck Rozete 1xRJ45 5kat \n","gb",2,{"$nulls":5},0,0,0,0,0,0]
[4,"Normat.","Rozetes TF Plate balt. Siemens vai ekvivalents","gb",2,{"$nulls":5},0,0,0,0,0,0]
[5,"Normat.","Rāmitis 1d./balts Siemens vai ekvivalents","gb",2,{"$nulls":5},0,0,0,0,0,0]
[6,"Normat.","Esošo UAS devēju pārcelšana","gb",1,{"$nulls":5},0,0,0,0,0,0]
[7,"Normat.","Palīgmateriāli, stiprinājumi","k-ts",1,{"$nulls":5},0,0,0,0,0,0]
[{"$nulls":10},"Kopā:",0,0,0,0,0]
[null,"4","Apkure"]
[1,"Normat.","Esošo radiatoru demontāža","gb",2,{"$nulls":5},0,0,0,0,0,0]
[2,"Normat.","Rievu frēzēšana mūrī","m",12.4,{"$nulls":5},0,0,0,0,0,0]
[3,"Normat.","Pieslēgšanās pie esošās sistēmas","vietas",2,{"$nulls":5},0,0,0,0,0,0]
[4,"Normat.","Vara cauruļu montāža d18","m",14,{"$nulls":5},0,0,0,0,0,0]
[5,"Normat.","Izolācija d=6 mm     Ø32 (d18) “TUBOLIT”","m",12.4,{"$nulls":5},0,0,0,0,0,0]
[6,"Normat.","Vara veidgabali","kpl",1,{"$nulls":5},0,0,0,0,0,0]
[7,"Normat.","Lod.pāreja PAV d 18x1/2\"a.v.","gb",4,{"$nulls":5},0,0,0,0,0,0]
[8,"Normat.","Radiators Purmo Compact 22*500*1400","gb",2,{"$nulls":5},0,0,0,0,0,0]
[9,"Normat.","Radiatora stiprinājumi","gb",2,{"$nulls":5},0,0,0,0,0,0]
[10,"Normat.","Radiatora ventīlis RTD-G","gb",2,{"$nulls":5},0,0,0,0,0,0]
[11,"Normat.","Radiatora termostats tiešās darbības","gb",2,{"$nulls":5},0,0,0,0,0,0]
[12,"Normat.","Radiatoru pieslēgums","gb",2,{"$nulls":5},0,0,0,0,0,0]
[13,"Normat.","Palīgmateriāli, stiprinājumi","k-ts",1,{"$nulls":5},0,0,0,0,0,0]
[{"$nulls":10},"Kopā:",0,0,0,0,0]
[]
[{"$nulls":9},"Sadaļas kopā:","Ls.",0,0,0,0,0,0]
[{"$nulls":8},"Materiālu sagāde, transporta izmaksas",null,"Ls.",null,null,0,0,0,0]
[{"$nulls":9},"Sadaļas kopā:","Ls.",0,{"$nulls":4},0]
[{"$nulls":8},"Pieskaitāmās izmaksas, t.sk. darba aizsardzība",null,"Ls.",0,{"$nulls":4},0]
[{"$nulls":8},"Plānotie uzkrājumi",null,"Ls.",0,{"$nulls":4},0]
[{"$nulls":8},"Darba devēja sociālais nodoklis ","24.09%","Ls.",0,{"$nulls":4},0]
[{"$nulls":9},"Sadaļa kopā:","Ls.",0,{"$nulls":4},0]
[{"$nulls":9},"PVN 21%","Ls.",0,{"$nulls":4},0]
[{"$nulls":9},"Objekta kopējās izmaksas:","Ls.",0,{"$nulls":4},0]
[]
[null,null,"Durvju, ailas paneļu, gaiteņa aplodu nomaiņa vai restaurācija netiek paredzēta, dēļ ierobežotiem finanšu līdzekļiem"]
[]
[null,"Sastādīja:","_________________________"]
[]
[]
[]
[null,null,"Datums:_______________________"]
[null,null,"v.z."]